Insert the following provisions in the designated location in Part 2 of the casework specification section.

 **2. GALVANIZED IRON WORK SURFACE**

 A. Material: 24 gauge galvanized iron bonded to a one inch thick core of suitable material.

 B. Galvanized iron shall completely cover top, sides and shall return one inch on underside of top. Solder, clean and remove all burrs and sharp edges at corners.

##  END OF APPENDIX A.7