HAYSITE REINFORCED PLASTICS AN ALCO INDUSTRIES CO -- GLASS REINFORCED THERMOSET POLYESTER MOLDED -- 6115-00-057-2055
=====================  Product Identification  =====================

Product ID:GLASS REINFORCED THERMOSET POLYESTER MOLDED
MSDS Date:11/27/1985
FSC:6115
NIIN:00-057-2055
MSDS Number: BCWLG
=== Responsible Party ===
Company Name:HAYSITE REINFORCED PLASTICS AN ALCO INDUSTRIES CO
Address:5599 NEW PERRY HWY
City:ERIE
State:PA
ZIP:16509-3562
Country:US
Info Phone Num:814-868-3691 / FAX 814-864-7803
Emergency Phone Num:814-868-3691
Preparer's Name:WALTER MC CULLOUGH
CAGE:66019
=== Contractor Identification ===
Company Name:HAYSITE REINFORCED PLASTICS AN ALCO INDUSTRIES CO
Address:5599 NEW PERRY HWY
Box:City:ERIE
State:PA
ZIP:16509-3562
Country:US
Phone:814-868-3691
CAGE:66019

=============  Composition/Information on Ingredients  =============

Ingred Name:CURED POLYESTER RESIN ON A GLASS SUBSTRATE
Fraction by Wt: 100%

=====================  Hazards Identification  =====================

Health Hazards Acute and Chronic:NONE KNOWN TO MANUFACTURER.
Effects of Overexposure:MAY DEVELOP SKIN ITCHING FROM DUST IF MATERIAL
    IS FABRICATED.
Medical Cond Aggravated by Exposure:NONE

=======================  First Aid Measures  =======================

First Aid:SYMPTOMATIC. SKIN CONTACT:WASH WITH SOAP AND WATER.

=====================  Fire Fighting Measures  =====================

Extinguishing Media:WATER PREFERRED;MAY USE FOAM.
Fire Fighting Procedures:NONE. MAY BE SELF-EXTINGUISHING.
Unusual Fire/Explosion Hazard:NONE

==================  Accidental Release Measures  ==================

Spill Release Procedures:SWEEP UP AND PLACE IN SUITABLE DISPOSAL
    CONTAINER.

======================	Handling and Storage  ======================

Handling and Storage Precautions:NO SPECIAL REQUIREMENTS.

=============  Exposure Controls/Personal Protection  =============

Respiratory Protection:USE DUST MASK IF MACHINING DUST IS PRESENT AND
    NOT ADEQUATELY HANDLED BY LOCAL EXHAUST VENTILATION.
Ventilation:PROVIDE MECHANICAL (GENERAL),AND LOCAL EXHAUST WHEN
    MACHINING.
Protective Gloves:USE GLOVES TO PROTECT FROM ABRASION
Eye Protection:SAFETY GLASSES WHEN MACHINING
Other Protective Equipment:GLASS FIBRE DUST IS A CONTACT IRRITANT.WEAR
    FULL WORKING CLOTHING.
Work Hygienic Practices:NORMAL GOOD PRACTICES,SUFFICIENT.
Supplemental Safety and Health

==================  Physical/Chemical Properties  ==================

HCC:N1
Spec Gravity:1.8
Solubility in Water:NONE
Appearance and Odor:SOLID SHAPES OF VARIOUS COLORS. POSSIBLE SLIGHT
    SWEET ODOR

=================  Stability and Reactivity Data  =================

Stability Indicator/Materials to Avoid:YES
NONE
Stability Condition to Avoid:NONE
Hazardous Decomposition Products:THERMAL DECOMPOSITION MAY PRODUCE
    CO,CO*2.

====================  Disposal Considerations  ====================

Waste Disposal Methods:KEEP IN COVERED DRUMS,PENDING DISPOSAL. HANDLE &
    DISPOSE IN FULL COMPLIANCE WITH ALL APPLICABLE
    INTERNATIONAL,FEDERAL,STATE, & LOCAL REGULATIONS.

 Disclaimer (provided with this information by the compiling agencies):
 This information is formulated for use by elements of the Department
 of Defense.  The United States of America in no manner whatsoever,
 expressly or implied, warrants this information to be accurate and
 disclaims all liability for its use.  Any person utilizing this
 document should seek competent professional advice to verify and
 assume responsibility for the suitability of this information to their
 particular situation.