CITGO PETROLEUM CORP -- MP ATF, DEXTRON-III/MERCON, 33-123 -- 9150-00N057511
=======================================================
MSDS Safety Information 
=======================================================
FSC: 9150
MSDS Date: 11/18/1993
MSDS Num: BWQTM
LIIN: 00N057511
Tech Review: 02/14/1995
Product ID: MP ATF, DEXTRON-III/MERCON, 33-123
Responsible Party
Cage: 1JW40
Name: CITGO PETROLEUM CORP
Box: 3758
City: TULSA OK 74102 US
Info Phone Number: 918-495-5933
Emergency Phone Number: 800-424-9300(CHEMTREC)
Review Ind: N
=======================================================
Contractor Summary 
=======================================================
Cage: 1JW40
Name: CITGO PETROLEUM CORP
Address: OFF HWY 108
Box: 3758
City: LAKE CHARLES LA 70602 US
Phone: 918-561-5165
Cage: 71476
Name: CITIES SERVICE CO
Address: CITIES SERVICE BLDG
Box: 300
City: TULSA OK 74102 US
Phone: 918-561-5165, FOR MED:318-491-6215
=======================================================
Ingredients 
=======================================================
Cas: 64741-89-5
RTECS #: PY8041501
Name: MINERAL OIL, PETRO DISTILLATES, SOLV-REFINED (SEV) LIGHT
  PARAFFINIC;(REFINED PETRO DISTILLATES).LD50 (ORAL,RAT): >5G/KG.
% by Wt: >80
OSHA PEL: N/K (FP N)
ACGIH TLV: N/K (FP N)
Ozone Depleting Chemical: N
------------------------------
Cas: 64741-88-4
RTECS #: PY8040501
Name: MINERAL OIL, PETROLEUM DISTILLATES, SOLVENT-REFINED (SEVERE) HEAVY
  PARAFFINIC; (PARAFFINIC OIL)
OSHA PEL: N/K (FP N)
ACGIH TLV: N/K (FP N)
Ozone Depleting Chemical: N
------------------------------
Name: ANTI-OXIDANT
% by Wt: <20
OSHA PEL: N/K (FP N)
ACGIH TLV: N/K (FP N)
-----------------------------
Name: ANITWEAR AGENTS (TYPE UNSPECIFIED)
OSHA PEL: N/K (FP N)
ACGIH TLV: N/K (FP N)
-----------------------------
Name: RED, DYE; (DYE, RED). LD50 (ORAL,RAT): 12.6 G/KG.
% by Wt: <0.1
OSHA PEL: N/K (FP N)
ACGIH TLV: N/K (FP N)
-----------------------------
Name: VENTILATION: STANDARDS, AS EVALUATED BY DESIGNATED PERSONNEL.
=======================================================
Health Hazards Data 
=======================================================
LD50 LC50 Mixture: SEE INGREDIENTS.
Route Of Entry Inds - Inhalation: YES
Skin: YES
Ingestion: YES
Carcinogenicity Inds - NTP: NO
IARC: NO
OSHA: NO
Effects of Exposure: ACUTE: INHALATION: LOW RISK AT AMBIENT TEMPERATURES.
  MISTS OR FUMES MAY CAUSE DIZZINESS, HEADACHE, NAUSEA, RESPIRATORY
  IRRITATION, OR CHEMICAL PNEUMONITIS. SKIN: TRANSIENT, SLIGHT IRRITANT,
  POSSIBLE M ILD ALLERGEN. EYE: TRANSIENT, SLIGHT IRRITATION. INGESTION:
  LOW TOXICITY. IF LESS THAN 1 OZ IS INGEST, (EFTS OF OVEREXP)
Explanation Of Carcinogenicity: NOT RELEVANT.
Signs And Symptions Of Overexposure: HEALTH HAZARDS: MATERIAL MAY PASS
  THROUGH SYSTEM WITHOUT HARM. ON INGESTION OF LARGE QUANTITIES, SLIGHT GI
  DISCOMFORT, DIARRHEA, AND HEADACHE MAY OCCUR. INJECTION: SUBCUTANEOUS OR
  INTRAMUSCULAR INJECT ION MAY CAUSE IRRITATION, ERYTHEMA, EDEMA. CHRONIC:
  DERMAL, PROLONGED AND REPEATED EXPOSURE MAY CAUSE DRYING OF SKIN.
Medical Cond Aggravated By Exposure: NONE.
First Aid: INHAL: REMOVE FROM EXPOS TO INCIDENTAL FUMES & PROVIDE RESP
  SUPPORT IF NEC. SKIN: WASH W/SOAP & WATER, UNTIL ALL TRACES OF MATL ARE
  REMOVED. EYES: FLUSH WITH LRG VOLS OF WATER FOR AT LST 15 MINS. INGE ST:
  DO NOT INDUCE VOMIT. SEEK MED AID. INJECTION: SEEK MED AID. NOTES TO
  PHYS: FOLLOWING INGEST, AT SAYBOLT VISCOSITY OF  175 SUS, (100F), RISK
  OF ASPIR INTO LUNGS IS REDUCED. REMOVE ALL MATL (SUPDAT)
=======================================================
Handling and Disposal
=======================================================
Spill Release Procedures: SML SPILLS: TAKE UP W/NON-COMBUST ABSORB SUCH AS
  FULLER'S EARTH/SAND. PLACE INTO CNTNRS FOR LATER DISP. LRG SPILLS:
  CONTAIN SPILL OF PROD/USED OIL IN EARTHEN DIKES FOR LATER RECOVERY.
  CNTRL IGNIT SOUR CES AROUND SPILL AREA. REPORT SPILLS AS (SUPDAT)
Neutralizing Agent: NONE SPECIFIED BY MANUFACTURER.
Waste Disposal Methods: IT IS RESPONSIBILITY OF USER TO DETERM IF MATL IS
  HAZ WASTE AT TIME OF DISP. CHECK BEFORE DISPOSING TO BE SURE YOU ARE IN
  COMPLIANCE WITH ALL APPLICABLE LAWS AND REGULATIONS. DISPOSE OF IN
  ACCORDANCE  WITH FEDERAL, STATE AND LOCAL REGULATIONS (FP N).
Handling And Storage Precautions: KEEP CNTNRS AWAY FROM HEAT AND FLAME.
  CAUTION: INSPECT EMPTY CONTAINERS BEFORE USE. THEY MAY CONTAIN PROD
  RESIDUE WHICH COULD INCL FLAMM & EXPLO VAPS.
Other Precautions: CONSULT APPROPRIATE FEDERAL, STATE AND LOCAL
  AUTHORITIES BEFORE REUSING, RECONDITIONING, RECLAIMING OR DISPOSING OF
  EMPTY CONTAINERS AND/OR WASTE RESIDUES OF PRODUCT.
=======================================================
Fire and Explosion Hazard Information 
=======================================================
Flash Point Text: SUPP DATA
Extinguishing Media: CARBON DIOXIDE, DRY CHEMICAL, FOAM, WATER FOG.
Fire Fighting Procedures: WEAR NIOSH/MSHA APPROVED SCBA AND FULL
  PROTECTIVE EQUIPMENT (FP N).
Unusual Fire/Explosion Hazard: WATER MAY CAUSE FROTHING.
=======================================================
Control Measures 
=======================================================
Respiratory Protection: IF HIGH CONCENTRATIONS OF MISTS OR FUMES ARE
  EXPECTED, USE A NIOSH/MSHA APPROVED ORGANIC RESPIRATOR.
Ventilation: USE IN WELL VENT AREA.IN CONFINED SPACE,MECH VENT MAY BE REQD
  TO KEEP LEVS OF CERTAIN COMPONENTS BELOW MANDATED (ING 6)
Protective Gloves: OIL IMPERVIOUS GLOVES,RUBBER OR POLYMER.
Eye Protection: ANSI APPROVED CHEM WORKERS GOGG (FP N).
Other Protective Equipment: WEAR BODY-COVERING GARMENTS TO PREVENT
  PROLONGED OR REPEATED DIRECT DERMAL EXPOSURE.
Work Hygienic Practices: LAUNDER SOILED WORK CLOTHES BEFORE REUSE. WASH
  FLUID-EXPOSED SKIN THOROUGHLY WITH SOAP AND WATER.REMOVE SOILED
  CLOTHING.
Supplemental Safety and Health: BP: 587F,308C 760 MMHG. SPEC GRAV: 0.87
  (60/60F) (H*2O=1). FL PT/FL PT METH: 367F,186C, COC; 271F,133C, PM;
  403F,206C, COC. FIRST AID PROC: BY EMESIS/LAVAGE. SUBCUTANEOUS OR
  INTRAMUSCULAR INJECTION RE QS PROMPT SURGICAL DEBRIDEMENT. IF NOT
  FAMILIAR W/TECHNIQUE, SEEK SKILLED ADVICE. SPILL PROC:REQD TO APPROP
  AUTHORITIES.
=======================================================
Physical/Chemical Properties 
=======================================================
B.P. Text: SUPP DATA
Vapor Pres: 2X103 @25C
Vapor Density: >1
Spec Gravity: SUPP DATA
Solubility in Water: NEGLIGIBLE
Appearance and Odor: RED LIQUID, MILD PETROLEUM ODOR.
Percent Volatiles by Volume: NEGLIG
=======================================================
Reactivity Data 
=======================================================
Stability Indicator: YES
Stability Condition To Avoid: NONE.
Materials To Avoid: STRONG OXIDANTS.
Hazardous Decomposition Products: CARBON DIOXIDE, (CARBON MONOXIDE UNDER
  INCOMPLETE COMBUSTION), TRACES OF SULFUR OXIDES.
Hazardous Polymerization Indicator: NO
Conditions To Avoid Polymerization: NOT RELEVANT.
=======================================================
Toxicological Information 
=======================================================
=======================================================
Ecological Information 
=======================================================
=======================================================
MSDS Transport Information 
=======================================================
=======================================================
Regulatory Information 
=======================================================
=======================================================
Other Information 
=======================================================
=======================================================
HAZCOM Label 
=======================================================
Product ID: MP ATF, DEXTRON-III/MERCON, 33-123
Cage: 1JW40
Company Name: CITGO PETROLEUM CORP
Street: OFF HWY 108
PO Box: 3758
City: LAKE CHARLES LA
Zipcode: 70602 US
Health Emergency Phone: 800-424-9300(CHEMTREC)
Date Of Label Review: 02/14/1995
Label Date: 02/14/1995
Chronic Hazard IND: Y
Eye Protection IND: YES
Skin Protection IND: YES
Signal Word: WARNING
Respiratory Protection IND: YES
Health Hazard: Slight
Contact Hazard: Moderate
Fire Hazard: Slight
Reactivity Hazard: None
Hazard And Precautions: COMBUSTIBLE. ACUTE: INHALATION: LOW RISK AT
  AMBIENT TEMPERATURES. MISTS OR FUMES MAY CAUSE DIZZINESS, HEADACHE,
  NAUSEA, RESPIRATORY IRRITATION, OR CHEMICAL PNEUMONITIS. SKIN:
  TRANSIENT, SLIGHT IRRITAN T, POSSIBLE MILD ALLERGEN. EYE: TRANSIENT,
  SLIGHT IRRITATION. INGESTION: LOW TOXICITY. IF LESS THAN 1 OZ IS
  INGESTED, MAY PASS THROUGH WITHOUT HARM. LARGE QUANTITIES MAY CAUSE
  SLIGHT GASTROINTESTINAL  DISCOMFORT, DIARRHEA, AND HEADACHE. INJECTION
  MAY CAUSE IRRITATION, ERYTHEMA, EDEMA. CHRONIC: DERMAL; MAY CAUSE DRYING
  OF SKIN.
=======================================================
Disclaimer (provided with this information by the compiling agencies):
  This information is formulated for use by elements of the Department of
  Defense. The United States of America in no manner whatsoever expressly
  or implied warrants, states, or intends said information to have any
  application, use or viability by or to any person or persons outside the
  Department of Defense nor any person or persons contracting with any
  instrumentality of the United States of America and disclaims all
  liability for such use. Any person utilizing this instruction who is not
  a military or civilian employee of the United States of America should
  seek competent professional advice to verify and assume responsibility
  for the suitability of this information to their particular situation
  regardless of similarity to a corresponding Department of Defense or
  other government situation.