MINNESOTA MINING AND  MFG CO, DBA 3M -- 3M (TM) FOAMFAST 74 SPRAY ADHESIVE -- 8040-00-181-7761
=======================================================
MSDS Safety Information 
=======================================================
FSC: 8040
NIIN: 00-181-7761
MSDS Date: 06/27/2000
MSDS Num: CLRYG
Tech Review: 12/06/2001
Product ID: 3M (TM) FOAMFAST 74 SPRAY ADHESIVE
Responsible Party
Cage: 76381
Name: MINNESOTA MINING AND  MFG CO, DBA 3M
Address: 3M CENTER BLDG 224-5S-04
City: SAINT PAUL MN 55144-1000 US
Info Phone Number: 866-556 5712 / 612-733-1110
Emergency Phone Number: (800)424-9300
Preparer's Name: HENRY SIMMONS
Chemtrec IND/Phone: (800)424-9300
=======================================================
Contractor Summary 
=======================================================
Cage: 76381
Name: MINNESOTA MINING AND  MFG. CO.
Address: 3M CENTER BLDG
City: SAINT PAUL MN 55144-1000 US
Phone: 800-364-3577/651-737-6501(24 HRS)
=======================================================
Item Description Information 
=======================================================
Item Manager: GSA
Item Name: ADHESIVE
Specification Number: NK
Type/Grade/Class: NK
Unit of Issue: CN
Quantitative Expression: 00000000024OZ
UI Container Qty: B
=======================================================
Ingredients 
=======================================================
Name: TRADESECRET
% low Wt: 20.
% high Wt: 30.
-----------------------------
Cas: 67-64-1
RTECS #: AL3150000
Name: ACETONE
% low Wt: 7.
% high Wt: 13.
OSHA PEL: 2400 MG/M3;1000 PPM
ACGIH TLV: 500 PPM
ACGIH STEL: 750 PPM
EPA Rpt Qty: 5000 LBS
DOT Rpt Qty: 5000 LBS
Ozone Depleting Chemical: N
------------------------------
Cas: 64742-48-9
Name: NAPHTHA (PETROLEUM), HYDROTREATED HEAVY
% low Wt: 1.
% high Wt: 5.
Ozone Depleting Chemical: N
------------------------------
Cas: 115-10-6
RTECS #: PM4780000
Name: DIMETHYL ETHER
% low Wt: 30.
% high Wt: 40.
Ozone Depleting Chemical: N
------------------------------
Cas: 109-66-0
RTECS #: RZ9450000
Name: PENTANE
% low Wt: 20.
% high Wt: 30.
OSHA PEL: 2950 MG/M3;1000 PPM
ACGIH TLV: 1770 MG/M3;600 PPM
ACGIH STEL: 2210 MG/M3;750 PPM
Ozone Depleting Chemical: N
=======================================================
Health Hazards Data 
=======================================================
Signs And Symptions Of Overexposure: EYE CONTACT: MODERATE EYE IRRITATION:
  SIGNS/SYMPTOMS CAN INCLUDE REDNESS, SWELLING, PAIN, TEARING, AND HAZY
  VISION.  SKIN CONTACT: MILD SKIN IRRITATION (AFTER PROLONGED OR REPEATED
  CONTACT): SIGNS/SYM PTOMS CAN INCLUDE REDNESS, SWELLING, AND ITCHING. 
  INHALATION: INTENTIONAL CONCENTRATIONS AND INHALATION MAY BE HARMFUL OR
  FATAL.  CENTRAL NERVOUS SYSTEM DEPRESSION: SIGNS/SYMPTOMS CAN INCLUDE
  HEADACH E, DIZZINESS, DROWSINESS, INCOORDINATION, SLOWED REACTION TIME,
  SLURRED SPEECH, GIDDINESS AND UNCONSCIOUSNESS.  IRRITATION (UPPER
  RESPIRATORY) SIGNS/SYMPTOMS CAN INCLUDE SORENESS OF THE NOSE AND THROA
  T, COUGHING AND SNEEZING.
First Aid: EYE CONTACT: IMMEDIATELY FLUSH EYES WITH LARGE AMOUNTS OF
  WATER. GET IMMEDIATE MEDICAL ATTENTION.  SKIN CONTACT: FLUSH SKIN WITH
  LARGE AMOUNTS OF WATER. IF IRRITATIONS PERSISTS. GET MEDICAL ATTENTION. 
  INHALATION: REMOVE PERSON TO FRESH AIR. IF NOT BREATHING, GIVE
  ARTIFICIAL RESPIRATION. IF BREATHING IS DIFFICULT, GET IMMEDIATE MEDICAL
  ATTENTION.  IF SWALLOWED: DO NOT INDUCE VOMITING, DRINK TWO GLA SSES OF
  WATER. CALL A PHYSICIAN.
=======================================================
Handling and Disposal
=======================================================
Spill Release Procedures: REFER TO OTHER SECTIONS OF THIS MSDS FOR
  INFORMATION REGARDING PHYSICAL AND HEALTH HAZARDS, RESPIRATORY
  PROTECTION, VENTILATION, AND PERSONAL PROTECTIVE EQUIPMENT. VENTILATE
  AREA. EXTINGUISH ALL IGNIT ION SOURCES. COVER WITH ABSORBENT MATERIAL.
  COLLECT USING NONSPARKING TOOLS. PLACE IN A U.S. DOT-APPROVED CONTAINER.
Waste Disposal Methods: INCINERATE IN PERMITTING HAZARDOUS INCINERATOR IN
  THE PRESENCE OF A COMBUSTIBLE MATERIAL. FACILITY MUST BE CAPABLE
  HANDLING AEROSOL CANS. DISPOSE OF EMPTY CANS IN A SANITARY LANDFILL.
  DISPOSE OF EMPTY  CANS IN A SANITARY LANDFILL. DISPOSE OF COMPLETELY
  ABSORBED WASTE PRODUCT IN A FACILITY PERMITTED T O ACCEPT CHEMICAL
  WASTES.
Handling And Storage Precautions: STORE AT TEMPERATURES BELOW 120 DEGREES
  F (49 DEGREES C). STORE OUT OR DIRECT SUNLIGHT. KEEP OUT OF REACH OF
  CHILDREN
Other Precautions: EYE PROTECTION: AVOID EYE CONTACT WITH VAPOR, SPRAY, OR
  MIST. WEAR SAFETY GLASSES WITH SIDE SHIELDS.	SKIN PROTECTION: AVOID
  PROLONGED OR REPEATED SKIN CONTRACT.	DO NOT	USE IN A CONFINED AREA OR
  ARE AS WITH LITTLE OR NO AIR MOVEMENT. IF EXHAUST VENTILATION IS NOT
  ADEQUATE, USE APPROPRIATE RESPIRATO RY PROTECTION.
=======================================================
Fire and Explosion Hazard Information 
=======================================================
Flash Point Method: TCC
Flash Point: =-45.4C, -50.F
Lower Limits: 1.0%
Upper Limits: FLAMMABL GAS
Extinguishing Media: WATER SPRAY, CARBON DIOXIDE, DRY CHEMICAL, FOAM
Fire Fighting Procedures: WEAR FULL PROTECTIVE CLOTHING, INCLUDING HELMET,
  SELF-CONTAINED, POSITIVE PRESSURE OR PRESSURE DEMAND BREATHING
  APPARATUS, BUNKER COAT AND PANTS, BANDS AROUND ARMS, WAIST AND LEGS,
  FACE MASK, AND PROT ECTIVE COVERING FOR EXPOSED AREAS OF THE HEAD. WATER
  MAY NOT EFFECTIVELY EXTINGUISH FIRE.
Unusual Fire/Explosion Hazard: CLOSED CONTAINERS EXPOSED TO HEAT FROM FIRE
  MAY BUILD PRESSURE AND EXPLODE. VAPORS MAY TRAVEL LONG DISTANCE ALONG
  THE GROUND OR FLOOR TO AN IGNITOIN SOURCE AND FLASH BACK.
=======================================================
Control Measures 
=======================================================
Respiratory Protection: AVOID BREATHING OF VAPORS, MISTS OR SPRAY. SELECT
  ONE OF THE FOLLOWING NIOSH APPROVED RESPIRATORS BASED ON AIRBORNE
  CONCENTRATION OF CONTAMINANTS AND IN ACCORDANCE WITH OSHA REGULATIONS.
  HALF MASK ORG ANIC VAPOR RESPIRATOR.
Ventilation: DO NOT USE IN A CONFINED AREA OR AREAS WITH LITTLE OR NO AIR
  MOVEMENT. IF EXHAUST VENTILATION IS NOT ADEQUATE, USE APPROPRIATE
  RESPIRATORY PROTECTION.
Protective Gloves: AVOID PROLONGED SKIN CONTACT.
Eye Protection: WEAR SAFETY GLASSES.
Other Protective Equipment: PROVIDE VENTILATION ADEQUATE TO CONTROL VAPOR
  CONCENTRATIONS BELOW RECOMMENDED EXPOSURE LIMITS AND/OR CONTROL SPRAY OR
  MIST.
Supplemental Safety and Health: AEROSOL CONTAINER CONTAINER FLAMMABLE GAS
  UNDER PRESSURE. KEEP AWAY FROM HEAT, SPARKS, OPEN FLAME, AND OTHER
  SOURCES OF IGNITION. EXTREMELY FLAMMABLE LIQUID AND VAPOR. DO NOT PIERCE
  OR BURN CONTAINER,  EVEN AFTER USE. NO SMOKING WHILE HANDLING THIS
  MATERIAL. AVOID STATIC DISCHARGE.
=======================================================
Physical/Chemical Properties 
=======================================================
Vapor Density: > 2 AIR=1
Volatile Org Content %: 78
Spec Gravity: 0.725 WATER=1
Evaporation Rate & Reference: 2.00 ETHER=1
Solubility in Water: NIL
Appearance and Odor: LIQUID IN AEROSOL, ORANGE, SWEET/FRUITY ODOR
=======================================================
Reactivity Data 
=======================================================
Stability Indicator: YES
Stability Condition To Avoid: HEAT
Hazardous Polymerization Indicator: NO
=======================================================
Regulatory Information 
=======================================================
Sara Title III Information: VOLATILE ORGANIC COMPOUNDS CA. 66% BY WT. VOC
  LESS H20 & EXEMPT SOLVENTS: CA 563 GMS/LITER CACULATED PER SCAQMD RULE
  443.1. HAZARDOUS AIR POLLUTANTS: 0% BY WT CALCULATED. SINCE REGULATIONS
  VARY, CONSU LT APPLICABLE REGULATIONS OR AUTHORITIES BEFORE DISPOSAL.
  U.S EPA HAZARDOUS NUMBER = D001 (IGNITABLE)
=======================================================
Other Information 
=======================================================
Other Information: AEROSOL CONTAINER CONTAINS FLAMMABLE GAS UNDER
  PRESSURE. KEEP AWAY FROM HEAT, SPARKS, OPEN FLAME, AND OTHER SOURCES OF
  IGNITION. EXTREMELY FLAMMABLE LIQUID AND VAPOR. DO NOT PIERCE OR BURN
  CONTAINER,  EVEN AFTER USE. NO SMOKING WHILE HANDLING THIS MATERIAL.
  AVOID STATIC DISCHARGE.
=======================================================
HAZCOM Label 
=======================================================
Product ID: 3M (TM) FOAMFAST 74 SPRAY ADHESIVE
Cage: 76381
Company Name: MINNESOTA MINING AND  MFG. CO.
Street: 3M CENTER BLDG
City: SAINT PAUL MN
Zipcode: 55144-1000 US
Health Emergency Phone: (800)424-9300
Date Of Label Review: 12/06/2001
=======================================================
Disclaimer (provided with this information by the compiling agencies):
  This information is formulated for use by elements of the Department of
  Defense. The United States of America in no manner whatsoever expressly
  or implied warrants, states, or intends said information to have any
  application, use or viability by or to any person or persons outside the
  Department of Defense nor any person or persons contracting with any
  instrumentality of the United States of America and disclaims all
  liability for such use. Any person utilizing this instruction who is not
  a military or civilian employee of the United States of America should
  seek competent professional advice to verify and assume responsibility
  for the suitability of this information to their particular situation
  regardless of similarity to a corresponding Department of Defense or
  other government situation.