SHERWIN-WILLIAMS CO -- E61 H 6, KEM FLASH PRIME BUFF -- 8010-00N032338
=====================  Product Identification  =====================

Product ID:E61 H 6, KEM FLASH PRIME BUFF
MSDS Date:12/15/1986
FSC:8010
NIIN:00N032338
MSDS Number: BNQZG
=== Responsible Party ===
Company Name:SHERWIN-WILLIAMS CO
Address:101 PROSPECT AVE NW
City:CLEVELAND
State:OH
ZIP:44115
Country:US
Info Phone Num:216-566-2902
Emergency Phone Num:216-566-2917
CAGE:54636
=== Contractor Identification ===
Company Name:SHERWIN-WILLIAMS CO THE
Address:101 PROSPECT AVE NW
Box:City:CLEVELAND
State:OH
ZIP:44115-1042
Country:US
Phone:800-251-2486/216-566-2242
CAGE:54636

=============  Composition/Information on Ingredients  =============

Ingred Name:SUPP DATA: WHEN NOT IN USE. TRANSFER ONLY TO APPRVD CNTNRS
    W/COMPLETE & APPROP LBLG.DO NOT TAKE INTERNALLY.KEEP (ING 6)
RTECS #:9999999ZZ

Ingred Name:ING 5:OUT OF REACH OF CHILDREN.COATING CONTAINS MATLS
    CLASSIFIED AS NUISANCE PARTICULATES, FOR EXAMPLE TITANIUM (ING 7)
RTECS #:9999999ZZ

Ingred Name:ING 6: DIOXIDE, CALCIUM CARBONATE, ETC. (SEE ACGIH TLV
    LIST, PREFACE & APPENDIX D) WHICH MAY BE PRESENT AT HAZ (ING 8)
RTECS #:9999999ZZ

Ingred Name:ING 7:LEVS ONLY DURING SANDING/ABRADING OF DRIED
    FILM.INTENTIONAL MISUSE BY DELIB CONC & INHAL CONTENTS CAN BE (ING
    9)
RTECS #:9999999ZZ

Ingred Name:ING 8: HARMFUL/FATAL. USE ONLY W/ADEQ VENT.AVOID BRTHG VAP
    & SPRAY MIST. AVOID CONT W/SKIN & EYES. WASH HANDS (ING 10)
RTECS #:9999999ZZ

Ingred Name:ING 9: AFTER USING. PROTECT AGAINST DUST WHICH MAY BE
    GENERATED BY SANDING OR ABRADING DRIED FILM.
RTECS #:9999999ZZ

Ingred Name:VENT: REFER TO OSHA STDS 1910.94, 1910.107, 1910.108.
RTECS #:9999999ZZ

Ingred Name:VM & P NAPHTHA. VP: 12.
CAS:64742-48-9
Fraction by Wt: 30-35%
OSHA PEL:300 PPM;400 STEL
ACGIH TLV:300 PPM

Ingred Name:KEROSENE (PETROLEUM), HYDROTREATED; (MINERAL SPIRITS). VP:
    2.
CAS:64742-47-8
RTECS #:OA5504000
Fraction by Wt: <5%
OSHA PEL:500 PPM (MFR)
ACGIH TLV:100 PPM (MFR)

Ingred Name:TOLUENE  (SARA III)
CAS:108-88-3
RTECS #:XS5250000
Fraction by Wt: <5%
OSHA PEL:200 PPM/150 STEL
ACGIH TLV:50 PPM; 9293
EPA Rpt Qty:1000 LBS
DOT Rpt Qty:1000 LBS

Ingred Name:TITANIUM OXIDE; (TITANIUM DIOXIDE)
CAS:13463-67-7
RTECS #:XR2275000
Fraction by Wt: 0-15%
OSHA PEL:15 MG/M3 TDUST
ACGIH TLV:10 MG/M3 TDUST; 9293

=====================  Hazards Identification  =====================

LD50 LC50 Mixture:NONE SPECIFIED BY MANUFACTURER.
Routes of Entry: Inhalation:YES  Skin:NO  Ingestion:YES
Reports of Carcinogenicity:NTP:NO    IARC:NO	OSHA:NO
Health Hazards Acute and Chronic:ACUTE:OVEREXP CAUSES EYE,SKIN & RESP
    IRRIT. MAY CAUSE NERV SYS DEPRESS ACCOMPANIED BY HDCH,DIZZ,NAUS,
    CONFUSN & STAG GAIT.EXTREME OVEREXP MAY RSLT IN UNCON & POSS DEATH.
    CHRONIC: PRLNGD OVEREXP TO ING REDS MAY CAUSE ADVERSE EFTS TO
    LIVER,URINARY,BLOOD FORMING,& CARDIO-VASCULAR SYS.RATS EXPOS TO
    TITANIUM (EFTS OF OVEREXP
Explanation of Carcinogenicity:NOT RELEVANT.
Effects of Overexposure:HLTH HAZ:DIOXIDE DUST AT 250 MG/M3 DEVELOPED
    LUNG CANCER, HOWEVER, SUCH EXPOS LEVS ARE NOT ATTAINABLE IN
    WORKPLACE. RPTS HAVE ASSOC RPTD & PRLNGD OVEREXP TO SOLV W/PERM
    BRAIN & NERV SYS DMG. TOLUENE 1 08-88-3 APPEARS ON NAVY LISTING OF
    OCCUP REPROD HAZ.SEEK CONSULTATION FROM APPROP HLTH PROFESSIONALS
    CONCERNING (SUPDAT)
Medical Cond Aggravated by Exposure:NONE SPECIFIED BY MANUFACTURER.

=======================  First Aid Measures  =======================

First Aid:INHALATION: REMOVE FROM EXPOSURE. RESTORE BREATHING. KEEP
    WARM AND QUIET. SKIN: WASH AFFECTED AREA THOROUGHLY WITH SOAP AND
    WATER. REMOVE CONTAMINATED CLOTHING AND LAUNDER BEFORE RE-USE.
    EYES: FLUSH W ITH LARGE AMOUNTS OF WATER FOR AT LEAST15 MINUTES.
    GET MEDICAL ATTENTION. INGESTION: CALL MD IMMEDIATELY .

=====================  Fire Fighting Measures  =====================

Flash Point Method:PMCC
Flash Point:50.0F,10.0C
Lower Limits:0.9%
Extinguishing Media:CARBON DIOXIDE, DRY CHEMICAL, FOAM.
Fire Fighting Procedures:WEAR NIOSH/MSHA APPRVD SCBA& FULL PROT
    EQUIP.H2O SPRAY MAY BE INEFT.IF H2O USED,FOG NOZZ PREF.H2O MAY BE
    USED TO COOL CLSD CNTNRS TO PVNT PRESS(SUPDAT)
Unusual Fire/Explosion Hazard:KEEP CNTNRS TIGHTLY CLSD.ISOLATE FROM
    HEAT, ELEC EQUIP,SPARKS,& OPEN FLAME.CLSD CNTNRS MAY EXPLO WHEN
    EXPOS TO EXTREME HEAT.APPLIC TO HOT SURFS REQS (SUPDAT)

==================  Accidental Release Measures  ==================

Spill Release Procedures:REMOVE ALL SOURCES OF IGNITION. VENTILATE AND
    REMOVE WITH INERT ABSORBENT.
Neutralizing Agent:NONE SPECIFIED BY MANUFACTURER.

======================	Handling and Storage  ======================

Handling and Storage Precautions:CONTENTS ARE FLAMMABLE. KEEP AWAY FROM
    HEAT, SPARKS, AND OPEN FLAME. DOL STORAGE CATEGORY-1B.
Other Precautions:DURING USE & UNTIL ALL VAPS ARE GONE:KEEP AREA
    VENT-DO NOT SMOKE-EXTING ALL FLAMES, PILOT LIGHTS,& HEATERS-TURN
    OFF STOVES, ELEC TOOLS & APPLIANCES,& ANY OTHER SOURCES OF IGNIT.
    CONSULT NFPA CODE.USE  APPRVD BONDING & GROUNDING PROC.(SUPDAT)

=============  Exposure Controls/Personal Protection  =============

Respiratory Protection:IF PERSONAL EXPOSURE CANNOT BE CONTROLLED BELOW
    APPLICABLE LIMITS BY VENTILATION, WEAR NIOSH/MSHA APPROVED
    RESPIRATORY DEVICE FOR PROTECTION AGAINST MATERIALS IN INGREDIENTS
    SECTION.
Ventilation:LOC EXHST PREF. GEN EXHST ACCEPTABLE IF EXPOS TO MATLS IN
    INGRED SEC IS MAINTAINED BELOW APPLIC EXPOS LIMITS. (ING 11)
Protective Gloves:IMPERVIOUS GLOVES .
Eye Protection:CHEMICAL WORKERS GOGGLES .
Other Protective Equipment:NONE SPECIFIED BY MANUFACTURER.
Work Hygienic Practices:USE ONLY W/ADEQ VENT. AVOID BRTHG VAPOR AND
    SPRAY MIST. AVOID CONTACT WITH SKIN AND EYES. WASH HANDS AFTER
    USING.
Supplemental Safety and Health
FIRE FIGHT PROC: BUILD-UP & POSS AUTOIGNIT/ EXPLO WHEN EXPOS TO EXTREME
    HEAT. EXPLO HAZ: SPECIAL PREC.DURING EMER CNDTNS OVEREXP TO DECOMP
    PRODS MAY CAUSE HLTH HAZ.SYMP MAY NOT BE IMMED APPARENT.OBTAI N MED
    ATTN. EFTS OF OVEREXP: LATEST HAZLIST INFO & SAFE HNDLG & EXPOS
    RECOM. OTHER PREC: KEEP CNTNR CLSD (ING 5)

==================  Physical/Chemical Properties  ==================

HCC:F3
Boiling Pt:B.P. Text:>222F,>106C
Vapor Pres:SEE INGRED
Vapor Density:HVR/AIR
Spec Gravity:1.2-1.3 
Evaporation Rate & Reference:SLOWER THAN ETHER
Appearance and Odor:NONE SPECIFIED BY MANUFACTURER.
Percent Volatiles by Volume:63

=================  Stability and Reactivity Data  =================

Stability Indicator/Materials to Avoid:YES
NONE SPECIFIED BY MANUFACTURER.
Stability Condition to Avoid:NONE SPECIFIED BY MANUFACTURER.
Hazardous Decomposition Products:BY FIRE: CO2, CO.

====================  Disposal Considerations  ====================

Waste Disposal Methods:WASTE FROM PROD MAY BE HAZ AS DEFINED UNDER RCRA
    40 CFR 261.WASTE MUST BE TESTED FOR IGNIT & EXTRACTABILITY TO
    DETERM APPLIC EPA HAZ WASTE NUMBERS. INCIN IN APPRVD FACILITY.DO
    NOT INCIN CLSD CNTNR. DI SP OF I/A/W FED,ST,& LOC REGS
    REGARDINGPOLLUTION.

 Disclaimer (provided with this information by the compiling agencies):
 This information is formulated for use by elements of the Department
 of Defense.  The United States of America in no manner whatsoever,
 expressly or implied, warrants this information to be accurate and
 disclaims all liability for its use.  Any person utilizing this
 document should seek competent professional advice to verify and
 assume responsibility for the suitability of this information to their
 particular situation.