|  |  |  |  |
| --- | --- | --- | --- |
| **OOR Number**: |  | **Dealer**: |  |
| **Project Name:** |  | **Date:** |  |
|  | | | |

🡸 Check for **ALL** **Standard Default** selections

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **1.** | **Cabinet Front Door/Drawer Flush Overlay Head Style** | | |  | **7.** | **Lock Types** | |
|  |  | | |  | Designated by cabinet suffix “**L**” | |
| **1a.** | **Door/Drawer Fronts – Wood Option, Flush Overlay** | | |  |  | Master 5-disc – **Standard Default** |
|  |  | Flush overlay, vertical-matched grain only | |  |  | Use when up to 225 primary key changes are |
|  |  | **Veneer selections** | |  |  | required (master-keyed) |
|  |  |  | Plain-sliced Red Oak |  |  | Master 5-pin |
|  |  |  | Rift-cut Red Oak |  |  |  |
|  |  |  | Rotary-sliced select Maple | **8.** | **Label Holders** | |
|  |  |  | Plain-sliced select Maple |  |  | None – **Standard Default** |
|  |  |  | Color Code: |  |  | One each door, one each drawer head |
|  |  |  |  |  |  | Black  Stainless Steel |
| **1b.** | **Door/Drawer Fronts – Plastic Laminate Option, Flush Overlay** | | |  |  | One per *pair* of doors, one each drawer head |
|  | Plastic Laminate Color Code: | | |  |  | Black  Stainless Steel |
|  |  | 3mm PVC edgeband color: | |  | ***Check “None” if full-width and semi-recessed*** | |
|  |  | | Black  Gray  Chameleon  White |  | ***polypropylene pulls are selected*** | |
|  |  |  | |  |  |  |
| **2.** | **Drawer Suspension** | | | **9.** | **Base Unit Shelf** | |
|  |  | Self-closing, self-centering hold open feature | |  |  | One piece – **Standard Default** |
|  |  | 100-pound drawer runs – **Standard Default** | |  |  | Split (two-piece) |
|  |  | SEFA 8 150-pound full extension drawer slides | |  |  | |
|  |  | – **Standard on file drawers** | | **10.** | **Removable Access Panel** | |
|  |  |  | |  | At base cabinets only; 100J/200J cupboard cabinets have removable | |
| **3.** | **Cabinet Hinges – 5-Knuckle, Flush or Radius Overlay** | | |  | backs standard. For removable backs in 100J/200J series drawer or | |
|  |  | Stainless steel – **Standard Default** | |  | combination cabinets, select “at both cupboard and drawer areas.” | |
|  |  | Black | |  |  | At cupboard areas only – **Standard Default** |
|  |  | | |  |  | At both cupboard and drawer areas |
| **4.** | **Pull Location** | | |  |  | |
|  |  | Configuration 1 | | **11.** | **Glass** | |
|  |  | Horizontal on drawers, vertical on doors | |  |  | Float glass – clear 6 mm – **Standard Default** |
|  |  | Configuration 2 | |  |  | Safety glass – laminated 6 mm (framed) |
|  |  | Horizontal on drawers and base unit doors | |  |  | Safety glass – tempered 6 mm (framed) |
|  |  | Configuration 3 | |  |  | |
|  |  | Continuous full-width horizontal pull on base cabinet doors and | | **12.** | **Security Panel (between locked sections)** | |
|  |  | drawers | |  |  | Without panel – **Standard Default** |
|  | ***Wall, upper and tall cases feature vertical pulls*** | | |  |  | With panel |
|  |  |  | |  |  | |
| **5a.** | **Pull Types –** Available in Configurations **1** & **2** Only | | | **13.** | **Suspension Hardware** | |
|  |  | Brushed aluminum rectangular pull – **Standard Default** | |  |  | Hanger at MAX/Lab – **Standard Default** |
|  |  | Stainless steel wire pull | |  |  | |
|  |  |  | | **14.** | **Finish (wood door and drawer fronts only)** | |
| **5b.** | **Pull Types** – Available in Configuration **1** Only | | |  |  | SEFA 8 – **Standard Default** |
|  |  | Semi-recessed polypropylene | |  |  | |
|  |  |  | Black  Gray  Chameleon  White |  |  | |
|  |  |  | |  |  |  |
| **6.** | **Door Catches** | | |  |  |  |
|  | Roller – **Standard Default** | | |  |  |  |
|  |  |  | |  |  |  |
|  |  |  | |  |  | |
|  |  | | |  |  | |
|  |  |  | |  |  | |
|  |  |  |  |  |  | |
|  |  | | |  |  |  |
|  |  |  | |  |  | |
|  |  |  |  |  |  | |
|  |  |  | |  |  | |