|  |  |  |  |
| --- | --- | --- | --- |
| **OOR Number**: |       | **Dealer**: |       |
| **Project Name:** |       | **Date:** |       |
|  |

[ ]  🡸 Check for **ALL** **Standard Default** selections

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **1.** | **Cabinet Front Door/Drawer Flush Overlay Head Style** |  | **7.** | **Lock Types** |
|  |  |  | Designated by cabinet suffix “**L**” |
| **1a.** | **Door/Drawer Fronts – Wood Option, Flush Overlay** |  | [ ]  | Master 5-disc – **Standard Default** |
|  | [ ]  | Flush overlay, vertical-matched grain only |  |  | Use when up to 225 primary key changes are |
|  |  | **Veneer selections** |  |  | required (master-keyed) |
|  |  | [ ]  | Plain-sliced Red Oak |  | [ ]  | Master 5-pin |
|  |  | [ ]  | Rift-cut Red Oak |  |  |  |
|  |  | **[ ]**  | Rotary-sliced select Maple | **8.** | **Label Holders** |
|  |  | **[ ]**  | Plain-sliced select Maple |  | [ ]  | None – **Standard Default** |
|  |  |  | Color Code:  |  | [ ]  | One each door, one each drawer head |
|  |  |  |  |  |  | **[ ]**  Black [ ]  Stainless Steel  |
| **1b.** | **Door/Drawer Fronts – Plastic Laminate Option, Flush Overlay**  |  | [ ]  | One per *pair* of doors, one each drawer head |
|  | Plastic Laminate Color Code:       |  |  | **[ ]**  Black [ ]  Stainless Steel |
|  |  | 3mm PVC edgeband color: |  | ***Check “None” if full-width and semi-recessed*** |
|  |  | [ ]  Black [ ]  Gray [ ]  Chameleon [ ]  White |  | ***polypropylene pulls are selected*** |
|  |  |  |  |  |  |
| **2.** | **Drawer Suspension** | **9.** | **Base Unit Shelf** |
|  | [ ]  | Self-closing, self-centering hold open feature  |  | **[ ]**  | One piece – **Standard Default**  |
|  |  | 100-pound drawer runs – **Standard Default** |  | **[ ]**  | Split (two-piece) |
|  | [ ]  | SEFA 8 150-pound full extension drawer slides |  |  |
|  |  | – **Standard on file drawers** | **10.**  | **Removable Access Panel** |
|  |  |  |  | At base cabinets only; 100J/200J cupboard cabinets have removable |
| **3.** | **Cabinet Hinges – 5-Knuckle, Flush or Radius Overlay** |  | backs standard. For removable backs in 100J/200J series drawer or |
|  | [ ]  | Stainless steel – **Standard Default** |  | combination cabinets, select “at both cupboard and drawer areas.” |
|  | [ ]  | Black  |  | [ ]  | At cupboard areas only – **Standard Default** |
|  |  |  | **[ ]**  | At both cupboard and drawer areas |
| **4.** | **Pull Location** |  |  |
|  | [ ]  | Configuration 1 | **11.** | **Glass** |
|  |   | Horizontal on drawers, vertical on doors |  | **[ ]**  | Float glass – clear 6 mm – **Standard Default** |
|  | **[ ]**  | Configuration 2 |  | [ ]  | Safety glass – laminated 6 mm (framed) |
|  |  | Horizontal on drawers and base unit doors |  | **[ ]**  | Safety glass – tempered 6 mm (framed) |
|  | [ ]  | Configuration 3 |  |  |
|  |  | Continuous full-width horizontal pull on base cabinet doors and | **12.** | **Security Panel (between locked sections)** |
|  |  | drawers |  | [ ]  | Without panel – **Standard Default**   |
|  | ***Wall, upper and tall cases feature vertical pulls*** |  | [ ]  | With panel |
|  |  |  |  |  |
| **5a.** | **Pull Types –** Available in Configurations **1** & **2** Only | **13.** | **Suspension Hardware** |
|  | [ ]  | Brushed aluminum rectangular pull – **Standard Default** |  | [ ]  | Hanger at MAX/Lab – **Standard Default** |
|  | [ ]  | Stainless steel wire pull |  |  |
|  |  |  | **14.** | **Finish (wood door and drawer fronts only)** |
| **5b.** | **Pull Types** – Available in Configuration **1** Only |  | [ ]  | SEFA 8 – **Standard Default**  |
|  | [ ]  | Semi-recessed polypropylene |  |  |
|  |  |  | [ ]  Black [ ]  Gray [ ]  Chameleon [ ]  White |  |  |
|  |  |  |  |  |  |
| **6.**  | **Door Catches** |  |  |  |
|  | Roller – **Standard Default** |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |