|  |  |  |  |
| --- | --- | --- | --- |
| **OOR Number**: |       | **Dealer:** |       |
| **Project Name:** |       | **Date:** |       |
|  |

[ ]  🡸 Check for **ALL** **Standard Default** selections

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **1.** | **Drawer Suspension** |  | **6.** | **Lock Types**  |
|  | [ ]  | Self-closing, self-centering hold open feature |  | Designated by cabinet suffix “**L**” |
|  |  | 100-pound drawer runs – **Standard Defaul**t |  | **[ ]**  | Master 5-disc – **Standard Default** |
|  | [ ]  | SEFA 8 150-pound, full-extension drawer slides– **Standard on file drawers** |  |  | Use when up to 225 key changes are required (master-keyed) |
|  |  |  |  | [ ]  | Master 5-pin |
| **2.** | **Cabinet Hinges** |  |  |  |
|  | [ ]  | Stainless steel – **Standard Default** | **7.** | **Label Holders** |
|  | [ ]  | Black  |  | [ ]  | None – **Standard Default** |
|  |  |  |  | [ ]  | One per door, one each drawer head |
| **3.** | **Pull Location** |  |  | [ ]  Stainless Steel [ ]  Black  |
|  | [ ]  | Configuration 1 |  | [ ]  | One per *pair* of doors, one each drawer head |
|  |  | Horizontal on drawers, vertical on doors – **Standard Defaul**t |  |  | [ ]  Stainless Steel [ ]  Black  |
|  | [ ]  | Configuration 2 |  | ***Check “None” if full-width and semi-*** |
|  |  | Horizontal on drawers and doors |  | ***recessed polypropylene pulls are selected*** |
|  | [ ]  | Configuration 3 |  |  |  |
|  |  | Continuous full-width pull is horizontal on drawers, vertical pull on | **8.** | **Base Unit Shelf** |
|  |  | doors |  | [ ]  | One-piece unit – **Standard Default** |
|  | ***Wall, upper and tall cases feature vertical pulls*** |  | [ ]  | Split (two-piece) |
|  |  |  |  |  |  |
| **4a.** | **Pull Types –** Available in Configurations **1** and **2** **only** | **9.** | **Removable Access Panel** |
|  | [ ]  | Brushed aluminum rectangular pull – **Standard Default** |  | At base cabinets only – 100J/200J cupboard cabinets have removable |
|  | [ ]  | Stainless steel wire pull |  | backs standard. For removable backs in 100J/200J series drawer or |
|  |  |  |  | combination cabinets, select “at both cupboard and drawer areas” |
| **4b.** | **Pull Types –** Available in Configuration **1** **only** |  | **[ ]**  | At cupboard areas only – **Standard Default** |
|  | [ ]  | Semi-recessed polypropylene |  | [ ]  | At both cupboard and drawer areas |
|  |  | [ ]  Black [ ]  Gray [ ]  Chameleon [ ]  White |  |  |
|  |  |  | **10.** | **Glass** |
| **5.** | **Door Catches**  |  | [ ]  | Float glass – clear 6mm – **Standard Default** |
|  | Roller – **Standard Default** |  | [ ]  | Safety glass – laminated 6 mm (framed) |
|  |  |  |  | **[ ]**  | Safety glass – tempered 6 mm (framed) |
|  |  |  |  |  |
|  |  |  | **11.** | **Security Panel (between locked sections)** |
|  |  |  |  | **[ ]**  | Without security panel  **– Standard Default** |
|  |  |  | [ ]  | With security panel |
|  |  |  |  |  |
|  |  | **12.** | **Suspension Hardware (for suspended cabinets)** |
|  |  |  |  | [ ]  | Hanger at MAX/Lab – **Standard Default** |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |   |  |  |  |