|  |  |  |  |
| --- | --- | --- | --- |
| **OOR Number**: |  | **Dealer:** |  |
| **Project Name:** |  | **Date:** |  |
|  | | | |

🡸 Check for **ALL** **Standard Default** selections

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **1.** | **Drawer Suspension** | | | | | | | |  | **6.** | **Lock Types** | |
|  |  | Self-closing, self-centering hold open feature | | | | | | |  | Designated by cabinet suffix “**L**” | |
|  |  | 100-pound drawer runs – **Standard Defaul**t | | | | | | |  |  | Master 5-disc – **Standard Default** |
|  |  | SEFA 8 150-pound, full-extension drawer slides  – **Standard on file drawers** | | | | | | |  |  | Use when up to 225 key changes are required (master-keyed) |
|  |  |  | | | | | | |  |  | Master 5-pin |
| **2.** | **Cabinet Hinges** | | | | | | | |  |  |  |
|  |  | Stainless steel – **Standard Default** | | | | | | | **7.** | **Label Holders** | |
|  |  | Black | | | | | | |  |  | None – **Standard Default** |
|  |  |  | | | | | | |  |  | One per door, one each drawer head |
| **3.** | **Pull Location** | | | | | | | |  |  | Stainless Steel  Black |
|  |  | Configuration 1 | | | | | | |  |  | One per *pair* of doors, one each drawer head |
|  |  | Horizontal on drawers, vertical on doors – **Standard Defaul**t | | | | | | |  |  | Stainless Steel  Black |
|  |  | Configuration 2 | | | | | | |  | ***Check “None” if full-width and semi-*** | |
|  |  | Horizontal on drawers and doors | | | | | | |  | ***recessed polypropylene pulls are selected*** | |
|  |  | Configuration 3 | | | | | | |  |  |  |
|  |  | Continuous full-width pull is horizontal on drawers, vertical pull on | | | | | | | **8.** | **Base Unit Shelf** | |
|  |  | doors | | | | | | |  |  | One-piece unit – **Standard Default** |
|  | ***Wall, upper and tall cases feature vertical pulls*** | | | | | | | |  |  | Split (two-piece) |
|  |  |  | | | | | | |  |  |  |
| **4a.** | **Pull Types –** Available in Configurations **1** and **2** **only** | | | | | | | | **9.** | **Removable Access Panel** | |
|  |  | Brushed aluminum rectangular pull – **Standard Default** | | | | | | |  | At base cabinets only – 100J/200J cupboard cabinets have removable | |
|  |  | Stainless steel wire pull | | | | | | |  | backs standard. For removable backs in 100J/200J series drawer or | |
|  |  |  | | | | | | |  | combination cabinets, select “at both cupboard and drawer areas” | |
| **4b.** | **Pull Types –** Available in Configuration **1** **only** | | | | | | | |  |  | At cupboard areas only – **Standard Default** |
|  |  | Semi-recessed polypropylene | | | | | | |  |  | At both cupboard and drawer areas |
|  |  | Black  Gray  Chameleon  White | | | | | | |  |  | |
|  |  |  | | | | | | | **10.** | **Glass** | |
| **5.** | **Door Catches** | | | | | | | |  |  | Float glass – clear 6mm – **Standard Default** |
|  | Roller – **Standard Default** | | | | | | | |  |  | Safety glass – laminated 6 mm (framed) |
|  |  |  | | | | | | |  |  | Safety glass – tempered 6 mm (framed) |
|  |  | | | | | | | |  |  |  |
|  |  |  | | | | | | | **11.** | **Security Panel (between locked sections)** | |
|  |  |  | | | | | | |  |  | Without security panel  **– Standard Default** |
|  |  | | | | | | | |  |  | With security panel |
|  |  | | | | | | | |  |  |  |
|  |  | | | | | | | | **12.** | **Suspension Hardware (for suspended cabinets)** | |
|  |  |  | | | | | | |  |  | Hanger at MAX/Lab – **Standard Default** |
|  |  | | | | | | | |  |  |  |
|  |  | | | | | | | |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  | |
|  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  | | | | | | |  |  |  |
|  |  | | | | | | | |  |  |  |
|  |  | | | | | | | |  |  |  |
|  |  | | | | | | | |  |  |  |