|  |  |  |  |
| --- | --- | --- | --- |
| **OOR Number**: |       | **Dealer:** |       |
| **Project Name:** |       | **Date:** |       |
|  |

[ ]  🡸 Check for **ALL** **Standard Default** selections

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **1.** | **Contrast Inset Steel Door/Drawer Front Style** |  | **7.** | **Lock Types** |
|  |  |  | Designated by cabinet suffix "**L**." |
| **1a.** | **Red Oak Wood Door/Drawer Front Style** |  | [ ]  | Master 5-Disc – **Standard Default** |
|  | **[ ]**  | Plain-sliced Oak (vertical matched grain) |  |  | Use when up to 225 primary key changes are required (master-keyed). |
|  | [ ]  | Rift-cut Red Oak (vertical matched grain) |  | [ ]  | Master 5-pin |
|  |  |  |  |  |
| **1b.** | **Maple (select White) Wood Door/Drawer Fronts** | **8.** | **Label Holders** |
|  | [ ]  | Plain-sliced Maple (vertical matched grain) |  | [ ]  | None – **Standard Default** |
|  | [ ]  | Rotary-cut Maple (vertical matched grain) |  | [ ]  | One each door, one each drawer head. |
|  |  |  |  | [ ]  Black  |
| **2.** | **Drawer Suspension** |  |  | [ ]  Stainless Steel |
|  | [ ]  | Self-closing, self-centering hold open feature. |  | **[ ]**  | One per *pair* of doors, one each drawer head. |
|  |  | 100-pound drawer runs. – **Standard Default** |  |  | **[ ]** Black  |
|  | [ ]  | SEFA 8 150-pound full extension drawer slides. |  |  | [ ]  Stainless Steel |
|  |  | – **Standard on file drawers.** |  | ***Check "None" if full-width and semi-recessed*** |
|  |  |  |  | ***polypropylene pulls are selected.*** |
| **3.** | **Cabinet Hinges** |  |  |  |
|  | **[ ]**  | Stainless steel – **Standard Default** | **9.** | **Base Unit Shelf** |
|  | **[ ]**  | Black  |  | [ ]  One piece – **Standard Default**   |
|  |  |  | [ ]  Split (two piece) |
| **4.** | **Pull Location** |  |  |
|  | [ ]  | Configuration 1 – Horizontal on drawers, vertical on doors. – **Standard Default** | **10.** | **Removable Access Panel** |
|  | **[ ]**  | Configuration 2 – Horizontal on drawers and base unit doors. |  | Available on 100S and 200S Series base cabinets only. |
|  | [ ]  | Configuration 3 (MAX style) – Horizontal on drawers and doors. |  | [ ]  | At cupboard areas only. – **Standard Default** |
|  |  | Single pull on drawers 30" and wider. |  | [ ]  | At both cupboard and drawer areas. |
|  | ***Wall, upper and tall cases feature vertical pulls****.* |  |  |  |
|  |  |  | **11.** | **Glass** |
| **5a.** | **Pull Types –** Available in Configurations **1** & **2** Only |  | [ ]  | Float glass – clear 6 mm. – **Standard Default** |
|  | [ ]  | Brushed aluminum rectangular pull. – **Standard Default** |  | **[ ]**  | Safety glass – laminated 6 mm (framed) |
|  | [ ]  | Stainless steel wire pull |  | [ ]  | Safety glass – tempered 6 mm (framed) |
|  |  |  |  |  |
| **5b.** | **Pull Types –** Available in Configuration **1**, **2** & **3** | **12.** | **Security Panels** (between locked sections) |
|  | [ ]  | Semi-recessed polypropylene. |  | [ ]  Without panel. – **Standard Default**  |
|  |  | [ ]  Black [ ]  Gray [ ]  Chameleon [ ]  White |  | [ ]  With panel |
|  |  |  |  |
| **6.** | **Door Catches** | **13.** | **Finish** (wood door and drawer fronts only) |
|  |  | Roller catch – **Standard Default** |  | [ ]  | SEFA 8 – **Standard Default** |
|  |  |  |  |  |
|  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |
|  |  |   |  |  |  |
|  |  |  |  |
|  |  |  |  |  |
|  |  |  |  | . |
|  |  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |