|  |  |  |  |
| --- | --- | --- | --- |
| **OOR Number**: |  | **Dealer:** |  |
| **Project Name:** |  | **Date:** |  |
|  | | | |

🡸 Check for **ALL** **Standard Default** selections

|  |  |  |  |
| --- | --- | --- | --- |
| **1.** | **Drawer Suspension** | | |
|  |  | Self-closing, self-centering, hold open feature. 100-pound drawer runs – **Standard Default** | |
|  |  | SEFA 8 150-pound full extension drawer slides – **Standard Default on file drawers** | |
|  | | | |
| **2.** | **Hinges** | | |
|  |  | Stainless steel – **Standard Default** | |
|  | | | |
| **3.** | **Pull Locations** | | |
|  | Standard MAX/Lab polypropylene pull locations – horizontal on base cabinet doors and drawers | | |
|  | – **Standard Default** | | |
|  |  | | ***Wall, upper, and tall cases feature vertical pulls*** |
|  | | | |
| **4.** | **Pull Types** | | |
|  |  | Semi-recessed polypropylene | |
|  |  |  | Chameleon – **Standard Default** |
|  |  |  | Black |
|  |  |  | Gray |
|  |  |  | White |
|  | | | |
| **5.** | **Door Catches** | | |
|  |  | Roller catch – **Standard Default** | |
|  | | | |
| **6.** | **Lock Types** | | |
|  | Designated by cabinet suffix “**L**” | | |
|  |  | Master 5-disc – **Standard Default**  Use when up to 225 primary key changes are required (master-keyed) | |
|  |  | Master 5-pin | |
|  | | | |
| **7.** | **Glass** | | |
|  | Framed and/or unframed doors | | |
|  |  | Float glass – clear 6 mm – **Standard Default** | |
|  |  | Safety glass – laminated 6 mm (framed) | |
|  |  | Safety glass – tempered 6 mm (framed) | |
|  | | | |
| **8.** | **Security Panel** | | |
|  | Between locked sections | | |
|  |  | Without security panel – **Standard Default** | |
|  |  | With security panel | |