|  |  |  |  |
| --- | --- | --- | --- |
| **OOR Number**: |  | **Dealer:** |  |
| **Project Name:** |  | **Date:** |  |
|  | | | |

🡸 Check for **ALL** **Standard Default** selections

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **1.** | **Cabinet Front: Flush Overlay Door/Drawer Head Style with** | |  | **7.** | **Label Holders** | | |
|  | **Radiused Vertical Edge Profile** | |  |  | None – **Standard Default** | |
|  | Steel flush overlay cabinet fronts provide modern styling with tight | |  |  | One per door, one each drawer head | |
|  | reveals between doors and drawers | |  |  | Stainless Steel  Black | |
|  |  | |  |  | One per *pair* of doors, one each drawer head |  |
| **2.** | **Drawer Suspension** | |  |  | Stainless Steel  Black | |
|  |  | Self-closing, self-centering, hold open feature |  |  | Full width on drawers, aluminum | |
|  |  | 100-pound drawer runs – **Standard Default** |  |  |  | |
|  |  | SEFA 8 150-pound, full-extension drawer slide – **Standard Default** | **8.** | **Base Unit Shelf** | | |
|  |  | **on file drawers** |  |  | One-piece unit – **Standard Default** | |
|  |  |  |  |  | Split (2-piece) | |
| **3.** | **Cabinet Hinges** | |  |  | | |
|  | Concealed Hinge – **Standard Default** | | **9**. | **Removable Access Panel** | | |
|  |  | |  | At base cabinets only | | |
| **4.** | **Pull Direction at Doors** | |  | 100J/200J cupboard cabinets have removable backs | | |
|  |  | Configuration 1 (Prestige Vertical) |  | as standard. For removable backs in 100J/200J | | |
|  |  | Horizontal on drawers, vertical on doors |  | series drawer or combination cabinets, select | | |
|  |  | Configuration 2 (Prestige Horizontal) |  | “At both cupboard and drawer areas” | | |
|  |  | Horizontal on drawers including base cabinet doors |  |  | At cupboard areas only – **Standard Default** | |
|  |  |  |  |  | At both cupboard and drawer areas | |
|  | ***Wall, upper and tall cases feature vertical pulls*** | |  |  |  | |
|  |  | | **10.** | **Glass** | | |
| **5.** | **Pull Types** | |  |  | Float glass – clear 6 mm – **Standard Default** | |
|  |  | Wire aluminum pull – Configuration **1 only** |  |  | Safety glass – laminated 6 mm (framed) | |
|  |  | Large sweep matt chrome wire pull – Configuration **1 only** |  |  | Safety glass – tempered 6mm (framed) | |
|  |  | Small sweep matt stainless steel wire pull – |  |  |  | |
|  |  | Configuration **1 only** | **11.** | **Security Panels** | | |
|  |  | Slotted nickel matt pull – Configuration **1 only** |  |  | Without security panel – **Standard Default** | |
|  |  | Contour matt stainless steel pull – Configuration **1 only** |  |  | With security panel | |
|  |  | Waterfall nickel matt pull – Configuration **2 only** |  |  |  | |
|  |  |  | **12.** | **Suspension Hardware** | | |
| **6.** | **Lock Types** | |  |  | Hanger at MAX/Lab – **Standard Default** | |
|  | Designated by cabinet suffix “**L**” | |  |  | | |
|  |  | Master 5-disc – **Standard Default** |  |  |  | |
|  |  | Use when up to 225 key changes are required (master-keyed) |  |  |  | |
|  |  | Master 5-pin |  |  |  | |
|  |  |  |  |  |  | |
|  | ***For Waterfall pull (No. 00028144), locks are not available on*** | |  |  |  | |
|  | ***15" wide drawer frames and base cabinets*** | |  |  | | |
|  |  |  |  |  | | |
|  |  |  |  |  |  | | |
|  |  |  |  |  |  | | |
|  |  |  |  |  |  | | |
|  |  |  |  |  |  | | |
|  |  |  |  |  |  | | |