|  |  |  |  |
| --- | --- | --- | --- |
| **OOR Number**: |       | **Dealer:** |       |
| **Project Name:** |       | **Date:** |       |
|  |

[ ]  🡸 Check for **ALL** **Standard Default** selections

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **1.** | **Cabinet Front: Flush Overlay Door/Drawer Head Style with** |  | **7.** | **Label Holders** |
|  | **Radiused Vertical Edge Profile** |  | [ ]  | None – **Standard Default** |
|  | Steel flush overlay cabinet fronts provide modern styling with tight |  | [ ]  | One per door, one each drawer head |
|  | reveals between doors and drawers  |  |  | [ ]  Stainless Steel [ ]  Black  |
|  |  |  | [ ]  | One per *pair* of doors, one each drawer head |  |
| **2.** | **Drawer Suspension** |  |  | [ ]  Stainless Steel [ ]  Black  |
|  | [ ]  | Self-closing, self-centering, hold open feature |  | [ ]  | Full width on drawers, aluminum |
|  |  | 100-pound drawer runs – **Standard Default** |  |  |  |
|  | [ ]  | SEFA 8 150-pound, full-extension drawer slide – **Standard Default**  | **8.** | **Base Unit Shelf** |
|  |  | **on file drawers** |  | [ ]  | One-piece unit – **Standard Default** |
|  |  |  |  | [ ]  | Split (2-piece) |
| **3.** | **Cabinet Hinges** |  |  |
|  | Concealed Hinge – **Standard Default** | **9**. | **Removable Access Panel** |
|  |  |  | At base cabinets only |
| **4.** | **Pull Direction at Doors** |  | 100J/200J cupboard cabinets have removable backs |
|  | [ ]  | Configuration 1 (Prestige Vertical) |  | as standard. For removable backs in 100J/200J |
|  |  | Horizontal on drawers, vertical on doors |  | series drawer or combination cabinets, select |
|  | **[ ]**  | Configuration 2 (Prestige Horizontal) |  | “At both cupboard and drawer areas” |
|  |  | Horizontal on drawers including base cabinet doors |  | [ ]  | At cupboard areas only – **Standard Default** |
|  |  |  |  | **[ ]**  | At both cupboard and drawer areas |
|  | ***Wall, upper and tall cases feature vertical pulls*** |  |  |  |
|  |  | **10.** | **Glass** |
| **5.** | **Pull Types**  |  | **[ ]**  | Float glass – clear 6 mm – **Standard Default** |
|  | [ ]  | Wire aluminum pull – Configuration **1 only** |  | **[ ]**  | Safety glass – laminated 6 mm (framed) |
|  | [ ]  | Large sweep matt chrome wire pull – Configuration **1 only** |  | [ ]  |  Safety glass – tempered 6mm (framed) |
|  | [ ]  | Small sweep matt stainless steel wire pull –  |  |  |  |
|  |  | Configuration **1 only** | **11.** | **Security Panels** |
|  | [ ]  | Slotted nickel matt pull – Configuration **1 only** |  | **[ ]**  | Without security panel – **Standard Default** |
|  | [ ]  | Contour matt stainless steel pull – Configuration **1 only** |  | **[ ]**  | With security panel |
|  | [ ]  | Waterfall nickel matt pull – Configuration **2 only** |  |  |  |
|  |  |  | **12.** | **Suspension Hardware** |
| **6.** | **Lock Types** |  | **[ ]**  | Hanger at MAX/Lab – **Standard Default** |
|  | Designated by cabinet suffix “**L**” |  |  |
|  | [ ]  | Master 5-disc – **Standard Default** |  |  |  |
|  |  | Use when up to 225 key changes are required (master-keyed) |  |  |  |
|  | [ ]  | Master 5-pin |  |  |  |
|  |  |  |  |  |  |
|  | ***For Waterfall pull (No. 00028144), locks are not available on*** |  |  |  |
|  | ***15" wide drawer frames and base cabinets***  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |