|  |  |  |  |
| --- | --- | --- | --- |
| **OOR Number**: |       | **Dealer:** |       |
| **Project Name:** |       | **Date:** |       |
|  |

[ ]  🡸 Check for **ALL** **Standard Default** selections

|  |  |
| --- | --- |
| **1.** | **Drawer Suspension** |
|  | [ ]  | SEFA 8 150-pound full extension drawer slides, zinc coated – **Standard Default** |
|  | [ ]  | 100-pound ¾ extension, stainless steel |
|  | [ ]  | 150-pound full extension, stainless steel |
|  |
| **2.** | **Hinges** |
|  | [ ]  | Stainless steel – **Standard Default**  |
|  |
| **3.** | **Pull Location** |
|  | Horizontal on drawers, vertical on doors – **Standard Default**  |
|  |
| **4.** | **Pull Types** |
|  | [ ]  | Stainless steel wire finger pull – **Standard Default**  |
|  |
| **5.** | **Door Catches** |
|  | [ ]  | Roller catch – **Standard Default** |
|  | [ ]  | Non-metallic catch  |
|  |
| **6.** | **Lock Types** |
|  | Only if designated by Cabinet suffix “**L**” |
|  | [ ]  | Master 5-disc – **Standard Default**Use when up to 225 primary key changes are required (master-keyed) |
|  | [ ]  | Master 5-Pin |
|  |  |  |
| **7.** | **Toe Space Soffit** |
|  | [ ]  | Without toe space soffit – **Standard Default** |
|  | [ ]  | With toe space soffit |
|  |  |  |
| **8.** | **Label Holders** |
|  | [ ]  | None – **Standard Default** |
|  | [ ]  | Stainless steel, one per door, one each drawer head |
|  | [ ]  | Stainless steel, one per *pair o*f doors, one each drawer head |
|  |  |  |
| **9.** | **Removable Access Panel** |
|  | [ ]  | At cupboard areas only – **Standard Default** |
|  | [ ]  | At both cupboard and drawer areas |
|  |  |  |
| **10.** | **Glass – Framed and/or Unframed Doors** |
|  | [ ]  | Float glass – clear 6mm – **Standard Default** |
|  | [ ]  | Safety glass – laminated 6mm (framed) |
|  | [ ]  | Safety glass – tempered 6mm (framed) |
|  |  |  |
| **11.** | **Security Panels Between Locked Sections** |
|  | [ ]  | Without security panel – **Standard Default** |
|  | [ ]  | With security panel |