|  |  |  |  |
| --- | --- | --- | --- |
| **OOR Number**: |       | **Dealer:** |   |
| **Project Name:** |       | **Date:** |       |
|  |

[ ]  🡸 Check for **ALL** **Standard Default** selections

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **1.** | **Drawer Suspension** |  | **7.** | **Label Holders** |
|  | [ ]  | Self-closing, self-centering, hold open feature |  | [ ]  | None – **Standard Default** |
|  |  | 100-pound drawer runs – **Standard Default** |  | [ ]  | One per door, one each drawer head |
|  | [ ]  | SEFA 8 – 150-pound full extension drawer slides |  |  | [ ]  Black [ ]  Stainless Steel |
|  |  | – **Standard on file drawers** |  | [ ]  | One per *pair* of doors, one each drawer head |
|  |  |  |  |  | [ ]  Black [ ]  Stainless Steel |
| **2.** | **Hinges** |  | ***Check “None” if full-width and semi-recessed*** |
|  | [ ]  | Stainless steel – **Standard Default** |  | ***polypropylene pulls are selected*** |
|  | [ ]  | Black  |  |  |  |
|  |  |  | **8.** | **Base Unit Shelf** |
| **3.** | **Pull Location** |  | [ ]  | One piece – **Standard Default** |
|  | [ ]  | Configuration 1 – **Standard Default** |  | [ ]  | Split (two pieces) |
|  |  | Horizontal on drawers, vertical on doors |  |  |  |
|  | [ ]  | Configuration 2 | **9.** | **Removable Access Panel** |
|  |  | Horizontal on drawers and base unit doors |  | Available on 100S and 200S Series base cabinets |
|  | [ ]  | Configuration 3  |  | **only** |
|  |  | Horizontal, 1 per door/drawer, centered left to right |  | [ ]  | At cupboard areas only – **Standard Default** |
|  | [ ]  | Configuration 4 |  | [ ]  | At both cupboard and drawer areas |
|  |  | Full width, horizontal on drawers; vertical on doors |  |  |  |
|  |  |  | **10.** | **Glass**  |
| **4a.** | **Pull Types**  |  | [ ]  | 6 mm clear float glass – **Standard Default** |
|  | Available in Configurations **1** and **2** **only** |  | [ ]  | 6 mm tempered safety glass (framed) |
|  | [ ]  | Stainless steel wire pull – **Standard Default** |  | [ ]  | 6 mm laminated safety glass (framed) |
|  | [ ]  | Brushed aluminum rectangular pull |  |  |  |
|  |  |  | **11.** | **Security Panel – Between Locked Sections** |
| **4b.** | **Pull Types** |  | [ ]  | Without security panel – **Standard Default** |
|  | Available in Configurations **1,** **2** and **3** only |  | [ ]  | With security panel |
|  | [ ]  | Semi-recessed polypropylene pull |  |  |
|  |  | [ ]  Chameleon [ ]  Black [ ]  Gray [ ]  White |  |  |
|  |  |  |  |  |
| **5.** | **Door Catches** |  |  |  |
|  | [ ]  | Roller – **Standard Default** |  |  |  |
|  |  |  |  |  |  |
| **6.** | **Lock Types**  |  |  |
|  | Designated by cabinet suffix “**L**” |  |  |
|  | **[ ]**  | Master 5-disc – **Standard Default** |  |  |
|  |  | Use when up to 225 key changes are required (master-keyed) |  |  |  |
|  | [ ]  | Master 5-pin |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |