|  |  |  |  |
| --- | --- | --- | --- |
| **OOR Number**: |  | **Dealer:** |  |
| **Project Name:** |  | **Date:** |  |
|  | | | |

🡸 Check for **ALL** **Standard Default** selections

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **1.** | **Drawer Suspension** | | | | | | | |  | **7.** | **Label Holders** | |
|  |  | Self-closing, self-centering, hold open feature | | | | | | |  |  | None – **Standard Default** |
|  |  | 100-pound drawer runs – **Standard Default** | | | | | | |  |  | One per door, one each drawer head |
|  |  | SEFA 8 – 150-pound full extension drawer slides | | | | | | |  |  | Black  Stainless Steel |
|  |  | – **Standard on file drawers** | | | | | | |  |  | One per *pair* of doors, one each drawer head |
|  |  |  | | | | | | |  |  | Black  Stainless Steel |
| **2.** | **Hinges** | | | | | | | |  | ***Check “None” if full-width and semi-recessed*** | |
|  |  | Stainless steel – **Standard Default** | | | | | | |  | ***polypropylene pulls are selected*** | |
|  |  | Black | | | | | | |  |  |  |
|  |  |  | | | | | | | **8.** | **Base Unit Shelf** | |
| **3.** | **Pull Location** | | | | | | | |  |  | One piece – **Standard Default** |
|  |  | Configuration 1 – **Standard Default** | | | | | | |  |  | Split (two pieces) |
|  |  | Horizontal on drawers, vertical on doors | | | | | | |  |  |  |
|  |  | Configuration 2 | | | | | | | **9.** | **Removable Access Panel** | |
|  |  | Horizontal on drawers and base unit doors | | | | | | |  | Available on 100S and 200S Series base cabinets | |
|  |  | Configuration 3 | | | | | | |  | **only** | |
|  |  | Horizontal, 1 per door/drawer, centered left to right | | | | | | |  |  | At cupboard areas only – **Standard Default** |
|  |  | Configuration 4 | | | | | | |  |  | At both cupboard and drawer areas |
|  |  | Full width, horizontal on drawers; vertical on doors | | | | | | |  |  |  |
|  |  |  | | | | | | | **10.** | **Glass** | |
| **4a.** | **Pull Types** | | | | | | | |  |  | 6 mm clear float glass – **Standard Default** |
|  | Available in Configurations **1** and **2** **only** | | | | | | | |  |  | 6 mm tempered safety glass (framed) |
|  |  | Stainless steel wire pull – **Standard Default** | | | | | | |  |  | 6 mm laminated safety glass (framed) |
|  |  | Brushed aluminum rectangular pull | | | | | | |  |  |  |
|  |  |  | | | | | | | **11.** | **Security Panel – Between Locked Sections** | |
| **4b.** | **Pull Types** | | | | | | | |  |  | Without security panel – **Standard Default** |
|  | Available in Configurations **1,** **2** and **3** only | | | | | | | |  |  | With security panel |
|  |  | Semi-recessed polypropylene pull | | | | | | |  |  | |
|  |  | Chameleon  Black  Gray  White | | | | | | |  |  | |
|  |  |  | | | | | | |  |  | |
| **5.** | **Door Catches** | | | | | | | |  |  |  |
|  |  | Roller – **Standard Default** | | | | | | |  |  |  |
|  |  |  | | | | | | |  |  |  |
| **6.** | **Lock Types** | | | | | | | |  |  | |
|  | Designated by cabinet suffix “**L**” | | | | | | | |  |  | |
|  |  | Master 5-disc – **Standard Default** | | | | | | |  |  | |
|  |  | Use when up to 225 key changes are required (master-keyed) | | | | | | |  |  |  |
|  |  | Master 5-pin | | | | | | |  |  |  |
|  |  |  | | | | | | |  |  |  |
|  |  |  | | | | | | |  |  | |
|  |  |  | | | | | | |  |  |  |
|  |  |  | | | | | | |  |  |  |
|  |  |  | | | | | | |  |  |  |
|  |  | | | | | | | |  |  |  |
|  |  | | | | | | | |  |  | |
|  |  |  | | | | | | |  |  |  |
|  |  | | | | | | | |  |  |  |
|  |  | | | | | | | |  |  |  |
|  |  | | | | | | | |  |  | |
|  |  |  | | | | | | |  |  | |
|  |  | |  |  |  |  |  |  |  |  |  |
|  |  | |  |  |  |  |  |  |  |  |  |
|  |  | |  |  |  |  |  |  |  |  |  |
|  |  |  | | | | | | |  |  |  |
|  |  |  | | | | | | |  |  |  |
|  |  |  | | | | | | |  |  |  |  |
|  |  | | | | | | | |  |  |  |  |