SPRAYON PRODUCTS -- 00607 BELT DRESSING AEROSOL -- 8030-00-018-9525
=======================================================
MSDS Safety Information 
=======================================================
FSC: 8030
NIIN: 00-018-9525
MSDS Date: 05/18/1989
MSDS Num: BHHDW
Tech Review: 01/22/1990
Product ID: 00607 BELT DRESSING AEROSOL
Responsible Party
Cage: 09800
Name: SPRAYON PRODUCTS
Address: 26300 FARGO AVENUE
Box: NK
City: BEDFORD HEIGHTS OH 44146 US
Info Phone Number: (216) 292-7400
Emergency Phone Number: (216) 292-7400
Preparer's Name: NK
=======================================================
Preparer Co. when other than Responsible Party Co. 
=======================================================
Cage: 09800
Assigned Ind: N
Name: SHERWIN-WILLIAMS DIVERSIFIED BRANDS, INC.
Address: 26300 FARGO AVENUE
City: BEDFORD HEIGHTS OH 44146
=======================================================
Contractor Summary 
=======================================================
Cage: 09800
Name: SHERWIN-WILLIAMS DIVERSIFIED BRANDS, INC.
Address: 26300 FARGO AVENUE
City: BEDFORD HEIGHTS OH 44146 US
Phone: 216-292-7400 OR 216-595-8634
=======================================================
Item Description Information 
=======================================================
Item Manager: GSA
Item Name: BELT DRESSING,PRESERVATIVE
Specification Number: NK
Type/Grade/Class: NK
Unit of Issue: CN
Quantitative Expression: 00000000016OZ
UI Container Qty: 1
Type of Container: METAL
=======================================================
Ingredients 
=======================================================
Cas: 8052-41-3
RTECS #: WJ8925000
Name: STODDARD SOLVENT
% by Wt: <5
Other REC Limits: NK
OSHA PEL: 500 PPM
ACGIH TLV: 100 PPM; 9293
Ozone Depleting Chemical: N
------------------------------
Cas: 71-55-6
RTECS #: KJ2975000
Name: METHYL CHLOROFORM (1,1,1-TRICHLOROEHANE)	(SARA III)
% by Wt: 45
Other REC Limits: NK
OSHA PEL: 350 PPM/450 STEL
ACGIH TLV: 350 PPM/450STEL;9192
EPA Rpt Qty: 1000 LBS
DOT Rpt Qty: 1000 LBS
Ozone Depleting Chemical: 1
------------------------------
Cas: 75-28-5
RTECS #: TZ4300000
Name: ISOBUTANE
% by Wt: 10
Other REC Limits: NK
OSHA PEL: 1000 PPM
ACGIH TLV: 1000 PPM 1800 MG/M3
Ozone Depleting Chemical: N
------------------------------
Cas: 74-98-6
RTECS #: TX2275000
Name: PROPANE
% by Wt: 10
Other REC Limits: NK
OSHA PEL: 1000 PPM
ACGIH TLV: ASPHYXIANT; 9192
Ozone Depleting Chemical: N
=======================================================
Health Hazards Data 
=======================================================
LD50 LC50 Mixture: NK
Route Of Entry Inds - Inhalation: YES
Skin: YES
Ingestion: YES
Effects of Exposure: IN CONFINED AREA VAPORS IN HIGH CONCENTRATION ARE
  ANESTHETIC.IRR TO SKIN/UPPER	RESPIRATORY SYS.OVER-EXPOSURE MAY RESULT
  IN LIGHT HEADNESS,STAG GAIT,GIDDINESS  AND POSS NAUSEA.HARMFUL OR FATAL
  IF SWAL LOWED.CHRONIC:REPEATED/PROLONGED OVER-EXPOSURE,PERMANENT
  BRAIN/NERVOUS SYS DAMAGE,KIDNEY AND LIVER DAMAGE.
Explanation Of Carcinogenicity: NK
Signs And Symptions Of Overexposure: IRRITATION TO SKIN & UPPER
  RESPIRATORY SYSTEM, LIGHT HEADEDNESS, STAGGERING GAITGIDDINESS, POSSIBLE
  NAUSEA. CHRONIC: PERMANENT BRAIN, NERVOUS SYSTEM DAMAGE.    POSSIBLE
  KIDNEY AND LIVER DAMAGE.
Medical Cond Aggravated By Exposure: NONE KNOWN.
First Aid: INHALE: REMOVE PATIENT TO FRESH AIR. EYES: FLUSH WITH WATER FOR
  AT LEAST 15 MIN.SKIN: WASH WITH SOAP AND WATER. INGESTED: CALL PHYSICIAN
  IMMEDIATELY. DO NOT	 INDUCE VOMITING.
=======================================================
Handling and Disposal
=======================================================
Spill Release Procedures: REMOVE ALL SOURCES OF IGNITION, VENTILATE AREA. 
   AVOID BREATHING VAPORS. REMOVE WITH INERT	     ABSORBENT.
Neutralizing Agent: NONE KNOWN.
Waste Disposal Methods: DO NOT INCINERATE. DISPOSE OF IN ACCORDANCE WITH 
  FEDERAL, STATE AND LOCAL REGULATIONS REGARDING    POLLUTION.
Handling And Storage Precautions: DO NOT STORE ABOVE 120 F. KEEP AT ROOM
  TEMPERATUREAS EXPOSURE TO DIRECT SUNLIGHT OR HEAT MAY CAUSE  BURSTING.
Other Precautions: KEEP AWAY FROM CHILDREN. DO NOT PUNCTURE OR INCINERATE.
  DO NOT SPRAY NEAR FIRE  OR OPEN FLAME.
=======================================================
Fire and Explosion Hazard Information 
=======================================================
Flash Point Text: NK
Autoignition Temp Text: NK
Lower Limits: NK
Upper Limits: NK
Extinguishing Media: CARBON DIOXIDE, DRY CHEMICAL OR FOAM.
Fire Fighting Procedures: WATER MAY BE INEFFECTIVE. BUT WATER MAY BE USED
  TO KEEP FIRE EXPOSED CONTAINERS COOL.
Unusual Fire/Explosion Hazard: DO NOT SPRAY NEAR OPEN FLAME. KEEP AT ROOM
  TEMPERATURE AS EXPOSURE TO DIRECT    SUNLIGHT OR OTHER HEAT MAY CAUSE
  BURSTING.
=======================================================
Control Measures 
=======================================================
Respiratory Protection: AVOID BREATHING OF VAPOR OR SPRAY MIST.
Ventilation: PROVIDE LOCAL EXHAUST VENTILATION IN VOLUME/PATTERN TO KEEP
  TLV OF ALL HAZARDOUS INGREDIENT BELOW ACCEPTABLE LIMIT.
Protective Gloves: RECOMMENDED FOR PROLONGED/REPEATED USE.
Eye Protection: SAFETY GLASSES W/UNPERFORATED SIDESHIELD
Other Protective Equipment: NONE KNOWN.
Work Hygienic Practices: NONE KNOWN.
Supplemental Safety and Health: NONE KNOWN.
=======================================================
Physical/Chemical Properties 
=======================================================
NRC/State LIC No: NK
B.P. Text: NK
M.P/F.P Text: NK
Decomp Text: NK
Vapor Pres: NK
Vapor Density: > AIR
Spec Gravity: NK
PH: NK
Viscosity: NK
Evaporation Rate & Reference: FASTER THAN ETHER
Solubility in Water: NK
Appearance and Odor: COATINGS.
Percent Volatiles by Volume: 75
Corrosion Rate: NK
=======================================================
Reactivity Data 
=======================================================
Stability Indicator: YES
Stability Condition To Avoid: DO NOT STORE ABOVE 120 F.
Materials To Avoid: NONE KNOWN.
Hazardous Decomposition Products: CARBON MONOXIDE, CARBON DIOXIDE,
  HYDROGEN CHLORIDE AND      PHOSGENE GAS.
Hazardous Polymerization Indicator: NO
Conditions To Avoid Polymerization: NONE KNOWN.
=======================================================
Toxicological Information 
=======================================================
=======================================================
Ecological Information 
=======================================================
=======================================================
MSDS Transport Information 
=======================================================
=======================================================
Regulatory Information 
=======================================================
=======================================================
Other Information 
=======================================================
=======================================================
Transportation Information 
=======================================================
Responsible Party Cage: 09800
Trans ID NO: 43797
Product ID: 00607 BELT DRESSING AEROSOL
MSDS Prepared Date: 05/18/1989
Review Date: 01/22/1990
Article W/O MSDS: N
Tech Entry NOS Shipping Nm: NONE KNOWN.
Coast Guard AMMO Code: NK
Net Unit Weight: NK
AF MMAC Code: NK
Multiple KIT Number: 0
Unit Of Issue: CN
Container QTY: 1
Type Of Container: METAL
Additional Data: CONTENTS UNDER PRESSURE.
=======================================================
Detail DOT Information 
=======================================================
DOT PSN Code: DTJ
Symbols: D
DOT Proper Shipping Name: CONSUMER COMMODITY
Hazard Class: ORM-D
Label: NONE
Non Bulk Pack: 156,306
Bulk Pack: NONE
Max Qty Pass: 30KGGROSS
Max Qty Cargo: 30KGGROSS
Vessel Stow Req: A
=======================================================
Detail IMO Information 
=======================================================
IMO PSN Code: AKH
IMO Proper Shipping Name: AEROSOLS/AEROSOL PRODUCT ?
IMDG Page Number: SEE 9022
UN Number: 1950
UN Hazard Class: 9?
IMO Packaging Group: -
Subsidiary Risk Label: -
EMS Number: 2-13
=======================================================
Detail IATA Information 
=======================================================
IATA PSN Code: ALS
IATA UN ID Num: 1950
IATA Proper Shipping Name: AEROSOLS, FLAMMABLE
IATA PSN Modifier: (EACH NOT EXCEEDING 1 L CAPACITY)
IATA UN Class: 2.1
IATA Label: FLAMMABLE GAS
Packing Note Passenger: 203
Max Quant Pass: 75KG
Max Quant Cargo: 150KG
Packaging Note Cargo: 203
=======================================================
Detail AFI Information 
=======================================================
AFI PSN Code: ALS
AFI Proper Shipping Name: AEROSOLS, NONFLAMMABLE, N.O.S.
AFI PSN Modifier: CONTAINING SUBSTANCES IN CLASS 8, PACKING GROUP I OR II
AFI Hazard Class: FORB
Back Pack Reference: FORBIDDEN
=======================================================
HAZCOM Label 
=======================================================
Product ID: 00607 BELT DRESSING AEROSOL
Cage: 09800
Company Name: SHERWIN-WILLIAMS DIVERSIFIED BRANDS, INC.
Street: 26300 FARGO AVENUE
City: BEDFORD HEIGHTS OH
Zipcode: 44146 US
Health Emergency Phone: 216-292-7400
Date Of Label Review: 12/16/1998
Label Date: 12/16/1998
Hazard And Precautions: VAPORS MAY CAUSE DIZZINESS OR SUFFOCATION. CONTACT
  WITH LIQUID MAY CAUSE FROSTBITE. FIRE MAY PRODUCE IRRITATING OR
  POISONOUS GASES.
=======================================================
Disclaimer (provided with this information by the compiling agencies):
  This information is formulated for use by elements of the Department of
  Defense. The United States of America in no manner whatsoever expressly
  or implied warrants, states, or intends said information to have any
  application, use or viability by or to any person or persons outside the
  Department of Defense nor any person or persons contracting with any
  instrumentality of the United States of America and disclaims all
  liability for such use. Any person utilizing this instruction who is not
  a military or civilian employee of the United States of America should
  seek competent professional advice to verify and assume responsibility
  for the suitability of this information to their particular situation
  regardless of similarity to a corresponding Department of Defense or
  other government situation.