ENERPAC HF-100 HYDRAULIC OIL: ENERPAC,DIVISION OF APPLIED POWDER

 =========== 1.	Product Identification ===========
 
 Product ID:ENERPAC HF-100 HYDRAULIC OIL
 MSDS Date:01/01/1987
 Tech Review:11/15/1988
 FSC:9150
 NIIN:LIIN:00F005368
 Submitter:F BT
 MFN:01
 === Responsible Party ===
 Company Name:ENERPAC,DIVISION OF APPLIED POWDER
 Address:13000 W. SILVER SPRING DR
 Box:N/R
 City:BUTLER
 State:WI
 ZIP:53007
 Country:US
 Info Phone Num:414-781-6600
 Emergency Phone Num:414-781-6600
 Review Ind:Y
 Published:Y
 CAGE:FO058
 === Contractor Identification ===
 Company Name:APPLIED POWER INC ENERPAC DIV
 Address:13000 W SILVER SPRING DR
 Box:City:BUTLER
 State:WI
 ZIP:53007-1093
 Country:US
 Phone:414-781-6600
 CAGE:26952
 Company Name:ENERPAC,DIVISION OF APPLIED POWDER
 Address:13000 W. SILVER SPRING DR
 Box:N/R
 City:BUTLER
 State:WI
 ZIP:53007
 Country:US
 Phone:414-781-6600
 CAGE:FO058
 === Item Description Information ===
 Item Name:HIGH PERFORMANCE COATINGS
 Type of Container:
 
 =========== 2.	Composition/Information on Ingredients ===========
 
 Ingred Name:PARAFFINIC LUBE STOCKS
 Fraction by Wt: 96-100%
 Other REC Limits:5MG/CUM
 Ozone Depleting Chemical:Ingred Name:ANTI-WEAR HYDRAULIC OIL ADDITIVE
     CONTAINING(ZINC DITHIOPHOSPHATE)
 Fraction by Wt: 0-3%
 Ozone Depleting Chemical:Ingred Name:METHACRYLATEPOLYMER
 Fraction by Wt: 0-1%
 Ozone Depleting Chemical:Ingred Name:BLUE DYE
 Fraction by Wt: TRACE
 Ozone Depleting Chemical:
 
 =========== 3.	Hazards Identification ===========
 
 =Routes of Entry=
  Inhalation:YES
 Skin:YES
 Ingestion:YES
 =Reports of Carcinogenicity=
 Health Hazards Acute and Chronic:ACUTE:IRRITATION OF EYES AND SKIN.
     CHRONIC:MILD SKIN IRRITATION.
 Effects of Overexposure:PROLONGED OR REPEATED SKIN CONTACT MAY CAUSE
     MILD SKIN IRRITATION.
 Medical Cond Aggravated by Exposure:NO DATA AVAILABLE.
 
 =========== 4.	First Aid Measures ===========
 
 First Aid:IN CASE OF SKIN CONTACT, WASH W/SOAP & WATER. EYES: FLUSH
     W/WATER FOR 15 MINS, INCLUDING UNDER EYELIDS. IF IRRIT PERSISTS,
     GET MED HELP. INHALATION: REMOVE TO FRESH AIR. GET MED HELP IF
     IRRIT PERSISTS . INGESTION: DON'T INDUCE VOMITING. CONSULT PHYS
 
 =========== 5.	Fire Fighting Measures ===========
 
 Flash Point:Flash Point Text:400F/204C (COC)
 Extinguishing Media:FOAM,DRY CHEMICAL,CO*2.
 Fire Fighting Procedures:DON'T USE WATER SPRAY. WATER COOL CONTAINERS.
 Unusual Fire/Explosion Hazard:DON'T MIX WITH STRONG OXIDANTS LIKE
     LIQUID CHLORINE OR CONCENTRATED OXYGEN.
 
 =========== 6.	Accidental Release Measures ===========
 
 Spill Release Procedures:RECOVER FREE LIQUID. ADD ABSORBENT (SAND,
     EARTH, SAWDUST, ETC.) TO SPILL AREA. KEEP TROLEUM PRODUCTS OUT OF
     SEWERS/WATERCOURSES BY DIKING OR IMPOUNDING. ADVE AUTHORITIES OF
     PRODUCT HAS ENTERED SEWERS,  WATERCOURSES OR EXTENSIVE LD AREAS.
 
 =========== 7.	Handling and Storage ===========
 
 Handling and Storage Precautions:KEEP CONTAINER CLOSED WHEN NOT IN USE.
     DON'T HANDLE OR STORE NEAR HEAT, SPARK, FLAME OR STRONGXIDANTS.
 Other Precautions:AVOID BREATHING OIL MIST. REMOVE OIL SOAKED CLOTHING
     AND LAUNDER BEFORE REUSE. DISCARD OIL SOAKED SHOES. WASH SKIN WITH
     SOAPND WATER AFTER HANDLING.
 
 =========== 8.	Exposure Controls/Personal Protection ===========
 
 Respiratory Protection:USE SUPPLIED AIR RESPIRATORY PROTECTION IN
     CONFINED/ENCLOSED SPACES.
 Ventilation:PROVIDE LOCAL TO CAPTURE FUMES & VAPORS/>60 FPM HOOD.
 Protective Gloves:CHEM-RESISTANT
 Eye Protection:GOGGLES OR FACE SHIELD
 Other Protective Equipment:USE CHM-RESISTANT APRON/CLOTHING. AVOID
     PROLONGED SKIN CONT.
 Supplemental Safety and Health
 MSDS DATE: 5/85.
 
 =========== 9.	Physical/Chemical Properties ===========
 
 HCC:V6
 NRC/State Lic Num:N/R
 Boiling Pt:B.P. Text:670F
 Vapor Pres:.01
 Vapor Density:12
 Spec Gravity:0.87
 Evaporation Rate & Reference:(BU AC = 1): 0.01
 Solubility in Water:NEGLIGIBLE
 Appearance and Odor:CLEAR BLUE NON-VISCOUS LIQ, VERY SLGT HYDROCBN.
 Percent Volatiles by Volume:NONE
 
 =========== 10.  Stability and Reactivity Data ===========
 
 Stability Indicator/Materials to Avoid:YES
 STRONG OXIDANTS LIKE: LIQUID CHLORINE, CONCENTRATED OXYGEN.
 Hazardous Decomposition Products:FUMES/SMOKE/CO/SULFUR OXIDES/IN CASE
     OF INCOM COMBUSTION.
 Hazardous Polymerization Indicator:NO
 
 =========== 11.  Toxicological Information ===========

 =========== 12.  Ecological Information ===========

 =========== 13.  Disposal Considerations ===========
 
 Waste Disposal Methods:ASSURE CONFORMITY WITH APPLICABLE DISPOSAL
     REGULATIONS. DISPOSE OF ABSORBED MATERIAL AT A LICENSED WASTE
     DISPOSAL SITE OR FACITITY.
 
 =========== 14.  MSDS Transport Information ===========

 =========== 15.  Regulatory Information ===========

 =========== 16.  Other Information ===========

 ===============================================================
  Disclaimer (provided with this information by the compiling agencies):
  This information is formulated for use by elements of the Department
  of Defense.  The United States of America in no manner whatsoever,
  expressly or implied, warrants this information to be accurate and
  disclaims all liability for its use.  Any person utilizing this
  document should seek competent professional advice to verify and
  assume responsibility for the suitability of this information to their
  particular situation.