SPRAYON PRODUCTS -- 2X987B  BELT DRESSING -- 9150-00F031097
=======================================================
MSDS Safety Information 
=======================================================
FSC: 9150
MSDS Date: 02/06/1991
MSDS Num: BSMPT
LIIN: 00F031097
Tech Review: 11/16/1993
Product ID: 2X987B  BELT DRESSING
Responsible Party
Cage: 09800
Name: SPRAYON PRODUCTS
Address: 26300 FARGO AVE
City: BEDFORD HTS OH 44146-1310 US
Info Phone Number: 216-292-7400
Emergency Phone Number: 216-292-7400
=======================================================
Preparer Co. when other than Responsible Party Co. 
=======================================================
Cage: 09800
Assigned Ind: N
Name: SHERWIN-WILLIAMS DIVERSIFIED BRANDS, INC.
Address: 26300 FARGO AVENUE
City: BEDFORD HEIGHTS OH 44146
=======================================================
Contractor Summary 
=======================================================
Cage: 09800
Name: SHERWIN-WILLIAMS DIVERSIFIED BRANDS, INC.
Address: 26300 FARGO AVENUE
City: BEDFORD HEIGHTS OH 44146 US
Phone: 216-292-7400 OR 216-595-8634
=======================================================
Ingredients 
=======================================================
Cas: 74-98-6
RTECS #: TX2275000
Name: PROPANE
% by Wt: 10
Other REC Limits: 1800 MG/CUM
OSHA PEL: 1000 PPM
ACGIH TLV: SIMPLE ASPHYXIANT
Ozone Depleting Chemical: N
------------------------------
Cas: 75-28-5
RTECS #: TZ4300000
Name: ISOBUTANE, 2-METHYLPROPANE
% by Wt: 10
Other REC Limits: 1000 PPM
OSHA PEL: 1800 MG/CUM
ACGIH TLV: 1000 PPM
Ozone Depleting Chemical: N
------------------------------
Cas: 8052-41-3
RTECS #: WJ8925000
Name: STODDARD SOLVENT (PETROLEUM DISTILLATE), MINERAL SPIRITS
% by Wt: <5
Other REC Limits: 525 MG/CUM
OSHA PEL: 500 PPM
ACGIH TLV: 100 PPM
Ozone Depleting Chemical: N
------------------------------
Cas: 71-55-6
RTECS #: KJ2975000
Name: METHYL CHLOROFORM (1,1,1-TRICHLOROETHANE) (CHLOROTHENE NU),
  AEROTHANE TT, CHLOROTHENE
% by Wt: 50
Other REC Limits: 450 PPM STEL
OSHA PEL: 350 PPM
ACGIH TLV: 1910 MG/CUM
EPA Rpt Qty: 1000 LBS
DOT Rpt Qty: 1000 LBS
Ozone Depleting Chemical: 1
=======================================================
Health Hazards Data 
=======================================================
Route Of Entry Inds - Inhalation: YES
Skin: NO
Ingestion: YES
Carcinogenicity Inds - NTP: NO
IARC: NO
OSHA: NO
Effects of Exposure: EYES, SKIN & RESPIRATORY SYSTEM: IRRITATION. MAY
  CAUSE NERVOUS SYSTEM DEPRESSION & CAN BE FATAL. OVEREXPOSURE TO SOLVENTS
  MAY CAUSE PERMANENT BRAIN & NERVOUS SYSTEM DAMAGE & ADVERSE EFFECTS TO
  LIVER/U RINARY & CARDIOVASCULAR SYSTEMS.
Explanation Of Carcinogenicity: NONE
Signs And Symptions Of Overexposure: EYES/SKIN: REDNESS, ITCHING, BURNING
  SENSATION. INHALATION: HEADACHE, DIZZINESS, NAUSEA, LOSS OF
  COORDINATION.
First Aid: INHALATION: REMOVE FROM EXPOSURE. RESTORE BREATHING IF STOPPED.
  KEEP WARM & QUIET. SKIN: WASH W/SOAP & WATER. EYES: FLUSH W/WATER FOR 15
  MINS. INGESTION: DON'T INDUCE VOMITING. GIVE SEVERAL GLASSES OF  WATER.
  NEVER GIVE ANYTHING BY MOUTH TOAN UNCONSCIOUS PERSON. OBTAIN MEDICAL
  ATTENTION IN ALL CASES.
=======================================================
Handling and Disposal
=======================================================
Spill Release Procedures: REMOVE IGNITION SOURCES. VENTILATE AREA. REMOVE
  W/ABSORBANT.
Waste Disposal Methods: WASTE MAY BE HAZARDOUS & MUST BE TESTED FOR
  IGNITABILITY. DON'T INCINERATE OR DEPRESSURIZE CONTAINERS. DISPOSE I/A/W
  LOCAL, STATE & FEDERAL REGULATIONS. EXTREMELY FLAMMABLE.
Handling And Storage Precautions: KEEP AWAY FROM IGNITION SOURCES. KEEP
  AREA VENTILATED. DON'T SMOKE. USE APPROVED BONDING & GROUNDING
  PROCEDURES. DON'T PUNCTURE/EXPOSE TO TEMP >120F.
Other Precautions: DON'T TAKE INTERNALLY. KEEP OUT OF REACH OF CHILDREN.
  INTENTIONAL MISUSE BY DELIBERATELY CONCENTRATING & INHALING THE CONTENTS
  CAN BE HARMFUL/FATAL. AVOID BREATHING VAPORS/SPRAY MIST & CONTACT W/SKIN
   & EYES.
=======================================================
Fire and Explosion Hazard Information 
=======================================================
Flash Point Method: PMCC
Flash Point Text: <0F
Lower Limits: 1%
Upper Limits: 7%
Extinguishing Media: CO2, FOAM, DRY CHEMICAL
Fire Fighting Procedures: WEAR FULL PROTECTIVE CLOTHING & SCBA. WATER
  STREAM MY BE INEFFECTIVE, USE WATER FOG. USE WATER TO COOL CONTAINERS &
  PREVENT AUTOIGNITION OR EXPLOSION.
Unusual Fire/Explosion Hazard: CLOSED CONTAINERS MAY EXPLODE DUE TO
  BUILT-UP PRESSURE WHEN EXPOSED TO EXTREME HEAT. VAPORS WILL ACCUMULATE
  READILY & IGNITE EXPLOSIVELY.
=======================================================
Control Measures 
=======================================================
Respiratory Protection: IF EXPOSURE ABOVE LIMITS, WEAR A PROPERLY FITTED
  ORGANIC VAPOR/PARITCULATE RESPIRATOR APPROVED BY NIOSH/MSHA. WHEN
  SANDING/ABRADING DRIED FILM, WEAR A DUST/MIST RESPIRATOR APPROVED BY
  NIOSH/MSHA.
Ventilation: IF EXPOSURE ABOVE LIMITS, USE LOCAL OR GENERAL EXHAUST.
Protective Gloves: REQUIRED
Eye Protection: SAFETY GLASSES W/SIDESHILDS
Work Hygienic Practices: WASH THOROUGHLY AFTER HANDLING. REMOVE/LAUNDER
  CLOTHING BEFORE REUSE.
Supplemental Safety and Health: PRODUCT MAY CONTAIN MATERIALS CLASSIFIED
  AS NUISANCE PARTICULATES WHICH MAY BE PRESENT AT HAZARDOUS LEVELS ONLY
  DURING SANDING & ABRADING OF THE DRIED FILM.
=======================================================
Physical/Chemical Properties 
=======================================================
B.P. Text: <0-292F
Vapor Density: >1
Evaporation Rate & Reference: FASTER THAN ETHER
Percent Volatiles by Volume: >75
=======================================================
Reactivity Data 
=======================================================
Stability Indicator: YES
Stability Condition To Avoid: EXTREME HEAT, TEMP >120F, DIRECT SUNLIGHT, &
  OTHER IGNITION SOURCES
Hazardous Decomposition Products: CO, CO2
Hazardous Polymerization Indicator: NO
=======================================================
Toxicological Information 
=======================================================
=======================================================
Ecological Information 
=======================================================
=======================================================
MSDS Transport Information 
=======================================================
=======================================================
Regulatory Information 
=======================================================
=======================================================
Other Information 
=======================================================
=======================================================
HAZCOM Label 
=======================================================
Product ID: 2X987B  BELT DRESSING
Cage: 09800
Company Name: SHERWIN-WILLIAMS DIVERSIFIED BRANDS, INC.
Street: 26300 FARGO AVENUE
City: BEDFORD HEIGHTS OH
Zipcode: 44146 US
Health Emergency Phone: 216-292-7400
Date Of Label Review: 11/16/1993
Label Date: 11/16/1993
Chronic Hazard IND: Y
Eye Protection IND: YES
Skin Protection IND: YES
Signal Word: DANGER
Respiratory Protection IND: YES
Health Hazard: Severe
Contact Hazard: Slight
Fire Hazard: Severe
Reactivity Hazard: Slight
Hazard And Precautions: EYES, SKIN & RESPIRATORY SYSTEM: IRRITATION. MAY
  CAUSE NERVOUS SYSTEM DEPRESSION & CAN BE FATAL. OVEREXPOSURE TO SOLVENTS
  MAY CAUSE PERMANENT BRAIN & NERVOUS SYSTEM DAMAGE & ADVERSE EFFECTS TO
  LIVER/U RINARY & CARDIOVASCULAR SYSTEMS. TARGETORGANS: SKIN, EYES,
  RESPIRATORY & DIGESTIVE TRACTS, BRAIN, LIVER, URINARY & CARDIOVASCULAR
  SYSTEMS.		      EYES: SLIGHT IRRITATION. SKIN: MILD IRRITA
  TION, BURNING. INGESTION: IRRITATION OF THE GASTROINTESTINAL TRACT,
  ULCERATION/BURNS IN THE MOUTH & THROAT.
=======================================================
Disclaimer (provided with this information by the compiling agencies):
  This information is formulated for use by elements of the Department of
  Defense. The United States of America in no manner whatsoever expressly
  or implied warrants, states, or intends said information to have any
  application, use or viability by or to any person or persons outside the
  Department of Defense nor any person or persons contracting with any
  instrumentality of the United States of America and disclaims all
  liability for such use. Any person utilizing this instruction who is not
  a military or civilian employee of the United States of America should
  seek competent professional advice to verify and assume responsibility
  for the suitability of this information to their particular situation
  regardless of similarity to a corresponding Department of Defense or
  other government situation.