SPRAYON PRODUCTS -- 40-640 DRY MOLY LUBE -- 9150-00F023916
=======================================================
MSDS Safety Information 
=======================================================
FSC: 9150
MSDS Date: 05/01/1991
MSDS Num: BNJTC
LIIN: 00F023916
Tech Review: 06/30/1992
Product ID: 40-640 DRY MOLY LUBE
Responsible Party
Cage: 09791
Name: SPRAYON PRODUCTS
Address: 26300 FARGO AVE
City: BEDFORD HEIGHTS OH 44146 US
Info Phone Number: (216)292-7400
Emergency Phone Number: (216)292-7400
=======================================================
Preparer Co. when other than Responsible Party Co. 
=======================================================
Cage: 09791
Assigned Ind: N
Name: SPRAYON PRODUCTS
Address: 26300 FARGO AVE
City: BEDFORD HEIGHTS OH 44146
=======================================================
Contractor Summary 
=======================================================
Cage: 09791
Name: SPRAYON PRODUCTS
Address: 26300 FARGO AVE
City: BEDFORD HEIGHTS OH 44146 US
Phone: (216)292-7400
=======================================================
Ingredients 
=======================================================
Cas: 1330-20-7
RTECS #: ZE2100000
Name: XYLENE, DIMETHYLBENZENE, XYLOL
% by Wt: <5%
Other REC Limits: 100 PPM
OSHA PEL: 100 PPM
ACGIH TLV: 100 PPM, SKIN
EPA Rpt Qty: 1000 LBS
DOT Rpt Qty: 1000 LBS
Ozone Depleting Chemical: N
------------------------------
Cas: 67-63-0
RTECS #: NT8050000
Name: ISOPROPANOL (ISOPROPYL ALCOHOL), 2-PROPANOL, DIMETHYL CARBINOL
% by Wt: 20%
Other REC Limits: 400 PPM
OSHA PEL: 400 PPM
ACGIH TLV: 400 PPM
Ozone Depleting Chemical: N
------------------------------
Cas: 75-09-2
RTECS #: PA8050000
Name: DICHLOROMETHANE (METHYLENE CHLORIDE) (SUSPECTED HUMAN CARCINOGEN BY
  ACGIH, NTP)
% by Wt: 55%
OSHA PEL: 500 PPM
ACGIH TLV: 174 MG/CUM (A2)
EPA Rpt Qty: 1000 LBS
DOT Rpt Qty: 1000 LBS
Ozone Depleting Chemical: N
------------------------------
Cas: 75-28-5
RTECS #: TZ4300000
Name: ISOBUTANE, 2-METHYLPROPANE
% by Wt: 10%
Other REC Limits: 1000 PPM
OSHA PEL: 1800 MG/CUM
ACGIH TLV: 1000 PPM
Ozone Depleting Chemical: N
------------------------------
Cas: 74-98-6
RTECS #: TX2275000
Name: PROPANE
% by Wt: 10%
Other REC Limits: 1800 MG/CUM
OSHA PEL: 1000 PPM
ACGIH TLV: SIMPLE ASPHYXIANT
Ozone Depleting Chemical: N
=======================================================
Health Hazards Data 
=======================================================
Route Of Entry Inds - Inhalation: YES
Skin: YES
Ingestion: YES
Carcinogenicity Inds - NTP: YES
IARC: NO
OSHA: NO
Effects of Exposure: SKIN: IRRITATION. INHALATION: UPPER RESPIRATORY TRACT
  IRRITATION, LIGHT- HEADENESS, STAGGERING GAIT, GIDDINESS & NAUSEA, BRAIN
  & NERVOUS SYSTEM DAMAGE. INGESTION: HARMFUL OR FATAL, LIVER & KIDNEY
  DAMA GE.
Explanation Of Carcinogenicity: METHYLENE CHLORIDE IS A SUSPECTED HUMAN
  CARCINOGEN BY ACGIH
Signs And Symptions Of Overexposure: SKIN: IRRITATION. INHALATION: UPPER
  RESPIRATORY TRACT IRRITATION, LIGHT-HEADENESS, STAGGERING GAIT,
  GIDDINESS, NAUSEA, BRAIN & NERVOUS SYSTEM DAMAGE. INGESTION: HARFUL OR
  FATAL, KIDNEY & LIVER DAMAGE.
Medical Cond Aggravated By Exposure: CARDIOVASCULAR
First Aid: INHALATION: REMOVE TO FRESH AIR. EYES: FLUSH W/PLENTY OF WATER.
  SKIN: WASH W/SOAP & WATER. INGESTION: DON'T INDUCE VOMITING. OBTAIN
  MEDICAL ATTENTION IN ALL CASES.
=======================================================
Handling and Disposal
=======================================================
Spill Release Procedures: REMOVE ALL SOURCES OF IGNITION. VENTILATE, &
  REMOVE W/INERT ABSORBENT.
Waste Disposal Methods: DISPOSE OF IN ACCORDANCE W/FEDERAL, STATE & LOCAL
  REGULATIONS.
Handling And Storage Precautions: KEEP AT ROOM TEMPERATURE. TEMPS>120F
Other Precautions: AVOID BREATHING VAPORS OR SPRAY MIST. KEEP OUT OF THE
  REACH OF CHILDREN. DON'T PUNCTURE OR INCINERATE. DON'T SPRAY NEAR FIRE
  OR OP
=======================================================
Fire and Explosion Hazard Information 
=======================================================
Flash Point Method: TOC
Flash Point Text: <20F
Extinguishing Media: CO2, DRY CHEMICAL OR FOAM
Fire Fighting Procedures: WATER MAY BE USED TO KEEP FIRE EXPOSED
  CONTAINERS COOL
Unusual Fire/Explosion Hazard: EXPOSURE TO DIRECT SUNLIGHT OR OTHER HEAT
  MAY CAUSE BURSTING
=======================================================
Control Measures 
=======================================================
Respiratory Protection: WEAR A NIOSH/MSHA APPROVED RESPIRATOR
Ventilation: PROVIDE LOCAL EXHAUST TO KEEP <TLV
Protective Gloves: RECOMMENDED
Eye Protection: SAFETY GLASSES
=======================================================
Physical/Chemical Properties 
=======================================================
B.P. Text: <0
Vapor Density: >AIR
Evaporation Rate & Reference: FASTER THAN ETHER
Appearance and Odor: LUBRICANTS
=======================================================
Reactivity Data 
=======================================================
Stability Indicator: YES
Stability Condition To Avoid: TEMPS>120F. OPEN FLAME, FIRE, DIRECT
  SUNLIGHT
Hazardous Decomposition Products: CO, CO2, HYDROGEN CHLORIDE, & PHOSGENE
  GAS
Hazardous Polymerization Indicator: NO
=======================================================
Toxicological Information 
=======================================================
=======================================================
Ecological Information 
=======================================================
=======================================================
MSDS Transport Information 
=======================================================
=======================================================
Regulatory Information 
=======================================================
=======================================================
Other Information 
=======================================================
=======================================================
HAZCOM Label 
=======================================================
Product ID: 40-640 DRY MOLY LUBE
Cage: 09791
Company Name: SPRAYON PRODUCTS
Street: 26300 FARGO AVE
City: BEDFORD HEIGHTS OH
Zipcode: 44146 US
Health Emergency Phone: (216)292-7400
Date Of Label Review: 06/30/1992
Label Date: 06/30/1992
Chronic Hazard IND: Y
Eye Protection IND: YES
Signal Word: WARNING
Respiratory Protection IND: YES
Health Hazard: Moderate
Contact Hazard: Moderate
Fire Hazard: Slight
Reactivity Hazard: Slight
Hazard And Precautions: SKIN: IRRITATION. INHALATION: UPPER RESPIRATORY
  TRACT IRRITATION, LIGHT HEADENESS, STAGGERING GAIT, GIDDINESS & NAUSEA,
  BRAIN & NERVOUS SYSTEM DAMAGE. INGESTION: HARMFUL OR FATAL, LIVER &
  KIDNEY DAMAG E. METHYLENE CHLORIDE IS A SUSPECTED HUMAN CARCINOGEN.
=======================================================
Disclaimer (provided with this information by the compiling agencies):
  This information is formulated for use by elements of the Department of
  Defense. The United States of America in no manner whatsoever expressly
  or implied warrants, states, or intends said information to have any
  application, use or viability by or to any person or persons outside the
  Department of Defense nor any person or persons contracting with any
  instrumentality of the United States of America and disclaims all
  liability for such use. Any person utilizing this instruction who is not
  a military or civilian employee of the United States of America should
  seek competent professional advice to verify and assume responsibility
  for the suitability of this information to their particular situation
  regardless of similarity to a corresponding Department of Defense or
  other government situation.