SPRAYON PRODUCTS -- 00708 TFE DRY LUBE, LUBRICANTS, RUST (SUP DAT) -- 9150-00N078241
=======================================================
MSDS Safety Information 
=======================================================
FSC: 9150
MSDS Date: 05/17/1993
MSDS Num: CFLTJ
LIIN: 00N078241
Tech Review: 10/22/1997
Product ID: 00708 TFE DRY LUBE, LUBRICANTS, RUST (SUP DAT)
Responsible Party
Cage: 09800
Name: SPRAYON PRODUCTS
Address: 6830 COCHRAN RD
City: SOLON OH 44139 US
Info Phone Number: 800-777-2966
Emergency Phone Number: 216-292-7400
Review Ind: N
=======================================================
Contractor Summary 
=======================================================
Cage: 09800
Name: SHERWIN-WILLIAMS DIVERSIFIED BRANDS, INC.
Address: 26300 FARGO AVENUE
City: BEDFORD HEIGHTS OH 44146 US
Phone: 216-292-7400 OR 216-595-8634
=======================================================
Ingredients 
=======================================================
Cas: 74-98-6
RTECS #: TX2275000
Name: PROPANE. VP: 760.0
% by Wt: 14
OSHA PEL: 1000 PPM
ACGIH TLV: ASPHYXIANT
Ozone Depleting Chemical: N
------------------------------
Cas: 75-28-5
RTECS #: TZ4300000
Name: PROPANE, 2-METHYL-; (2-METHYLPROPANE (PROPELLANT)) VP: 760.0
% by Wt: 14
OSHA PEL: N/K (FP N)
ACGIH TLV: N/K (FP N)
Ozone Depleting Chemical: N
------------------------------
Cas: 142-82-5
RTECS #: MI7700000
Name: N-HEPTANE; (HEPTANE) VP: 40
% by Wt: 60
OSHA PEL: 500 PPM
ACGIH TLV: 400 PPM/500 STEL
Ozone Depleting Chemical: N
------------------------------
Cas: 67-63-0
RTECS #: NT8050000
Name: ISOPROPYL ALCOHOL; (2-PROPANOL) (SARA 313) VP: 33
% by Wt: 11
OSHA PEL: 400 PPM
ACGIH TLV: 400 PPM/500 STEL
Ozone Depleting Chemical: N
------------------------------
Name: VOC AS PERCENT BY WEIGHT EXCLUDING FEDERALLY EXEMPT SOLVENTS: 88
OSHA PEL: N/K (FP N)
ACGIH TLV: N/K (FP N)
=======================================================
Health Hazards Data 
=======================================================
LD50 LC50 Mixture: NONE SPECIFIED BY MANUFACTURER.
Route Of Entry Inds - Inhalation: YES
Skin: YES
Ingestion: NO
Carcinogenicity Inds - NTP: NO
IARC: NO
OSHA: NO
Effects of Exposure: ACUTE: IRRIT OF EYES, SKIN & RESP SYS. MAY CAUSE NERV
  SYS DEPRESS. EXTREME OVEREXP MAY RSLT IN UNCON & POSS DEATH. SIGNS &
  SYMPS OF OVEREXP: EXCESS EXPOS TO VAPS/SPRAY MISTS MAY CAUSE HDCH, DIZZ,
  NAUS	& LOSS OF COORD. EXCESS SKIN & EYE EXPOS MAY CAUSE REDNESS &
  ITCH/BURNING SENSATION. CHRONIC: PRLNG (EFTS OF OVEREXP)
Explanation Of Carcinogenicity: NOT RELEVANT.
Signs And Symptions Of Overexposure: HLTH HAZ: OVEREXP TO SOLV INGS MAY
  CAUSE ADVERSE EFTS TO LIVER, URINARY, BLOOD-FORMING, CARDIOVASCULAR &
  REPRO SYS. RPTS HAVE ASSOC RPTD & PRLNG OVEREXP TO SOLVS W/PERM BRAIN &
  NERV SYS DMG.
Medical Cond Aggravated By Exposure: NONE GENERALLY RECOGNIZED.
First Aid: INHAL: REMOVE FROM EXPOSURE. RESTORE BREATHING. KEEP WARM &
  QUIET. SKIN: WASH AFFECTED AREA THOROUGHLY W/SOAP & WATER. REMOVE
  CONTAMINATED CLOTHING & LAUNDER BEFORE REUSE. EYES: FLUSH W/LARGE
  AMOUNTS  OF WATER FOR AT LEAST 15 MINUTES. GET MEDICAL ATTENTION.
  INGEST: NEVER GIVE ANYTHING BY MOUTH TO AN UNCONSCIOUS PERSON. DO NOT
  INDUCE VOMITING. GIVE SEVERAL GLASSES OF WATER. SEEK MEDICAL ATTENTION.
=======================================================
Handling and Disposal
=======================================================
Spill Release Procedures: REMOVE ALL SOURCES OF IGNITION. VENTILATE AND
  REMOVE WITH INERT ABSORBENT.
Neutralizing Agent: NONE SPECIFIED BY MANUFACTURER.
Waste Disposal Methods: WASTE FROM THESE PRODUCTS MAY BE HAZARDOUS AS
  DEFINED UNDER RCRA 40 CFR 261. DO NOT INCINERATE. DEPRESSURIZE
  CONTAINER. DISPOSE OF IN ACCORDANCE WITH FEDERAL, STATE & LOCAL
  REGULATIONS REGARDING POLLU TION.
Handling And Storage Precautions: CONTENTS UNDER PRESSURE. DO NOT
  PUNCTURE, INCINERATE OR EXPOSURE TO TEMPERATURE ABOVE 120F. DO NOT TAKE
  INTERNALLY. KEEP OUT OF REACH OF CHILDREN.
Other Precautions: HEAT FROM SUNLIGHT, RADIATORS, STOVES, HOT WATER, &
  OTHER HEAT SOURCES COULD CAUSE CONTR TO BURST. INTENTIONAL MISUSE BY
  DELIBERATELY CONC & INHALING CONTENTS CAN BE HARMFUL/FATAL. USE ONLY
  W/ADEQ VEN T. AVOID BRTHG VAP & SPRAY MIST.
=======================================================
Fire and Explosion Hazard Information 
=======================================================
Flash Point Method: PMCC
Flash Point Text: >200F,>93C
Extinguishing Media: CARBON DIOXIDE, DRY CHEMICAL, FOAM.
Fire Fighting Procedures: WEAR NIOSH APPRVD SCBA & FULL PROT EQUIP (FP N).
  WATER SPRAY MAY BE INEFFECTIVE. IF WATER IS USED, FOG NOZ ARE PREF.
  WATER MAY BE USED TO COOL CLSD (SUP DAT)
Unusual Fire/Explosion Hazard: CLOSED CONTAINERS MAY EXPLODE DUE TO THE
  BUILD-UP OF PRESSURE WHEN EXPOSED TO EXTREME HEAT.
=======================================================
Control Measures 
=======================================================
Respiratory Protection: IF PERSONAL EXPOSURE CANNOT BE CONTROLLED BELOW
  APPLICABLE LIMITS BY VENTILATION, WEAR A PROPERLY FITTED ORGANIC
  VAPOR/PARTICULATE RESPIRATOR APPROVED BY NIOSH FOR PROTECTION.
Ventilation: LOC EXHST PREF. GEN EXHST ACCEPTABLE IF EXPOS IS MAINTAINED
  < APPLIC EXPOS LIM. REFER TO OSHA STDS 1910.91, (SUP DAT)
Protective Gloves: IMPERVIOUS GLOVES (FP N).
Eye Protection: ANSI APPRVD CHEM WORKERS GOGGLES (FP N).
Other Protective Equipment: EMERGENCY EYEWASH AND DELUGE SHOWER MEETING
  ANSI DESIGN CRITERIA (FP N).
Work Hygienic Practices: WASH HANDS AFTER USING. AVOID CONTACT WITH SKIN
  AND EYES.
Supplemental Safety and Health: TRADE NAME/PART #: PREVENTATIVES &
  MAINTENANCE PRODUCTS-1. FIRE FIGHT PROC: CONTRS TO PVNT PRESS BUILD-UP &
  POSS AUTOIGNIT/EXPLO WHEN EXPOSED TO EXTREME HEAT. VENT: 1910.107,
  1910.108.
=======================================================
Physical/Chemical Properties 
=======================================================
B.P. Text: >176F,>80C
Vapor Pres: SEE INGS
Vapor Density: HVR/AIR
Evaporation Rate & Reference: FASTER THAN ETHER
Appearance and Odor: NONE SPECIFIED BY MANUFACTURER
Percent Volatiles by Volume: >25
=======================================================
Reactivity Data 
=======================================================
Stability Indicator: YES
Stability Condition To Avoid: NONE SPECIFIED BY MANUFACTURER.
Materials To Avoid: NONE KNOWN.
Hazardous Decomposition Products: BY FIRE: CARBON DIOXIDE, CARBON
  MONOXIDE, OXIDES OF METALS LISTED IN INGREDIENT SECTION.
Hazardous Polymerization Indicator: NO
Conditions To Avoid Polymerization: NOT RELEVANT.
=======================================================
Toxicological Information 
=======================================================
=======================================================
Ecological Information 
=======================================================
=======================================================
MSDS Transport Information 
=======================================================
=======================================================
Regulatory Information 
=======================================================
=======================================================
Other Information 
=======================================================
=======================================================
HAZCOM Label 
=======================================================
Product ID: 00708 TFE DRY LUBE, LUBRICANTS, RUST (SUP DAT)
Cage: 09800
Company Name: SHERWIN-WILLIAMS DIVERSIFIED BRANDS, INC.
Street: 26300 FARGO AVENUE
City: BEDFORD HEIGHTS OH
Zipcode: 44146 US
Health Emergency Phone: 216-292-7400
Date Of Label Review: 10/23/1997
Label Date: 10/23/1997
Chronic Hazard IND: Y
Eye Protection IND: YES
Skin Protection IND: YES
Signal Word: WARNING
Respiratory Protection IND: YES
Health Hazard: Moderate
Contact Hazard: Moderate
Fire Hazard: Slight
Reactivity Hazard: None
Hazard And Precautions: ACUTE: IRRITATION OF EYES, SKIN AND RESPIRATORY
  SYSTEM. MAY CAUSE NERVOUS SYSTEM DEPRESSION. EXTREME OVEREXPOSURE MAY
  RESULT IN UNCONSCIOUSNESS AND POSSIBLE DEATH. SIGNS AND SYMPTOMS OF
  OVEREXPOSURE:  EXCESSIVE EXPOSURE TO VAPORS OR SPRAY MISTS MAY CAUSE
  HEADACHE, DIZZINESS, NAUSEA AND LOSS OF COORDINATION. EXCESSIVE SKIN AND
  EYE EXPOSURE MAY CAUSE REDNESS AND ITCHING OR BURNING SENSATION.
  CHRONIC:  PROLONGED OVEREXPOSURE TO SOLVENTS MAY CAUSE ADVERSE EFFECTS
  TO LIVER, URINARY, BLOOD-FORMING, CARDIOVASCULAR AND REPRODUCTIVE
  SYSTEMS AND HAS BEEN REPORTED TO CAUSE PERMANENT BRAIN AND NERVOUS SYSTE
  M DAMAGE.
=======================================================
Disclaimer (provided with this information by the compiling agencies):
  This information is formulated for use by elements of the Department of
  Defense. The United States of America in no manner whatsoever expressly
  or implied warrants, states, or intends said information to have any
  application, use or viability by or to any person or persons outside the
  Department of Defense nor any person or persons contracting with any
  instrumentality of the United States of America and disclaims all
  liability for such use. Any person utilizing this instruction who is not
  a military or civilian employee of the United States of America should
  seek competent professional advice to verify and assume responsibility
  for the suitability of this information to their particular situation
  regardless of similarity to a corresponding Department of Defense or
  other government situation.