LPS LABORATORIES,INC. -- LPS 1 GREASELESS LUBRICANT (SUPPLEMENTAL) -- 9150-01-142-9773
=======================================================
MSDS Safety Information 
=======================================================
FSC: 9150
NIIN: 01-142-9773
MSDS Date: 05/01/1993
MSDS Num: BGWKB
Tech Review: 07/31/1998
Product ID: LPS 1 GREASELESS LUBRICANT (SUPPLEMENTAL)
Responsible Party
Cage: 66724
Name: LPS LABORATORIES,INC.
Address: 4647 HUGH HOWELL ROAD
City: TUCKER GA 30084-5096 US
Info Phone Number: 404-934-7800
Emergency Phone Number: 404-934-7800/800-424-9300(CHEMTREC)
Preparer's Name: JOHN ROUDEBUSH
=======================================================
Preparer Co. when other than Responsible Party Co. 
=======================================================
Cage: 66724
Assigned Ind: N
Name: LPS LABORATORIES,  INC.
Address: 4647 HUGH HOWELL ROAD
City: TUCKER GA 30085-5052
=======================================================
Contractor Summary 
=======================================================
Cage: 2X264
Name: ALL-SAFE INC
Address: 4767 LANGTON RD
Box: 116
City: HIILIARD OH 43026 US
Phone: 614-876-4041
Cage: 32861
Name: HOLT LLOYD CORP
Address: 4647 HUGH HOWELL RD
City: TUCKER GA 30084-5004 US
Phone: 404-934-7800
Cage: 66724
Name: LPS LABORATORIES,  INC.
Address: 4647 HUGH HOWELL ROAD
City: TUCKER GA 30085-5052 US
Phone: 404-934-7800
=======================================================
Item Description Information 
=======================================================
Item Manager: S9G
Item Name: LUBRICANT
Unit of Issue: CN
Quantitative Expression: 00000000005GL
UI Container Qty: 0
Type of Container: CAN
=======================================================
Ingredients 
=======================================================
Cas: 64742-96-7
Name: ALIPHATIC HYDROCARBON
% by Wt: 70-80
Other REC Limits: NONE RECOMMENDED
OSHA PEL: NOT ESTABLISHED
ACGIH TLV: NOT ESTABLISHED
Ozone Depleting Chemical: N
------------------------------
Cas: 64742-30-9
Name: ALIPHAATIC PETROLEUM NAPTHA
% by Wt: 20-30
Other REC Limits: NONE RECOMMENDED
OSHA PEL: 5 MG/M3 OIL MIST
ACGIH TLV: 5 MG/M3 OIL MIST
Ozone Depleting Chemical: N
------------------------------
Name: NON-HAZARDOUS PROPRIETARY BLEND
% by Wt: 3-5
Other REC Limits: NONE RECOMMENDED
OSHA PEL: NOT ESTABLISHED
ACGIH TLV: NOT ESTABLISHED
-----------------------------
Cas: 124-38-9
RTECS #: FF6400000
Name: CARBON DIOXIDE (AEROSOL ONLY)
% by Wt: 2-3
Other REC Limits: NONE RECOMMENDED
OSHA PEL: 5000 PPM
ACGIH TLV: 5000PPM/30000STEL;94
Ozone Depleting Chemical: N
=======================================================
Health Hazards Data 
=======================================================
LD50 LC50 Mixture: NONE SPECIFIED BY MANUFACTURER.
Route Of Entry Inds - Inhalation: YES
Skin: NO
Ingestion: NO
Carcinogenicity Inds - NTP: NO
IARC: NO
OSHA: NO
Effects of Exposure: INHAL:HEADACHE,DIZZINESS,NAUSEA,ANESTHETIC
  EFFECTS.EYE:IRRIT.SKIN:REP/PROL CONTACT MAY CAUSE DRYING OF
  SKIN.INGEST:NOT LIKELY ROUTE OF EXPO.LOW ORDER OR ORAL TOXICITY;HOWEVER
  MINUTE AMT ASPIRATED INTO  LUNGS DURING INGESTION MAY CAUSE SEVERE PULM
  INJURY.
Explanation Of Carcinogenicity: PER MSDS:CHEMS LISTED AS POTENTIAL
  CARC:NTP/IARC/
OSHA:NO.
Signs And Symptions Of Overexposure: HEADACHE,DIZZINESS,NAUSEA,ANESTHETIC
  EFFECTS,EYE IRRIT,DRYING OF SKIN,SEVERE PULMONARY INJURY IF MINUTE AMT
  ASPIRATED INTO LUNGS.
Medical Cond Aggravated By Exposure: NONE FROM NORMAL EXPOSURE.
First Aid: INHAL:MOVE TO FRESH AIR.CONTACT PHYSICIAN.EYE:FLUSH W/PLENTY OF
  WTER AND CONTACT PHYSICIAN.SKIN:WASH W/SOAP/WATER;APPLY MEDICATED SKIN
  CREAM.INGEST:CONTAINS ALIPHATIC HYDROCARBONS & PETROLEUM OIL.DONT 
  INDUCE VOMITING.CONTACT PHYSICIAN IMMED.
=======================================================
Handling and Disposal
=======================================================
Spill Release Procedures: VENTI AREA BY OPN DOORS/WINDOWS.REMOVE IGN
  SOURCS.REMOVE LEAKING CNTNR,TRANSFER REMIANING PROD TO ANOTHER
  VESSEL.PREVENT PRODUCT FRM GOING INTO SEWERS/WATER SOURCES BY
  DIKING/IMPOUNDING.USEING APPROP  SAF EQPMT MOPUP/SOAKUP W/ABSORBENT
  MATL(SAND,CLAY)
Neutralizing Agent: NONE SPECIFIED BY MANUFACTURER.
Waste Disposal Methods: DISPOSE OF IAW LOCAL, STATE AND FEDERAL
  REGULATIONS FOR PETROLEUM DISTILLATES.RCRA HAZ WASTE@:NA.CERCLA
  RQ:NONE.SARA TITLE III CHEMS:NONE.
Handling And Storage Precautions: STORE AEROSOLS BELOW 120F & ABOVE
  32F.STORE BULK BELOW 150F & ABOVE 32F.STORE AWAY FROM IGNITION SOURCES &
  AVOID BREATHING VAPORS.
Other Precautions: NONE SPECIFIED BY MANUFACTURER.
=======================================================
Fire and Explosion Hazard Information 
=======================================================
Flash Point Method: SCC
Flash Point Text: 175F,79C
Autoignition Temp Text: NP
Lower Limits: 1
Upper Limits: 6
Extinguishing Media: FOAM, DRY CHEMICAL, CARBON DIOXIDE.
Fire Fighting Procedures: DONT USE WATER.TREAT AS COMBUSTIBLE PETROLEUM
  DISTILLATES.
Unusual Fire/Explosion Hazard: INTENSIVE HEAT CREATED BY FIRE WILL CAUSE
  AEROSOLS TO BURST.
=======================================================
Control Measures 
=======================================================
Respiratory Protection: NONE REQUIRED IF GOOD VENTILATION IS
  MAINTAINED.FOR ENCLOSED AREAS USE NIOSH APPROV ORG VAPOR CARTRIDGE
  RESPIRATOR OR SELF-CONTAINED BREATHING APPARATUS.
Ventilation: LOC EXHAU IS USUALLY ADEQUATE.HOWEVER MECHANICAL VENTI SHOULD
  BE USED WHEN SPRAYING IN ENCLSD AREAS.VAP CONC SHOULD(SUP)
Protective Gloves: SOLVENT RESIST GLOVES
Eye Protection: FACE SHIELD OR GOGGLES
Other Protective Equipment: NONE
Work Hygienic Practices: WASH HANDS W/SOAP/WATER AFT USE &/OR BEF
  BREAKS/LUNC/@END OF WORK PERIODS.REMOVE CONTAM CLOTH,LAUNDER BEFORE
  REUSE.
Supplemental Safety and Health:
  PN3:00017,00116,01128,00105,00155,00122,LPS 1 TRIGGER SPRAY.
  VENTILATION:BE MINIMIZED AS MUCH AS POSSIBLE.
=======================================================
Physical/Chemical Properties 
=======================================================
HCC: V6
B.P. Text: 350F,177C
M.P/F.P Text: NP
Decomp Text: NP
Vapor Pres: 2 @100F
Vapor Density: 4.7
Spec Gravity: 0.80
PH: NP
Viscosity: NP
Evaporation Rate & Reference: 0.07, BUTYL ACETATE=1
Solubility in Water: NIL
Appearance and Odor: CLEAR, THIN LIQUID WITH SWEET ODOR
Percent Volatiles by Volume: 95
Corrosion Rate: NP
=======================================================
Reactivity Data 
=======================================================
Stability Indicator: YES
Stability Condition To Avoid: AVOID SPARKS OR OPEN FLAMES.SEE
  HANDLING/STORAGE PRECAUTIONS.
Materials To Avoid: STRONG OXIDIZING AGENTS
Hazardous Decomposition Products: THERMAL DECOMPOSITION MAY YIELD CARBON
  MONOXIDE.
Hazardous Polymerization Indicator: NO
=======================================================
Toxicological Information 
=======================================================
=======================================================
Ecological Information 
=======================================================
=======================================================
MSDS Transport Information 
=======================================================
=======================================================
Regulatory Information 
=======================================================
=======================================================
Other Information 
=======================================================
=======================================================
Transportation Information 
=======================================================
Responsible Party Cage: 66724
Trans ID NO: 110569
Product ID: LPS 1 GREASELESS LUBRICANT (SUPPLEMENTAL)
MSDS Prepared Date: 05/01/1993
Review Date: 07/31/1998
Article W/O MSDS: N
Net Unit Weight: 33.4 LBS
Multiple KIT Number: 0
Unit Of Issue: CN
Container QTY: 0
Type Of Container: CAN
Additional Data: PER MSDS:COMPOUND,BOILER,PRESERVING LIQUID.
=======================================================
Detail DOT Information 
=======================================================
DOT Proper Shipping Name: NOT REGULATED BY THIS MODE OF TRANSPORTATION
=======================================================
Detail IMO Information 
=======================================================
IMO Proper Shipping Name: NOT REGULATED FOR THIS MODE OF TRANSPORTATION
=======================================================
Detail IATA Information 
=======================================================
IATA Proper Shipping Name: NOT REGULATED BY THIS MODE OF TRANSPORTATION
=======================================================
Detail AFI Information 
=======================================================
AFI Proper Shipping Name: NOT REGULATED BY THIS MODE OF TRANSPORTATION
=======================================================
HAZCOM Label 
=======================================================
Product ID: LPS 1 GREASELESS LUBRICANT (SUPPLEMENTAL)
Cage: 66724
Company Name: LPS LABORATORIES,  INC.
Street: 4647 HUGH HOWELL ROAD
City: TUCKER GA
Zipcode: 30085-5052 US
Health Emergency Phone: 404-934-7800/800-424-9300(CHEMTREC)
Date Of Label Review: 07/31/1998
Label Date: 07/31/1998
Year Procured: 1995
Chronic Hazard IND: Y
Eye Protection IND: YES
Skin Protection IND: YES
Signal Word: CAUTION
Respiratory Protection IND: YES
Health Hazard: Slight
Contact Hazard: Slight
Fire Hazard: None
Reactivity Hazard: None
Hazard And Precautions: INHAL:HEAD,DIZZ,NAU,ANESTHETIC
  EFFECTS.EYE:IRRIT.SKIN:REP/PROL CONTACT MAY CAUSE DRYING OF
  SKIN.INGEST:NOT LIKELY ROUTE OF EXPO.LOW ORDER OR ORAL TOXICITY;HOWEVER
  MINUTE AMT ASPIRATED INTO LUNGS DURIN G INGESTION MAY CAUSE SEVERE PULM
  INJURY. STORE AEROSOLS BELOW 120F & ABOVE 32F.STORE BULK BELOW 150F &
  ABOVE 32F.STORE AWAY FROM IGNITION SOURCES & AVOID BREATHING VAPORS.
  FIRST AID: INHAL:MOVE TO FR ESH AIR.CONTACT PHYSICIAN.EYE:FLUSH W/PLENTY
  OF WTER AND CONTACT PHYSICIAN.SKIN:WASH W/SOAP/WATER;APPLY MEDICATED
  SKIN CREAM.INGEST:CONTAINS ALIPHATIC HYDROCARBONS & PETROLEUM OIL.DONT
  INDUCE VOMITING .CONTACT PHYSICIAN IMMED.TARORG:CNS/SKIN/EYE/LUNGS
=======================================================
Disclaimer (provided with this information by the compiling agencies):
  This information is formulated for use by elements of the Department of
  Defense. The United States of America in no manner whatsoever expressly
  or implied warrants, states, or intends said information to have any
  application, use or viability by or to any person or persons outside the
  Department of Defense nor any person or persons contracting with any
  instrumentality of the United States of America and disclaims all
  liability for such use. Any person utilizing this instruction who is not
  a military or civilian employee of the United States of America should
  seek competent professional advice to verify and assume responsibility
  for the suitability of this information to their particular situation
  regardless of similarity to a corresponding Department of Defense or
  other government situation.