LPS LABORATORIES INC -- LSP 2 INDUSTRIAL-STRENGTH LUBRICANT, 00255 -- 8030-00N087397
=======================================================
MSDS Safety Information 
=======================================================
FSC: 8030
MSDS Date: 08/21/1996
MSDS Num: CHGRH
LIIN: 00N087397
Tech Review: 06/25/1998
Product ID: LSP 2 INDUSTRIAL-STRENGTH LUBRICANT, 00255
Responsible Party
Cage: 66724
Name: LPS LABORATORIES INC
Address: 4647 HUGH HOWELL ROAD
City: TUCKER GA 30085-5052 US
Info Phone Number: 770-934-7800
Emergency Phone Number: 703-527-3887;800-424-9300(CHEMTREC)
Review Ind: N
=======================================================
Contractor Summary 
=======================================================
Cage: 66724
Name: LPS LABORATORIES,  INC.
Address: 4647 HUGH HOWELL ROAD
City: TUCKER GA 30085-5052 US
Phone: 404-934-7800
=======================================================
Ingredients 
=======================================================
Cas: 64742-47-8
RTECS #: OA5504000
Name: PETROLEUM HYDROCARBON; (ALIPHATIC HYDROCARBON)
% by Wt: 50-70
OSHA PEL: N/K (FP N)
ACGIH TLV: N/K (FP N)
Ozone Depleting Chemical: N
------------------------------
Cas: 64742-53-6
RTECS #: PY8036000
Name: MINERAL OIL, PETROLEUM DISTILLATES, HYDROTREATED (SEVERE) LIGHT
  NAPHTHENIC; (PETROLEUM OIL (SEVERELY HYDRO-TREATED)
% by Wt: 5-10
OSHA PEL: 5 MG/M3 (OIL MIST)
ACGIH TLV: 5 MG/M3 (OIL MIST)
Ozone Depleting Chemical: N
------------------------------
Cas: 124-38-9
RTECS #: FF6400000
Name: CARBON DIOXIDE; (CARBON DIOXIDE PROPELLANT (AEROSOL ONLY))
% by Wt: 2-3
OSHA PEL: 5000 PPM
ACGIH TLV: 5000PPM/30000STEL;95
Ozone Depleting Chemical: N
=======================================================
Health Hazards Data 
=======================================================
LD50 LC50 Mixture: NONE SPECIFIED BY MANUFACTURER.
Route Of Entry Inds - Inhalation: YES
Skin: NO
Ingestion: NO
Carcinogenicity Inds - NTP: NO
IARC: NO
OSHA: NO
Effects of Exposure: INHALATION: HEADACHE, DIZZINESS, NAUSEA AND
  ANESTHETIC EFFECTS. EYES: IRRITATION. SKIN: REPEATED OR PROLONGED
  CONTACT MAY CAUSE DRYING OF SKIN. INGESTION: NOT A LIKELY ROUTE OF
  EXPOSURE. LOW ORDER OF  ORAL TOXICITY; HOWEVER MINUTE AMOUNT ASPIRATED
  INTO LUNGS DURING INGESTION MAY CAUSE SEVERE PULMONARY INJURY.
Explanation Of Carcinogenicity: NOT RELEVANT.
Signs And Symptions Of Overexposure: SEE HEALTH HAZARDS.
Medical Cond Aggravated By Exposure: NONE FROM NORMAL EXPOSURE.
First Aid: INHALATION: MOVE TO FRESH AIR. CONTACT PHYSICIAN. EYES: FLUSH
  WITH PLENTY OF WATER FOR AT LEAST 15 MINUTES AND CONTACT PHYSICIAN.
  SKIN: WASH WITH SOAP AND WATER; APPLY MEDICATED SKIN CREAM. INGESTION: 
  CONTAINS ALIPHATIC HYDROCARBONS AND PERTOLEUM OIL. DO NOT INDUCE
  VOMITING. CONTACT PHYSICIAN IMMEDIATELY.
=======================================================
Handling and Disposal
=======================================================
Spill Release Procedures: VENT AREA BY OPENING DOORS & WINDOWS. REMOVE
  INGEST SOURCES. REMOVE LEAKING CNTNR & TRANSFER REMAINING PROD TO
  ANOTHER VESSEL. PVNT PROD FROM GOING INTO SEWERS & WATER SOURCES BY
  DIKING/IMPOUNDING. US E APPROP SAFETY EQUIP APPRVD BY NIOSH, (SUPDAT)
Neutralizing Agent: NONE SPECIFIED BY MANUFACTURER.
Waste Disposal Methods: DISPOSE OF IN ACCORDANCE WITH LOCAL, STATE AND
  FEDERAL REGULATIONS FOR PETROLEUM DISTILLATES.
Handling And Storage Precautions: STORE AEROSOLS BELOW 120F AND ABOVE 32F.
  STORE AWAY FROM IGNITION SOURCES AND AVOID BREATHING VAPORS.
Other Precautions: NONE SPECIFIED BY MANUFACTURER.
=======================================================
Fire and Explosion Hazard Information 
=======================================================
Flash Point Method: SCC
Flash Point Text: 175F,79C
Lower Limits: 1%
Upper Limits: 6%
Extinguishing Media: FOAM, DRY CHEMICAL, CARBON DIOXIDE.
Fire Fighting Procedures: USE NIOSH APPROVED SCBA & FULL PROTECTIVE
  EQUIPMENT (FP N). DO NOT USE WATER. TREAT AS COMBUSTIBLE PETROLEUM
  DISTILLATES.
Unusual Fire/Explosion Hazard: INTENSIVE HEAT CREATED BY FIRE WILL CAUSE
  AEROSOLS TO BURST.
=======================================================
Control Measures 
=======================================================
Respiratory Protection: NONE REQUIRED IF GOOD VENTILATION IS MAINTAINED.
  FOR ENCLOSED AREAS, USE NIOSH APPROVED ORGANIC VAPOR CATRIDGE RESPIRATOR
  OR NIOSH APPROVED SELF-CONTAINED BREATHING APPARATUS.
Ventilation: LOC EXHST IS USUALLY ADEQ. HOWEVER, MECH VENT SHOULD BE USED
  WHEN SPRAYING IN ENCLOSED AREA. VAP CONC SHOULD (SUPDAT)
Protective Gloves: SOLVENT RESISTANT GLOVES.
Eye Protection: ANSI APPROVED CHEM WORKERS GOGGS (FP N).
Other Protective Equipment: EYE WASH FOUNTAIN & DELUGE SHOWER WHICH MEET
  ANSI DESIGN CRITERIA (FP N). NONE.
Work Hygienic Practices: WASH HANDS W/SOAP & H*2O AFTER USE &/BEFORE
  BREAKS, LUNCH & AT END OF WORK PERIODS. REMOVE CONTAMD CLOTHING &
  (SUPDAT)
Supplemental Safety and Health: SPILL PROC: MOP UP OR SOAK UP WITH
  ABSORBENT MATERIAL, SUCH AS SAND OR CLAY. VENT: BE MINIMIZED AS MUCH AS
  POSSIBLE. HYGIENE PRACT: LAUNDER BEFORE REUSE.
=======================================================
Physical/Chemical Properties 
=======================================================
B.P. Text: 350F,177C
Vapor Pres: <2 @ 100F
Vapor Density: 4.7
Spec Gravity: 0.84 (H*2O = 1)
Evaporation Rate & Reference: 0.07 (N-BUTYL ACETATE =1)
Solubility in Water: NIL
Appearance and Odor: LIGHT AMBER LIQUID WITH SLIGHT ODOR.
Percent Volatiles by Volume: 70
=======================================================
Reactivity Data 
=======================================================
Stability Indicator: YES
Stability Condition To Avoid: AVOID SPARKS OR OPEN FLAMES. SEE HANDLING
  AND STORAGE PRECAUTIONS.
Materials To Avoid: STRONG OXIDIZING AGENTS.
Hazardous Decomposition Products: THERMAL DECOMPOSITION MAY YIELD CARBON
  MONOXIDE.
Hazardous Polymerization Indicator: NO
Conditions To Avoid Polymerization: NOT RELEVANT.
=======================================================
Toxicological Information 
=======================================================
=======================================================
Ecological Information 
=======================================================
=======================================================
MSDS Transport Information 
=======================================================
=======================================================
Regulatory Information 
=======================================================
=======================================================
Other Information 
=======================================================
=======================================================
HAZCOM Label 
=======================================================
Product ID: LSP 2 INDUSTRIAL-STRENGTH LUBRICANT, 00255
Cage: 66724
Company Name: LPS LABORATORIES,  INC.
Street: 4647 HUGH HOWELL ROAD
City: TUCKER GA
Zipcode: 30085-5052 US
Health Emergency Phone: 703-527-3887;800-424-9300(CHEMTREC)
Date Of Label Review: 06/25/1998
Label Date: 06/25/1998
Chronic Hazard IND: N
Eye Protection IND: YES
Skin Protection IND: YES
Signal Word: WARNING
Respiratory Protection IND: YES
Health Hazard: Moderate
Contact Hazard: Slight
Fire Hazard: Moderate
Reactivity Hazard: None
Hazard And Precautions: COMBUSTIBLE. ACUTE: INHALATION: HEADACHE,
  DIZZINESS, NAUSEA AND ANESTHETIC EFFECTS. EYES: IRRITATION. SKIN:
  REPEATED OR PROLONGED CONTACT MAY CAUSE DRYING OF SKIN. INGESTION: NOT A
  LIKELY ROUTE OF EXP OSURE. LOW ORDER OF ORAL TOXICITY; HOWEVER MINUTE
  AMOUNT ASPIRATED INTO LUNGS DURING INGESTION MAY CAUSE SEVERE PULMONARY
  INJURY. CHRONIC: NONE SPECIFIED BY MANUFACTURER.
=======================================================
Disclaimer (provided with this information by the compiling agencies):
  This information is formulated for use by elements of the Department of
  Defense. The United States of America in no manner whatsoever expressly
  or implied warrants, states, or intends said information to have any
  application, use or viability by or to any person or persons outside the
  Department of Defense nor any person or persons contracting with any
  instrumentality of the United States of America and disclaims all
  liability for such use. Any person utilizing this instruction who is not
  a military or civilian employee of the United States of America should
  seek competent professional advice to verify and assume responsibility
  for the suitability of this information to their particular situation
  regardless of similarity to a corresponding Department of Defense or
  other government situation.