LPS LABORATORIES,INC. -- LPS CFC-FREE ELECTRO CONTACT CLEANER -- 6850-01-412-0044
=======================================================
MSDS Safety Information 
=======================================================
FSC: 6850
NIIN: 01-412-0044
MSDS Date: 11/07/1996
MSDS Num: CJMHX
Tech Review: 09/21/1999
Product ID: LPS CFC-FREE ELECTRO CONTACT CLEANER
Responsible Party
Cage: 66724
Name: LPS LABORATORIES,INC.
Address: 4647 HUGH HOWELL ROAD
City: TUCKER GA 30084-5096 US
Info Phone Number: 770-934-7800
Emergency Phone Number: 770-934-7800
Resp. Party Other MSDS No.: P/N 03116,03101,03105,03155
=======================================================
Item Description Information 
=======================================================
Item Manager: S9G
Item Name: CLEANING COMPOUND,SOLVENT
Specification Number: NONE
Type/Grade/Class: NONE
Unit of Issue: CN
Quantitative Expression: 00000000005GL
UI Container Qty: 0
Type of Container: CAN
=======================================================
Ingredients 
=======================================================
Cas: 107-83-5
RTECS #: SA2985000
Name: ISOHEXANE
% low Wt: 70.
% high Wt: 90.
Ozone Depleting Chemical: N
------------------------------
Cas: 67-63-0
RTECS #: NT8050000
Name: ISO-PROPANOL; ISOPROPYL ALCOHOL
% low Wt: 5.
% high Wt: 20.
OSHA PEL: 980 MG/M3;400 PPM
ACGIH TLV: 983 MG/M3;400 PPM
ACGIH STEL: 1230 MG/M3;500 PPM
Ozone Depleting Chemical: N
------------------------------
Cas: 110-54-3
RTECS #: MN9275000
Name: N-HEXANE
% low Wt: 2.
% high Wt: 3.
OSHA PEL: 1800 MG/M3;500 PPM
EPA Rpt Qty: 1 LB
DOT Rpt Qty: 1 LB
Ozone Depleting Chemical: N
=======================================================
Health Hazards Data 
=======================================================
LD50 LC50 Mixture: LD50 (ORAL, RAT) IS UNKNOWN.
Route Of Entry Inds - Inhalation: YES
Skin: YES
Ingestion: NO
Carcinogenicity Inds - NTP: NO
IARC: NO
OSHA: NO
Effects of Exposure: TARGET ORGANS: EYE, SKIN, CENTRAL NERVOUS SYSTEM,
  RESPIRATORY TRACT. ACUTE- VAPOR AND LIQUID MAY CAUSE EYE IRRITATION.
  PROLONGED/REPEATED SKIN CONTACT MAY CAUSE DRYNESS. CAN BE ABSORBED
  THROUGH SKIN.  INHALATION MAY CAUSE HEADACHE, LIGHT HEADEDNESS, CENTRAL
  NERVOUS SYSTEM DEPRESSION. MAY IRRITATE MUCOSAL TISSUE AT HIGH
  CONCENTRATION. INGESTIOPN IS UNLIKELY ROUTE OF EXPOSURE. HOWEVER, MINUTE
  AMOUNTS  ASPIRATED INTO LUNGS DURING INGESTION MAY CAUSE CHEMICAL
  PNEUMONIA. CHRONIC - UNKNOWN.
Explanation Of Carcinogenicity: NONE
Signs And Symptions Of Overexposure: IRRITATION, HEADACHE, NAUSEA,
  VOMITING, DIZZINESS, SKIN DEFATTING AND DRYNESS, BLURRED VISION, TEARING
Medical Cond Aggravated By Exposure: PERSONS WITH PRE-EXISTING RESPIRATORY
  DISORDERS.
First Aid: GET MEDICAL HELP IF SYMPTOMS PERSIST. INHALED: REMOVE TO FRESH
  AIR. PROVIDE OXYGEN IF NEEDED. EYES: FLUSH WITH WATER FOR 15 MINUTES,
  HOLDING EYELIDS OPEN. SKIN: WASH WITH SOAP & WATER. APPLY MEDICATED 
  CREAM. INGESTION: DO NOT INDUCE VOMITING. GET MEDICAL ATTENTION
  IMMEDIATELY. NEVER GIVE ANYTHING BY MOUTH TO AN UNCONSCIOUS PERSON.
=======================================================
Handling and Disposal
=======================================================
Spill Release Procedures: WEAR PROTECTIVE EQUIPMENT. ELIMINATE SOURCES OF
  IGNITION. VENTILATE AREA. CONTAIN AND PICK UP SPILL WITH NON-FLAMMABLE
  ABSORBENT SUCH AS SAND OR EXPLOSION-PROOF PUMP. GROUND ALL HANDLING
  EQUIPMENTS. P REVENT LIQUID FROM ENTERING SEWERS OR WATERWAYS. STORE IN
  CLOSED CONTAINERS. DO NOT FLUSH PRODUCT TO SEWER. TRANSFER TO DRUMS
  USING NON-SPARKING TOOLS.
Neutralizing Agent: NOT RELEVANT
Waste Disposal Methods: DISPOSE OF IN ACCORDANCE WITH FEDERAL, STATE AND
  LOCAL REGULATIONS FOR FLAMMABLE HYDROCARBONS OR RECLAIM BY DISTILLATION.
Handling And Storage Precautions: STORE IN COOL, VENTILATED AREA, AWAY
  FROM FLAMES, SPARKS, HOT SURFACES & STRONG OXIDIZING AGENTS. KEEP
  CONTAINER TIGHTLY CLOSED. STORE BELOW 100F.
Other Precautions: EXTREMELY FLAMMABLE. "EMPTY" CONTAINERS RETAIN RESIDUE
  AND CAN BE DANGEROUS. FOLLOW ALL LABEL INSTRUCTIONS. AVOID
  REPEATED/PROLONGED SKIN CONTACT. KEEP OUT OF REACH OF CHILDREN. DO NOT
  BREATHE VAPORS.
=======================================================
Fire and Explosion Hazard Information 
=======================================================
Flash Point Method: TCC
Flash Point: <-17.8C, 0.F
Lower Limits: 1.2
Upper Limits: 7.7
Extinguishing Media: CARBON DIOXIDE, FOAM, DRY CHEMICAL.
Fire Fighting Procedures: WEAR NIOSH-APPROVED SELF-CONTAINED BREATHING
  APPARATUS. COOL FIRE-EXPOSED CONTAINERS WITH WATER SPRAY.
Unusual Fire/Explosion Hazard: VAPOR IS HEAVIER THAN AIR AND CAN TRAVEL
  CONSIDERABLE DISTANCE TO A SOURCE OF IGNITION AND FLASH BACK. CONTAINERS
  MAY RUPTURE DUE TO VAPOR PRESSURE BUILDUP.
=======================================================
Control Measures 
=======================================================
Respiratory Protection: IF TLV IS EXCEEDED, WEAR NIOSH-APPROVED ORGANIC
  VAPOR RESPIRATOR OR SELF-CONTAINED BREATHING APPARATUS.  NONE REQUIRED
  IF GOOD VENTILATION IS MAINTAINED.
Ventilation: MECHANICAL (GENERAL AND/OR LOCAL EXHAUST, EXPLOSION-PROOF)
  VENTILATION TO MAINTAIN EXPOSURE BELOW TLV(S).
Protective Gloves: USE SOLVENT RESISTANT GLOVES (BUNA-N OR NEOPRENE).
Eye Protection: CHEMICAL SAFETY GOGGLES
Other Protective Equipment: EYE WASH STATION & SAFETY SHOWERS SHOULD BE
  AVAILABLE IN THE IMMEDIATE VICINITY OF ANY POTENTIAL EXPOSURE.
Work Hygienic Practices: OBSERVE GOOD INDUSTRIAL HYGIENE PRACTICES AND
  RECOMMENDED PROCEDURES. WASH AFTER HANDLING AND BEFORE EATING OR
  DRINKING.
=======================================================
Physical/Chemical Properties 
=======================================================
HCC: F2
NRC/State LIC No: NOT RELEVANT
Boiling Point: =60.6C, 141.F
Vapor Pres: 352 @ 100F
Vapor Density: 3.0
Spec Gravity: 0.665
Appearance and Odor: CLEAR, COLORLESS LIQUID - MILD ALCOHOL ODOR
Percent Volatiles by Volume: 100
=======================================================
Reactivity Data 
=======================================================
Stability Indicator: YES
Stability Condition To Avoid: HIGH HEAT, OPEN FLAMES, SPARKS, HOT
  SURFACES, ELECTRICAL ARCS, OTHER SOURCES OF IGNITION
Materials To Avoid: STRONG OXIDIZING AGENTS, OXYGEN
Hazardous Decomposition Products: CARBON MONOXIDE, CARBON DIOXIDE
Hazardous Polymerization Indicator: NO
Conditions To Avoid Polymerization: NOT RELEVANT
=======================================================
Toxicological Information 
=======================================================
=======================================================
Ecological Information 
=======================================================
=======================================================
MSDS Transport Information 
=======================================================
Transport Information: FLAMMABLE LIQUID (HEXANES, ISOPROPANOL), 3, UN1993,
  PGII
=======================================================
Regulatory Information 
=======================================================
Sara Title III Information: YES, CAS # 110-54-3
=======================================================
Other Information 
=======================================================
=======================================================
Transportation Information 
=======================================================
Responsible Party Cage: 66724
Trans ID NO: 148565
Product ID: LPS CFC-FREE ELECTRO CONTACT CLEANER
MSDS Prepared Date: 11/07/1996
Review Date: 09/21/1999
Article W/O MSDS: N
Tech Entry NOS Shipping Nm: HEXANES, ISOPROPANOL
Net Unit Weight: 28 LBS
Limited Quantity IND: N
Multiple KIT Number: 0
Review IND: N
Unit Of Issue: CN
Container QTY: 0
Type Of Container: CAN
=======================================================
Detail DOT Information 
=======================================================
DOT PSN Code: GJJ
Symbols: G
DOT Proper Shipping Name: FLAMMABLE LIQUIDS, N.O.S.
Hazard Class: 3
UN ID Num: UN1993
DOT Packaging Group: II
Label: FLAMMABLE LIQUID
Special Provision: T8,T31
Non Bulk Pack: 202
Bulk Pack: 242
Max Qty Pass: 5L
Max Qty Cargo: 60 L
Vessel Stow Req: B
=======================================================
Detail IMO Information 
=======================================================
IMO PSN Code: HIN
IMO Proper Shipping Name: FLAMMABLE LIQUID, N.O.S. o
IMDG Page Number: 3230
UN Number: 1993
UN Hazard Class: 3.2
IMO Packaging Group: I/II
Subsidiary Risk Label: -
EMS Number: 3-07
MED First Aid Guide NUM: T
=======================================================
Detail IATA Information 
=======================================================
IATA UN ID Num: 1993
IATA Proper Shipping Name: FLAMMABLE LIQUID, N.O.S. *
IATA UN Class: 3
IATA Label: FLAMMABLE LIQUID
UN Packing Group: II
Packing Note Passenger: 305
Max Quant Pass: 5L
Max Quant Cargo: 60L
Packaging Note Cargo: 307
=======================================================
Detail AFI Information 
=======================================================
AFI Symbols: *
AFI Proper Shipping Name: FLAMMABLE LIQUIDS, N.O.S.
AFI Hazard Class: 3
AFI UN ID NUM: UN1993
AFI Packing Group: II
Special Provisions: P5
Back Pack Reference: A7.3
=======================================================
HAZCOM Label 
=======================================================
Product ID: LPS CFC-FREE ELECTRO CONTACT CLEANER
Cage: 66724
Company Name: LPS LABORATORIES,  INC.
Street: 4647 HUGH HOWELL ROAD
City: TUCKER GA
Zipcode: 30085-5052 US
Health Emergency Phone: 770-934-7800
Date Of Label Review: 09/21/1999
Eye Protection IND: YES
Skin Protection IND: YES
Signal Word: DANGER
Respiratory Protection IND: YES
Health Hazard: Severe
Contact Hazard: Moderate
Fire Hazard: Severe
Reactivity Hazard: None
Hazard And Precautions: TARGET ORGANS: EYE, SKIN, CENTRAL NERVOUS SYSTEM,
  RESPIRATORY TRACT. ACUTE- VAPOR AND LIQUID MAY CAUSE EYE IRRITATION.
  PROLONGED/REPEATED SKIN CONTACT MAY CAUSE DRYNESS. CAN BE ABSORBED
  THROUGH SKIN.  INHALATION MAY CAUSE HEADACHE, LIGHT HEADEDNESS, CENTRAL
  NERVOUS SYSTEM DEPRESSION. MAY IRRITATE MUCOSAL TISSUE AT HIGH
  CONCENTRATION. INGESTIOPN IS UNLIKELY ROUTE OF EXPOSURE. HOWEVER, MINUTE
  AMOUNTS  ASPIRATED INTO LUNGS DURING INGESTION MAY CAUSE CHEMICAL
  PNEUMONIA. CHRONIC - UNKNOWN.
=======================================================
Disclaimer (provided with this information by the compiling agencies):
  This information is formulated for use by elements of the Department of
  Defense. The United States of America in no manner whatsoever expressly
  or implied warrants, states, or intends said information to have any
  application, use or viability by or to any person or persons outside the
  Department of Defense nor any person or persons contracting with any
  instrumentality of the United States of America and disclaims all
  liability for such use. Any person utilizing this instruction who is not
  a military or civilian employee of the United States of America should
  seek competent professional advice to verify and assume responsibility
  for the suitability of this information to their particular situation
  regardless of similarity to a corresponding Department of Defense or
  other government situation.