SHERWIN-WILLIAMS SPRAYON PRODUCTS DIV -- 00711 PENETRANT-LUBRICANT -- 6850-00-142-9409
=======================================================
MSDS Safety Information 
=======================================================
FSC: 6850
NIIN: 00-142-9409
MSDS Date: 06/18/1991
MSDS Num: BMBZS
Tech Review: 05/16/1999
Product ID: 00711 PENETRANT-LUBRICANT
Responsible Party
Cage: DO642
Name: SHERWIN-WILLIAMS CO SPRAYON PRODUCTS DIV
Address: 26300 FARGO AVE
City: BEDFORD HEIGHTS OH 44146-1310 US
Info Phone Number: 216-292-7400
Emergency Phone Number: 216-292-7400
=======================================================
Contractor Summary 
=======================================================
Cage: DO642
Name: SHERWIN-WILLIAMS CO THE SPECIALTY DIV.
Address: 6830 COCHRAN RD.
Box: 6709
City: SOLON OH 44139-3908
Country: NK
Phone: 216-292-7400
Cage: 09800
Name: SHERWIN-WILLIAMS DIVERSIFIED BRANDS, INC.
Address: 26300 FARGO AVENUE
City: BEDFORD HEIGHTS OH 44146 US
Phone: 216-292-7400 OR 216-595-8634
=======================================================
Item Description Information 
=======================================================
Item Manager: GSA
Item Name: WATER-DISPLACING COMPOUND
Specification Number: NK
Type/Grade/Class: TYPE 2, CLASS 2
Unit of Issue: BX
Quantitative Expression: 00000000012EA
UI Container Qty: G
Type of Container: NK
=======================================================
Ingredients 
=======================================================
Cas: 111-76-2
Name: N-BUTOXYETHANOL
% by Wt: < 5%
Other REC Limits: NONE SPECIFIED
OSHA PEL: 25 PPM
ACGIH TLV: 240 MG/M3
Ozone Depleting Chemical: N
------------------------------
Cas: 64742-88-7
Name: NAPHTHA, MEDIUM ALIPHATIC
% by Wt: 60 %
Other REC Limits: NONE SPECIFIED
OSHA PEL: NOT ESTABLISHED
ACGIH TLV: NOT ESTABLISHED
Ozone Depleting Chemical: N
------------------------------
Cas: 25496-72-4
Name: GLYCERYL MONOOLEATE
% by Wt: < 5%
Other REC Limits: NONE SPECIFIED
OSHA PEL: NOT ESTABLISHED
ACGIH TLV: NOT ESTABLISHED
Ozone Depleting Chemical: N
------------------------------
Cas: 64741-97-5
RTECS #: PY8041000
Name: DISTILLATES, SOLVENT-REFINED LIGHT NAPHTHENIC
% by Wt: < 5%
Other REC Limits: 5.0 MG/M3
OSHA PEL: 300 PPM
ACGIH TLV: 300 PPM
Ozone Depleting Chemical: N
------------------------------
Cas: 25619-56-1
Name: BARIUM DINONYLNAPHTALNE SULFONATE
% by Wt: < 5%
Other REC Limits: NONE SPECIFIED
OSHA PEL: 0.5 MG/M3 (AS BA)
ACGIH TLV: 0.5 MG/M3 (AS BA)
Ozone Depleting Chemical: N
------------------------------
Cas: 64741-88-4
Name: REFINED HEAVY PARAFFINIC DISTILLATES
% by Wt: 15 %
Other REC Limits: NONE SPECIFIED
OSHA PEL: 5 MG/M3 (OIL MIST)
ACGIH TLV: 5 MG/M3 (OIL MIST)
Ozone Depleting Chemical: N
------------------------------
Cas: 74-98-6
RTECS #: TX2275000
Name: PROPANE (PROPELLANT)
% by Wt: 20 %
Other REC Limits: 1800 MG/M3
OSHA PEL: 1000 PPM
ACGIH TLV: ASPHYXIANT; 9192
Ozone Depleting Chemical: N
=======================================================
Health Hazards Data 
=======================================================
LD50 LC50 Mixture: NOT SPECIFIED BY MANUFACTURER.
Route Of Entry Inds - Inhalation: YES
Skin: YES
Ingestion: YES
Carcinogenicity Inds - NTP: NO
IARC: NO
OSHA: NO
Effects of Exposure: IN A CONFINED AREA VAPORS IN HIGH CONCENTRATIONS ARE
  ANESTHETIC. IRRITANT TO SKIN AND UPPER RESPIRATORY SYSTEM. HARMFUL OR
  FATAL IF SWALLOWED. REPORTS HAVE ASSOCIATED REPEATED AND PROLONGED
  OVEREXOSUR E TO SOLVENTS WITH PERMANENT BRAIN AND NERVOUS SYSTEM DAMAGE,
  ALSO KIDNEY  AND LIVER DAMAGE.
Explanation Of Carcinogenicity: THIS PRODUCT IS NOT CONSIDERED TO BE A
  CARCINOGEN BY NTP, IARC OR OSHA OR NIOSH.
Signs And Symptions Of Overexposure: OVER-EXPOSURE MAY RESULT IN
  LIGHT-HEADEDNESS, STAGGERING GAIT, GIDDINESS AND POSSIBLE NAUSEA.
Medical Cond Aggravated By Exposure: NONE ESTABLISHED
First Aid: BREATHING: REMOVE PATIENT TO FRESH AIR. EYES: FLUSH WITH WATER
  FOR AT LEAST 15 MINUTES. SKIN: WASH WITH SOAP AND WATER. SWALLOWING:
  CALL PHYSICIAN IMMEDIATELY. DO NOT INDUCE VOMITING.
=======================================================
Handling and Disposal
=======================================================
Spill Release Procedures: REMOVE ALL SOURCES OF IGNITION. VENTILATE AVOID
  BREATHING VAPORS AND REMOVE WITH INERT ABSORBENT.
Neutralizing Agent: NONE SPECIFIED BY MANUFACTURER.
Waste Disposal Methods: DO NOT INCINERATE -- DISPOSE IN ACCORDANCE WITH
  FEDERAL, STATE AND LOCAL REGULATIONS REGARDING POLLUTION.
Handling And Storage Precautions: DO NOT STORE ABOVE 120F. KEEP AT ROOM
  TEMPERATURE AS EXPOSURE TO DIRECT SUNLIGHT OR HEAT MAY CAUSE BURSTING.
Other Precautions: KEEP AWAY FROM CHILDREN. DO NOT PUNCTURE OR INCINERATE.
  DO NOT SPRAY NEAR FIRE OR OPEN FLAME.
=======================================================
Fire and Explosion Hazard Information 
=======================================================
Flash Point Method: TOC
Flash Point Text: <20F,<-7C
Lower Limits: NOT GIVEN
Upper Limits: NOT GIVEN
Extinguishing Media: CARBON DIOXIDE, DRY CHEMICAL OR FOAM
Fire Fighting Procedures: WATER MAY BE INEFFECTIVE -- WATER MAY BE USED TO
  COOL FIRE EXPOSED CONTAINERS.
Unusual Fire/Explosion Hazard: DO NOT SPRAY NEAR OPEN FLAME. KEEP AT ROOM
  TEMPERATURE AS EXPOSURE TO DIRECT SUNLIGHT OR OTHER HEAT MAY CAUSE
  BURSTING.
=======================================================
Control Measures 
=======================================================
Respiratory Protection: AVOID BREATHING OF VAPOR OR SPRAY MIST. IF
  PERSONAL EXPOSURE CANNOT BE CONTROLLED WEAR A PROPERLY FITTED RESPIRATOR
  APPROVED BY NIOSH/MSHA FOR PROTECTION.
Ventilation: PROVIDE LOCAL EXHAUST VENTILATION IN VOLUME AND PATTERN TO
  KEEP TLV OF ALL HAZARDOUS INGREDIENTS BELOW ACCEPTABLE LIMITS
Protective Gloves: NITRILE, NEOPRENE
Eye Protection: SAFETY GLASSES WITH SIDE SHIELDS
Other Protective Equipment: NONE SPECIFIED BY MANUFACTURER.
Work Hygienic Practices: WASH WITH SOAP AND WATER AFTER HANDLING PRODUCT
  AND BEFORE EATING DRINKING OR SMOKING.
Supplemental Safety and Health: PRODUCT IS AN AEROSOL MATERIAL. CONTENTS
  UNDER PRESSURE. DO NOT PUNCTURE CAN.
=======================================================
Physical/Chemical Properties 
=======================================================
HCC: F1
B.P. Text: <0F,<-18C
M.P/F.P Text: NOT GIVEN
Vapor Pres: NOT GIVEN
Vapor Density: NOT GIVEN
Spec Gravity: NOT GIVEN
Evaporation Rate & Reference: >1 (ETHER = 1)
Solubility in Water: NEGLIGIBLE
Appearance and Odor: MIXTURE, CLEAR LIQUID, HYDROCARBON ODOR
Percent Volatiles by Volume: 80 %
=======================================================
Reactivity Data 
=======================================================
Stability Indicator: YES
Stability Condition To Avoid: DO NOT STORE ABOVE 120F
Materials To Avoid: NONE SPECIFIED BY MANUFACTURER.
Hazardous Decomposition Products: BY OPEN FLAME: CARBON MONOXIDE, CARBON
  DIOXIDE.
Hazardous Polymerization Indicator: NO
Conditions To Avoid Polymerization: NONE. WILL NOT OCCUR.
=======================================================
Toxicological Information 
=======================================================
=======================================================
Ecological Information 
=======================================================
=======================================================
MSDS Transport Information 
=======================================================
=======================================================
Regulatory Information 
=======================================================
=======================================================
Other Information 
=======================================================
=======================================================
Transportation Information 
=======================================================
Responsible Party Cage: DO642
Trans ID NO: 50304
Product ID: 00711 PENETRANT-LUBRICANT
MSDS Prepared Date: 06/18/1991
Review Date: 03/02/1992
Article W/O MSDS: N
Tech Entry NOS Shipping Nm: (PROPANE)
Multiple KIT Number: 0
Unit Of Issue: BX
Container QTY: G
Type Of Container: NK
=======================================================
Detail DOT Information 
=======================================================
DOT PSN Code: DTJ
Symbols: D
DOT Proper Shipping Name: CONSUMER COMMODITY
Hazard Class: ORM-D
Label: NONE
Non Bulk Pack: 156,306
Bulk Pack: NONE
Max Qty Pass: 30KGGROSS
Max Qty Cargo: 30KGGROSS
Vessel Stow Req: A
=======================================================
Detail IMO Information 
=======================================================
IMO PSN Code: AIY
IMO Proper Shipping Name: AEROSOL DISPENSERS ?
IMO PSN Modifier: ,WITH A CAPACITY OF 1000 CUBIC CM OR LESS
IMDG Page Number: 9022
UN Number: 1950
UN Hazard Class: 9?
IMO Packaging Group: -
Subsidiary Risk Label: -
EMS Number: 2-13
=======================================================
Detail IATA Information 
=======================================================
IATA PSN Code: ALS
IATA UN ID Num: 1950
IATA Proper Shipping Name: AEROSOLS, FLAMMABLE
IATA PSN Modifier: (EACH NOT EXCEEDING 1 L CAPACITY)
IATA UN Class: 2.1
IATA Label: FLAMMABLE GAS
Packing Note Passenger: 203
Max Quant Pass: 75KG
Max Quant Cargo: 150KG
Packaging Note Cargo: 203
=======================================================
Detail AFI Information 
=======================================================
AFI PSN Code: ALS
AFI Proper Shipping Name: AEROSOLS, NONFLAMMABLE, N.O.S.
AFI PSN Modifier: CONTAINING SUBSTANCES IN CLASS 8, PACKING GROUP I OR II
AFI Hazard Class: FORB
Back Pack Reference: FORBIDDEN
=======================================================
HAZCOM Label 
=======================================================
Product ID: 00711 PENETRANT-LUBRICANT
Cage: DO642
Company Name: SHERWIN-WILLIAMS CO THE SPECIALTY DIV.
Street: 6830 COCHRAN RD.
PO Box: 6709
City: SOLON OH
Zipcode: 44139-3908
Country: NK
Health Emergency Phone: 216-292-7400
Date Of Label Review: 03/02/1992
MFG Label NO: 00711
Label Date: 03/02/1992
Eye Protection IND: YES
Skin Protection IND: YES
Signal Word: DANGER
Health Hazard: Moderate
Contact Hazard: Slight
Fire Hazard: Severe
Reactivity Hazard: Slight
Hazard And Precautions: EXTREMELY FLAMMABLE. DO NOT SPRAY NEAR SPARKS,
  HEAT OR OPEN FLAME. CONTENTS UNDER PRESSURE. EXPOSURE TO HEAT MAY CAUSE
  BURSTING. DO NOT PUNCTURE, INCINERATE (OR BURN) OR STORE ABOVE 120F.
  AVOID PROLON GED EXPOSURE TO SUNLIGHT. HARMFUL OR FATAL IF SWALLOWED. IF
  SWALLOWED, DO NOT INDUCE VOMITING. CALL PHYSICIAN IMMEDIATELY. CONTAINS
  PETROLEUM DISTILLATES. USE WITH ADEQUATE VENTILATION. AVOID BREATHIN G
  OF SPRAY MIST OR PROLONGED CONTACT WITH SKIN. IN CASE OF SKIN
  IRRITATION, FLUSH WITH SOAP AND WATER. DO NOT INHALE DIRECTLY.
  DELIBERATE INHALATION OF CONTENTS MAY BE HARMFUL OR FATAL. IF AFFECTED
  BY  INHALATION, REMOVE TO FRESH AIR.
=======================================================
Disclaimer (provided with this information by the compiling agencies):
  This information is formulated for use by elements of the Department of
  Defense. The United States of America in no manner whatsoever expressly
  or implied warrants, states, or intends said information to have any
  application, use or viability by or to any person or persons outside the
  Department of Defense nor any person or persons contracting with any
  instrumentality of the United States of America and disclaims all
  liability for such use. Any person utilizing this instruction who is not
  a military or civilian employee of the United States of America should
  seek competent professional advice to verify and assume responsibility
  for the suitability of this information to their particular situation
  regardless of similarity to a corresponding Department of Defense or
  other government situation.