SHERWIN-WILLIAMS CO., SPRAYON PRODUCTS DIV. -- 00601 RED INSULATING VARNISH -- 5970-00-167-1564
=======================================================
MSDS Safety Information 
=======================================================
FSC: 5970
NIIN: 00-167-1564
MSDS Date: 08/10/1990
MSDS Num: BJQNC
Tech Review: 03/22/1991
Product ID: 00601 RED INSULATING VARNISH
Responsible Party
Cage: DO642
Name: SHERWIN-WILLIAMS CO., SPRAYON PRODUCTS DIV.
Address: 26300 FARGO AVE
City: BEDFORD HEIGHTS OH 44146-1310 US
Info Phone Number: 216-292-7400
Emergency Phone Number: 216-292-7400
=======================================================
Contractor Summary 
=======================================================
Cage: DO642
Name: SHERWIN-WILLIAMS CO THE SPECIALTY DIV.
Address: 6830 COCHRAN RD.
Box: 6709
City: SOLON OH 44139-3908
Country: NK
Phone: 216-292-7400
Cage: 09800
Name: SHERWIN-WILLIAMS DIVERSIFIED BRANDS, INC.
Address: 26300 FARGO AVENUE
City: BEDFORD HEIGHTS OH 44146 US
Phone: 216-292-7400 OR 216-595-8634
=======================================================
Item Description Information 
=======================================================
Item Manager: S9G
Item Name: INSULATING VARNISH,ELECTRICAL
Specification Number: NONE
Type/Grade/Class: NONE
Unit of Issue: PT
UI Container Qty: 0
Type of Container: AEROSOL CAN
=======================================================
Ingredients 
=======================================================
Cas: 1330-20-7
RTECS #: ZE2100000
Name: XYLENES (O-,M-,P- ISOMERS)  (SARA III)
% by Wt: 20
Other REC Limits: NONE SPECIFIED
OSHA PEL: 100 PPM/150 STEL
ACGIH TLV: 100 PPM/150STEL;9192
EPA Rpt Qty: 1000 LBS
DOT Rpt Qty: 1000 LBS
Ozone Depleting Chemical: N
------------------------------
Cas: 108-88-3
RTECS #: XS5250000
Name: TOLUENE  (SARA III)
% by Wt: 15
Other REC Limits: NONE SPECIFIED
OSHA PEL: 200 PPM/150 STEL
ACGIH TLV: 50 PPM; 9293
EPA Rpt Qty: 1000 LBS
DOT Rpt Qty: 1000 LBS
Ozone Depleting Chemical: N
------------------------------
Cas: 67-64-1
RTECS #: AL3150000
Name: ACETONE  (SARA III)
% by Wt: 20
Other REC Limits: NONE SPECIFIED
OSHA PEL: 1000PPM
ACGIH TLV: 750PPM/1000STEL;9293
EPA Rpt Qty: 5000 LBS
DOT Rpt Qty: 5000 LBS
Ozone Depleting Chemical: N
------------------------------
Cas: 64742-95-6
Name: NAPHTHA, LIGHT AROMATIC
% by Wt: <5
Other REC Limits: NONE SPECIFIED
OSHA PEL: NOT ESTABLISHED
ACGIH TLV: NOT ESTABLISHED
Ozone Depleting Chemical: N
------------------------------
Cas: 75-28-5
RTECS #: TZ4300000
Name: ISOBUTANE (PROPELLANT)
% by Wt: 15
Other REC Limits: NONE SPECIFIED
OSHA PEL: NOT ESTABLISHED
ACGIH TLV: NOT ESTABLISHED
Ozone Depleting Chemical: N
------------------------------
Cas: 74-98-6
RTECS #: TX2275000
Name: PROPANE
% by Wt: 15
Other REC Limits: NONE SPECIFIED
OSHA PEL: 1000 PPM
ACGIH TLV: ASPHYXIANT; 9192
Ozone Depleting Chemical: N
------------------------------
Name: VARNISH, PIGMENTS, ETC.
Other REC Limits: NONE SPECIFIED
=======================================================
Health Hazards Data 
=======================================================
LD50 LC50 Mixture: ACCUTE ORAL LD50 (RAT) IS UNKNOWN
Route Of Entry Inds - Inhalation: YES
Skin: YES
Ingestion: NO
Carcinogenicity Inds - NTP: NO
IARC: NO
OSHA: NO
Effects of Exposure: ACUTE:USE IN AN ENCLOSED AREA (BREATHING CONCENTRATED
  VAPORS) MAY EFFECT THE CENTRAL NERVOUS SYSTEM AND MAY DAMAGE THE LIVER
  AND/OR KIDNEYS.  CHRONIC:CHRONIC OVEREXPOSURE TO SOLVENTS MAY CAUSE
  PERMINE NT CENTRAL NERVOUS SYSTEM DAMAGE OR LIVER/KIDNEY DAMAGE.
Explanation Of Carcinogenicity: THE PRODUCT CONTAINS NO INGREDIENT THAT IS
  LISTED BY IARC, NTP OR OSHA AS A CARCINOGEN.
Signs And Symptions Of Overexposure: OVEREXPOSURE MAY LEAD TO EYE, SKIN &
  RESPIRATORY TRACT IRRITATION. VAPORS MAY CAUSE DIZZINESS, HEADACHES,
  NAUSEA, AND SKIN/EYE IRRITATION. INHALING LIQUID WHILE VOMITING CAN
  SERIOUSLY INJURE LUNGS. MA Y BURN OR BE ABSORBED THROUGH SKIN DURING
  PROLONGED OR REPEATED CONTACT, CAUSING SERIOUS INTERNAL INJURY.
Medical Cond Aggravated By Exposure: NONE GIVEN BY MANUFACTURER
  (SUPPLIER).
First Aid: EYE:FLUSH W/WATER 15 MIN, HOLD LIDS OPEN.  SKIN:WASH WITH SOAP
  & WATER. REMOVE CONTAMINATED CLOTHING AND LAUNDER BEFORE REUSE. 
  INHALED:REMOVE TO FRESH AIR. RESTORE BREATHING IF NECESSARY.	INGESTED:D
  O NOT INDUCE VOMITING. GIVE 2 LARGE GLASSES OF MILK OR WATER AND GET
  IMMEDIATE MEDICAL CARE. GIVE NOTHING BY MOUTH IF UNCONSCIOUS.   IF
  IRRITATION PERSISTS OR IS SEVERE,SEE A DOCTOR.
=======================================================
Handling and Disposal
=======================================================
Spill Release Procedures: REMOVE SOURCES OF IGNITION. USE ABSORBENT
  MATERIAL TO COLLECT AND CONTAIN FOR DISPOSAL.
Waste Disposal Methods: DISPOSE I/A/W ALL FEDERAL, STATE AND LOCAL
  REGULATIONS.	MANUFACTURER SUGGESTS THAT DISPOSAL OF CONTENTS MAY BE
  DONE BY INCINERATION.  DO NOT PUNCTURE OR INCINERATE AEROSOL CANS.
Handling And Storage Precautions: STORE BELOW 130 F AND OUT OF DIRECT
  SUNLIGHT. CONTENTS UNDER PRESSURE. DO NOT PUNCTURE OR INCINERATE.
  DEPRESSURIZE BEFORE DISPOSAL.
Other Precautions: DO NOT SPRAY NEAR FIRE OR OPEN FLAME.
=======================================================
Fire and Explosion Hazard Information 
=======================================================
Flash Point Text: AEROSOL
Extinguishing Media: USE CARBON DIOXIDE, FOAM, OR DRY CHEMICAL.
Fire Fighting Procedures: WEAR FIRE FIGHTING PROTECTIVE EQUIPMENT AND A
  FULL FACED SELF CONTAINED BREATHING APPARATUS. COOL FIRE EXPOSED
  CONTAINERS WITH WATER SPRAY. CONTAIN RUNOFF.
Unusual Fire/Explosion Hazard: DO NOT SPRAY NEAR FIRE OR FLAME.  WATER
  ESPECIALLY AS A STREAM, MAY BE INEFFECTIVE.
=======================================================
Control Measures 
=======================================================
Respiratory Protection: RESPIRATOR WILL NOT NORMALLY BE NECESSARY.  USE
  NIOSH/MSHA APPROVED AIR SUPPLIED RESPIRATOR OR RESPIRATOR FOR ORGANIC
  DUST/VAPOR IF EXPOSURE IS ABOVE THE TLV/PEL. SEE 29 CFR 1910.134 FOR
  REGULATIONS P ERTAINING TO RESPIRATOR USE.
Ventilation: LOCAL AND MECHANICAL(GENERAL) ARE BOTH RECOMMENDED. AVOID
  OPEN ELECTRICAL IGNITION SOURCES NEAR PRODUCT VAPOR AREAS.
Protective Gloves: RUBBER OR PLASTIC RECOMMENDED.
Eye Protection: SAFETY GLASSES OR SAFETY GOGGLES
Other Protective Equipment: EYE WASH STATION & SAFETY SHOWER. WEAR
  INDUSTRIAL TYPE WORK CLOTHING AND APRON AS REQUIRED.
Work Hygienic Practices: USE GOOD CHEMICAL HYGIENE PRACTICE. AVOID
  UNNECESSARY CONTACT.
=======================================================
Physical/Chemical Properties 
=======================================================
HCC: V3
Vapor Pres: >1
PH: UNKNON
Percent Volatiles by Volume: 82
=======================================================
Reactivity Data 
=======================================================
Stability Indicator: YES
Stability Condition To Avoid: TEMPERATURES ABOVE 120F
Materials To Avoid: NONE GIVEN BY MANUFACTURER (SUPPLIER).
Hazardous Decomposition Products: CARBON DIOXIDE, CARBON MONOXIDE, AND
  TRACES OF INCOMPLETELY BURNED CARBON PRODUCTS.
Hazardous Polymerization Indicator: NO
=======================================================
Toxicological Information 
=======================================================
=======================================================
Ecological Information 
=======================================================
=======================================================
MSDS Transport Information 
=======================================================
=======================================================
Regulatory Information 
=======================================================
=======================================================
Other Information 
=======================================================
=======================================================
Transportation Information 
=======================================================
Responsible Party Cage: DO642
Trans ID NO: 52988
Product ID: 00601 RED INSULATING VARNISH
MSDS Prepared Date: 08/10/1990
Review Date: 03/22/1991
Article W/O MSDS: N
Tech Entry NOS Shipping Nm: TOLUENE, ACETONE
Multiple KIT Number: 0
Unit Of Issue: PT
Container QTY: 0
Type Of Container: AEROSOL CAN
=======================================================
Detail DOT Information 
=======================================================
DOT PSN Code: DTJ
Symbols: D
DOT Proper Shipping Name: CONSUMER COMMODITY
Hazard Class: ORM-D
Label: NONE
Non Bulk Pack: 156,306
Bulk Pack: NONE
Max Qty Pass: 30KGGROSS
Max Qty Cargo: 30KGGROSS
Vessel Stow Req: A
=======================================================
Detail IMO Information 
=======================================================
IMO PSN Code: AIY
IMO Proper Shipping Name: AEROSOL DISPENSERS ?
IMO PSN Modifier: ,WITH A CAPACITY OF 1000 CUBIC CM OR LESS
IMDG Page Number: 9022
UN Number: 1950
UN Hazard Class: 9?
IMO Packaging Group: -
Subsidiary Risk Label: -
EMS Number: 2-13
=======================================================
Detail IATA Information 
=======================================================
IATA PSN Code: ALS
IATA UN ID Num: 1950
IATA Proper Shipping Name: AEROSOLS, FLAMMABLE
IATA PSN Modifier: (EACH NOT EXCEEDING 1 L CAPACITY)
IATA UN Class: 2.1
IATA Label: FLAMMABLE GAS
Packing Note Passenger: 203
Max Quant Pass: 75KG
Max Quant Cargo: 150KG
Packaging Note Cargo: 203
=======================================================
Detail AFI Information 
=======================================================
AFI PSN Code: ALS
AFI Proper Shipping Name: AEROSOLS, NONFLAMMABLE, N.O.S.
AFI PSN Modifier: CONTAINING SUBSTANCES IN CLASS 8, PACKING GROUP I OR II
AFI Hazard Class: FORB
Back Pack Reference: FORBIDDEN
=======================================================
HAZCOM Label 
=======================================================
Product ID: 00601 RED INSULATING VARNISH
Cage: DO642
Company Name: SHERWIN-WILLIAMS CO THE SPECIALTY DIV.
Street: 6830 COCHRAN RD.
PO Box: 6709
City: SOLON OH
Zipcode: 44139-3908
Country: NK
Health Emergency Phone: 216-292-7400
Label Required IND: N
Date Of Label Review: 03/22/1991
Label Date: 03/22/1991
Eye Protection IND: YES
Skin Protection IND: YES
Signal Word: DANGER
Respiratory Protection IND: YES
Health Hazard: Moderate
Contact Hazard: Slight
Fire Hazard: Severe
Reactivity Hazard: None
=======================================================
Disclaimer (provided with this information by the compiling agencies):
  This information is formulated for use by elements of the Department of
  Defense. The United States of America in no manner whatsoever expressly
  or implied warrants, states, or intends said information to have any
  application, use or viability by or to any person or persons outside the
  Department of Defense nor any person or persons contracting with any
  instrumentality of the United States of America and disclaims all
  liability for such use. Any person utilizing this instruction who is not
  a military or civilian employee of the United States of America should
  seek competent professional advice to verify and assume responsibility
  for the suitability of this information to their particular situation
  regardless of similarity to a corresponding Department of Defense or
  other government situation.