SPRAYON PRODUCTS -- LUBRICANTS, 2X988B SILICONE LUBRICANT -- 9150-00N051709
=======================================================
MSDS Safety Information 
=======================================================
FSC: 9150
MSDS Date: 02/06/1991
MSDS Num: BTZQY
LIIN: 00N051709
Tech Review: 07/21/1994
Product ID: LUBRICANTS, 2X988B SILICONE LUBRICANT
Responsible Party
Cage: 09800
Name: SPRAYON PRODUCTS
Address: 26300 FARGO AVENUE
City: BEDFORD HEIGHTS OH 44146 US
Info Phone Number: 216-292-7400
Emergency Phone Number: 216-292-7400
Review Ind: N
=======================================================
Contractor Summary 
=======================================================
Cage: 09800
Name: SHERWIN-WILLIAMS DIVERSIFIED BRANDS, INC.
Address: 26300 FARGO AVENUE
City: BEDFORD HEIGHTS OH 44146 US
Phone: 216-292-7400 OR 216-595-8634
=======================================================
Ingredients 
=======================================================
Cas: 74-98-6
RTECS #: TX2275000
Name: PROPANE, 2-METHYL-; (2-METHYLPROPANE (PROPELLANT))   VP: 760
% by Wt: 60
OSHA PEL: N/K (FP N)
ACGIH TLV: N/K (FP N)
Ozone Depleting Chemical: N
------------------------------
Cas: 110-54-3
RTECS #: MN9275000
Name: HEXANE
% by Wt: 35
OSHA PEL: 500 PPM
ACGIH TLV: 50 PPM
EPA Rpt Qty: 1 LB
DOT Rpt Qty: 1 LB
Ozone Depleting Chemical: N
------------------------------
Name: SUPDAT: SOURCES OF IGNIT. CONSULT NFPA CODE. USE APPRVD BONDING &
  GROUNDING PROC. CONTENTS UNDER PRESS. DO NOT (ING 4)
-----------------------------
Name: ING 3: PUNCTURE, INCIN/EXPOSE TO TEMPS ABOVE 120F. HEAT FROM
  SUNLIGHT, RADIATORS, STOVES, HOT WATER & OTHER (ING 5)
-----------------------------
Name: ING 4: SOURCES COULD CAUSE CNTNR TO BURST. DO NOT TAKE INTERNALLY.
  KEEP OUT OF REACH OF CHILDREN.
-----------------------------
Name: OTHER PREC: IN INGREDS) WHICH MAY BE PRESENT AT HAZ LEVELS ONLY
  DURING SANDING/ABRADING OF DRIED FILM. IF NO (ING 7)
-----------------------------
Name: ING 6: SPECIFIC DUSTS ARE LISTED, THE APPLIC LIMITS FOR NUISANCE
  DUSTS ARE ACGIH TLV 10 MG/M3 (TDUST), OSHA PEL (ING 8)
-----------------------------
Name: ING 7: 15 MG/M3 (TDUST), 5 MG/M3 (RESPIRABLE FRACTION).
-----------------------------
Name: RESP PROT: GENERATED FROM THIS PRODUCT, UNDERLYING PAINT, OR THE
  ABRASIVE.
=======================================================
Health Hazards Data 
=======================================================
LD50 LC50 Mixture: NONE SPECIFIED BY MANUFACTURER.
Route Of Entry Inds - Inhalation: YES
Skin: NO
Ingestion: NO
Carcinogenicity Inds - NTP: NO
IARC: NO
OSHA: NO
Effects of Exposure: ACUTE: IRRIT OF EYES, SKIN & RESP SYSTEM. MAY CAUSE
  NERVOUS SYS DEPRESS. EXTREME OVEREXP MAY RSLT IN UNCON & POSS DEATH.
  HDCH, DIZZ, NAUS & INCOORDINATION ARE INDICATIONS OF EXCESS EXPOS TO
  VAP/SPRAY  MISTS. REDNESS & ITCH/BURNING SENSATIONMAY INDICATE
  EYE/EXCESS SKIN EXPOS. CHRONIC: PRLNG & RPTD (EFTS OF OVEREXP)
Explanation Of Carcinogenicity: NOT RELEVANT
Signs And Symptions Of Overexposure: HLTH HAZ: EXPOS TO HEXANE MAY CAUSE
  DMG TO NERVE TISS OF ARMS & LEGS (PERIPHERAL NEUROPATHY), RSLTG IN MUSC
  WEAK & LOSS OF SENSATION. EFT MAY BE INCR BY PRESENCE OF METHYL ETHYL
  KETONE. PRLNG OVEREXP  TO LISTED SOLV INGREDS MAY CAUSE ADVERSE EFTS TO
  LIVER, URINARY & CARDIOVASCULAR SYS. REPORTS ASSOC RPTD & (SUPDAT)
Medical Cond Aggravated By Exposure: NONE GENERALLY RECOGNIZED.
First Aid: INHAL: IF AFFECTED, REMOVE FROM EXPOSURE. RESTORE BREATHING.
  KEEP WARM & QUIET. SKIN: WASH AFFECTED AREA THORO W/SOAP & WATER. REMOVE
  CONTAMINATED CLOTHING & LAUNDER BEFORE REUSE. EYES: FLUSH EYES W/L ARGE
  AMOUNTS OF WATER FOR AT LEAST 15 MINUTES. GET MED ATTN. INGEST: NEVER
  GIVE ANYTHING BY MOUTH TO AN UNCONSCIOUS PERSON. DO NOT INDUCE VOMITING.
  GIVE SEVERAL GLASSES OF WATER. SEEK MED ATTN.
=======================================================
Handling and Disposal
=======================================================
Spill Release Procedures: REMOVE ALL SOURCES OF IGNITION. VENTILATE &
  REMOVE WITH INERT ABSORBENT.
Neutralizing Agent: NONE SPECIFIED BY MANUFACTURER.
Waste Disposal Methods: WASTE FROM THIS PROD MAY BE HAZARDOUS AS DEFINED
  UNDER RCRA 40 CFR 261. WASTE MUST BE TESTED FOR IGNITABILITY TO
  DETERMINE APPLIC EPA HAZ WASTE NUMBER. DO NOT INCIN. DEPRESSURIZE CNTNR.
  DISPOSE OF I/A /W FED, STATE & LOCAL REGS REGARDING POLLUTION.
Handling And Storage Precautions: CONTENTS ARE EXTREMELY FLAMM. KEEP AWAY
  FROM HEAT, SPKS & OPEN FLAME. VAPS WILL ACCUM READILY & MAY IGNITE
  EXPLO. DURING USE & UNTIL ALL VAPS (SUPDAT)
Other Precautions: INTENTIONAL MISUSE BY DELIB CONC & INHAL CONTENTS CAN
  BE HARMFUL/FATAL. USE ONLY W/ADEQ VENT. AVOID BRTHG VAP & SPRAY MIST.
  AVOID CNTCT W/SKIN & EYES. THIS COATING MAY CNTN MATLS CLASSIFIED AS
  NUISANC E PARTICULATES (LISTED AS DUST (ING 6)
=======================================================
Fire and Explosion Hazard Information 
=======================================================
Flash Point Method: PMCC
Flash Point Text: <0F,<-18C
Lower Limits: 1%
Upper Limits: 7%
Extinguishing Media: CARBON DIOXIDE, DRY CHEMICAL, FOAM.
Fire Fighting Procedures: USE NIOSH/MSHA APPRVD SCBA & FULL PROT EQUIP
  (FPN). WATER SPRAY MAY BE INEFTIVE. IF WATER IS USED, FOG NOZZ PREF.
  WATER MAY BE USED TO COOL CLSD CNTNRS (SUPDAT)
Unusual Fire/Explosion Hazard: CLOSED CONTAINERS MAY EXPLODE (DUE TO
  BUILD-UP OF PRESSURE) WHEN EXPOSED TO EXTREME HEAT.
=======================================================
Control Measures 
=======================================================
Respiratory Protection: IF PERSONAL EXPOS CANNOT BE CONTROLLED BELOW
  APPLIC LIMS BY VENT, WEAR NIOSH/MSHA APPRVD, PROPERLY FITTED ORG
  VAP/PARTICULATE RESP. WHEN SANDING/ABRADING DRIED FILM, WEAR DUST/MIST
  RESP APPRVD BY NIOS H/MSHA FOR DUST WHICH MAY BE (ING 9)
Ventilation: LOC EXHST PREF. GEN EXHST ACCEPTABLE IF EXPOS MAINTAINED
  BELOW APPLIC EXPOS LIM. REFER TO OSHA STDS 1910.94, 107, 108.
Protective Gloves: IMPERVIOUS GLOVES (FP N).
Eye Protection: ANSI APPRVD CHEM WORKER GOGGLES (FP N).
Other Protective Equipment: NONE SPECIFIED BY MANUFACTURER.
Work Hygienic Practices: WASH HANDS AFTER USING.
Supplemental Safety and Health: FIGHT PROC: TO PVNT PRESS BUILD-UP & POSS
  AUTOIGNIT/EXPLOS WHEN EXPOSED TO EXTREME HEAT. EFTS OF OVEREXP: PRLNG
  OVEREXP TO SOLV W/PERM BRAIN & NERVOUS SYS DMG. HNDLG/STOR PREC: GONE,
  KEEP AREA VENT. D O NOT SMOKE. EXTING ALL FLAMES, PILOT LIGHTS &
  HEATERS. TURN OFF STOVES, ELEC TOOLS & APPLIANCES & ANY OTHER (ING 3)
=======================================================
Physical/Chemical Properties 
=======================================================
B.P. Text: <292F,<144C
Vapor Pres: SEE INGS
Vapor Density: HVR/AIR
Evaporation Rate & Reference: FASTER THAN ETHER
Appearance and Odor: NONE SPECIFIED BY MANUFACTURER.
Percent Volatiles by Volume: >75
=======================================================
Reactivity Data 
=======================================================
Stability Indicator: YES
Stability Condition To Avoid: NONE SPECIFIED BY MANUFACTURER.
Materials To Avoid: NONE KNOWN.
Hazardous Decomposition Products: BY FIRE: CARBON DIOXIDE, CARBON MONOXIDE
Hazardous Polymerization Indicator: NO
Conditions To Avoid Polymerization: NOT RELEVANT
=======================================================
Toxicological Information 
=======================================================
=======================================================
Ecological Information 
=======================================================
=======================================================
MSDS Transport Information 
=======================================================
=======================================================
Regulatory Information 
=======================================================
=======================================================
Other Information 
=======================================================
=======================================================
HAZCOM Label 
=======================================================
Product ID: LUBRICANTS, 2X988B SILICONE LUBRICANT
Cage: 09800
Company Name: SHERWIN-WILLIAMS DIVERSIFIED BRANDS, INC.
Street: 26300 FARGO AVENUE
City: BEDFORD HEIGHTS OH
Zipcode: 44146 US
Health Emergency Phone: 216-292-7400
Date Of Label Review: 07/21/1994
Label Date: 07/21/1994
Chronic Hazard IND: Y
Eye Protection IND: YES
Skin Protection IND: YES
Signal Word: DANGER
Respiratory Protection IND: YES
Health Hazard: Moderate
Contact Hazard: Moderate
Fire Hazard: Severe
Reactivity Hazard: None
Hazard And Precautions: FLAMMABLE. ACUTE: IRRIT OF EYES, SKIN & RESP SYS.
  MAY CAUSE NERVOUS SYS DEPRESS. EXTREME OVEREXP MAY RESULT IN UNCON &
  POSSIBLY DEATH. HEADACHE, DIZZ, NAUS & INCOORDINATION ARE INDICATIONS OF
  EXCESS E XPOSURE TO VAPORS/SPRAY MISTS. REDNESS & ITCHING/BURNING
  SENSATION MAY INDICATE EYE/EXCESS SKIN EXPOSURE. INTENTIONAL MISUSE MAY
  BE HARMFUL/FATAL. CHRONIC: PRLNG & RPTD EXPOSURE TO HEXANE MAY CAUSE DA
  MAGE TO NERVE TISSUE OF ARMS & LEGS RESULTING IN MUSCULAR WEAK & LOSS OF
  SENSATION. PRLNG OVEREXP TO SOLVENTS MAY CAUSE ADVERSE EFFECTS TO LIVER,
  URINARY & CARDIOVASCULAR SYS. REPORTS ASSOCIATE OVEREX P TO SOLVENTS
  W/PERMANENT BRAIN & NERVOUS SYS DMG.
=======================================================
Disclaimer (provided with this information by the compiling agencies):
  This information is formulated for use by elements of the Department of
  Defense. The United States of America in no manner whatsoever expressly
  or implied warrants, states, or intends said information to have any
  application, use or viability by or to any person or persons outside the
  Department of Defense nor any person or persons contracting with any
  instrumentality of the United States of America and disclaims all
  liability for such use. Any person utilizing this instruction who is not
  a military or civilian employee of the United States of America should
  seek competent professional advice to verify and assume responsibility
  for the suitability of this information to their particular situation
  regardless of similarity to a corresponding Department of Defense or
  other government situation.