MATERIAL SAFETY DATA SHEET
1. CHEMICAL PRODUCT AND COMPANY IDENTIFICATION

Elmer's Products, Inc.

Emergency Phone Number:

1 Easton Oval

Poison Control Center

Columbus, OH 43219

1-888-516-2502

For additional product information, access our website at www.elmers.com or call 1-888-435-6377. To place an order, call 1-800-848-9400.

SUBSTANCE: ELMER'S PROBOND INTERIOR/EXTERIOR WOOD GLUE

TRADE NAMES/SYNONYMS:
P9721; P9722; P9723; P9724; P9725; P9726; P9727; P9728

PRODUCT USE: adhesives

CREATION DATE: May 01 2002
REVISION DATE: Feb 23 2007

2. COMPOSITION, INFORMATION ON INGREDIENTS

COMPONENT: PROPRIETARY NON-HAZARDOUS INGREDIENTS
CAS NUMBER: Not assigned.
PERCENTAGE: 95-100

COMPONENT: FORMALDEHYDE
CAS NUMBER: 50-00-0
PERCENTAGE: <0.1

3. HAZARDS IDENTIFICATION

NFPA RATINGS (SCALE 0-4):  HEALTH=1  FIRE=1  REACTIVITY=0

EMERGENCY OVERVIEW:
COLOR: yellow
PHYSICAL FORM: liquid
ODOR: mild odor
MAJOR HEALTH HAZARDS: No significant target effects reported.

POTENTIAL HEALTH EFFECTS:
INHALATION:
SHORT TERM EXPOSURE: no information on significant adverse effects
LONG TERM EXPOSURE: no information on significant adverse effects
SKIN CONTACT:
SHORT TERM EXPOSURE: no information on significant adverse effects
LONG TERM EXPOSURE: no information on significant adverse effects
EYE CONTACT:
SHORT TERM EXPOSURE: no information on significant adverse effects
LONG TERM EXPOSURE: no information on significant adverse effects
INGESTION:
SHORT TERM EXPOSURE: no information on significant adverse effects
LONG TERM EXPOSURE: no information on significant adverse effects

4. FIRST AID MEASURES

INHALATION: If adverse effects occur, remove to uncontaminated area. Give artificial respiration if not breathing. Get immediate medical attention.

SKIN CONTACT: Wash skin with soap and water for at least 15 minutes while removing contaminated clothing and shoes. Get medical attention, if needed. Thoroughly clean and dry contaminated clothing and shoes before reuse.

EYE CONTACT: Flush eyes with plenty of water for at least 15 minutes. Then get immediate medical attention.

INGESTION: If a large amount is swallowed, get medical attention.

5. FIRE FIGHTING MEASURES

FIRE AND EXPLOSION HAZARDS: Slight fire hazard.

EXTINGUISHING MEDIA: carbon dioxide, regular dry chemical, regular foam, water

FIRE FIGHTING: Move container from fire area if it can be done without risk. Avoid inhalation of material or combustion by-products. Stay upwind and keep out of low areas.

FLASH POINT: No data available.

6. ACCIDENTAL RELEASE MEASURES

WATER RELEASE:
Subject to California Safe Drinking Water and Toxic Enforcement Act of 1986 (Proposition 65). Keep out of water supplies and sewers.

OCCUPATIONAL RELEASE:
Stop leak if possible without personal risk. Small spills: Absorb with sand or other non-combustible material. Collect spilled material in appropriate container for disposal. Notify Local Emergency Planning Committee and State Emergency Response Commission for release greater than or equal to RQ (U.S. SARA Section 304). If release occurs in the U.S. and is reportable under CERCLA Section 103, notify the National Response Center at (800)424-8802 (USA) or (202)426-2675 (USA).

7. HANDLING AND STORAGE

STORAGE: Store and handle in accordance with all current regulations and standards. Store in a cool, dry place. Keep container tightly closed. Protect from freezing. See original container for storage recommendations. Keep separated from incompatible substances.

8. EXPOSURE CONTROLS, PERSONAL PROTECTION

EXPOSURE LIMITS:
ELMER'S PROBOND INTERIOR/EXTERIOR WOOD GLUE:
No occupational exposure limits established.

VENTILATION: Provide local exhaust ventilation system. Ensure compliance with applicable exposure limits.

EYE PROTECTION: Wear splash resistant safety goggles. Provide an emergency eye wash fountain and quick drench shower in the immediate work area.

CLOTHING: Wear appropriate chemical resistant clothing.

GLOVES: Wear appropriate chemical resistant gloves.

RESPIRATOR: Under conditions of frequent use or heavy exposure, respiratory protection may be needed. Respiratory protection is ranked in order from minimum to maximum. Consider warning properties before use.
Any powered, air-purifying respirator with a full facepiece and organic vapor and acid gas cartridge(s).
Any chemical cartridge respirator with a full facepiece and organic vapor and acid gas cartridge(s).
For Unknown Concentrations or Immediately Dangerous to Life or Health -
Any supplied-air respirator with full facepiece and operated in a pressure-demand or other positive-pressure mode in combination with a separate escape supply.
Any self-contained breathing apparatus with a full facepiece.

9. PHYSICAL AND CHEMICAL PROPERTIES

PHYSICAL STATE: liquid
COLOR: yellow
ODOR: mild odor
BOILING POINT: 212 F (100 C) approximate
FREEZING POINT: 32 F (0 C) approximate
VAPOR PRESSURE: 17.5 mmHg @ 20 C
VAPOR DENSITY (air=1): <1
SPECIFIC GRAVITY (water=1): 1.07-1.1
WEIGHT PER GALLON: 8.9-9.2 lb(s)
WATER SOLUBILITY: disperses
PH: 2.4-2.8
VOLATILITY: Not available
ODOR THRESHOLD: Not available
EVAPORATION RATE: <1 (butyl acetate=1)
VISCOSITY: 4500-5000 cP @ 25 C (Brookfield, Spindle #7)
PERCENT SOLIDS: 51%
COEFFICIENT OF WATER/OIL DISTRIBUTION: Not available

10. STABILITY AND REACTIVITY

REACTIVITY: Stable at normal temperatures and pressure.

CONDITIONS TO AVOID: Avoid heat, flames, sparks and other sources of ignition. Avoid contact with incompatible materials.

INCOMPATIBILITIES: strong acids, alkalis, oxidizing materials

HAZARDOUS DECOMPOSITION:
Thermal decomposition products: oxides of carbon

POLYMERIZATION: Will not polymerize.

11. TOXICOLOGICAL INFORMATION

Not available

12. ECOLOGICAL INFORMATION

Not available

13. DISPOSAL CONSIDERATIONS

Dispose in accordance with all applicable regulations.

14. TRANSPORT INFORMATION

U.S. DEPARTMENT OF TRANSPORTATION: No classification assigned.

CANADIAN TRANSPORTATION OF DANGEROUS GOODS: No classification assigned.

15. REGULATORY INFORMATION

U.S. REGULATIONS:
CERCLA SECTIONS 102a/103 HAZARDOUS SUBSTANCES (40 CFR 302.4):
Formaldehyde: 100 LBS RQ

SARA TITLE III SECTION 302 EXTREMELY HAZARDOUS SUBSTANCES (40 CFR 355.30): Not regulated.

SARA TITLE III SECTION 304 EXTREMELY HAZARDOUS SUBSTANCES (40 CFR 355.40): Not regulated.

SARA TITLE III SARA SECTIONS 311/312 HAZARDOUS CATEGORIES (40 CFR 370.21):
ACUTE: No
CHRONIC: No
FIRE: No
REACTIVE: No
SUDDEN RELEASE: No

SARA TITLE III SECTION 313 (40 CFR 372.65): Not regulated.

OSHA PROCESS SAFETY (29CFR1910.119):
Formaldehyde: 1000 LBS TQ

STATE REGULATIONS:
California Proposition 65:
Known to the state of California to cause the following:
Formaldehyde
Cancer (Jan 01, 1988)

CANADIAN REGULATIONS:
WHMIS CLASSIFICATION: Not determined.

NATIONAL INVENTORY STATUS:
U.S. INVENTORY (TSCA): All components of this product are in compliance.

TSCA 12(b) EXPORT NOTIFICATION: Not listed.

CANADA INVENTORY (DSL/NDSL): Not determined.

16. OTHER INFORMATION

©Copyright 1984-2006 MDL Information Systems, Inc. All rights reserved.

SELLER MAKES NO WARRANTY, EXPRESS OR IMPLIED, CONCERNING THE PRODUCT OR THE MERCHANTABILITY OR FITNESS THEREOF FOR ANY PURPOSE, except that the product shall conform to contracted specifications, and that the product does not infringe any valid United States or Canadian patent. No claim of any kind shall be greater in amount than the purchase price of the quantity of product in respect of which damages are claimed. In no event shall Seller be liable for incidental or consequential damages, whether Buyer's claim is based on contract, breach of warranty, negligence or otherwise.